<?xml version="1.0" encoding="ISO-8859-1"?>
<msq xmlns="http://www.msefi.com/:msq">
<bibliography author="TunerStudio MS 3.1.05 - EFI Analytics, Inc." tuneComment="" writeDate="Thu Apr 08 19:08:00 EDT 2021"/>
<versionInfo fileFormat="5.0" firmwareInfo="MS3+1.5.1+release+++++20171006+16%3A30BST+%28c%29+JSM%2FKC+********" nPages="20" signature="MS3 Format 0566.05P"/>
<page>
<pcVariable name="tsCanId">"0"</pcVariable>
<pcVariable name="tsCanId">"CAN ID 0"</pcVariable>
<pcVariable digits="0" name="rpmhigh" units="rpm">9000.0</pcVariable>
<pcVariable digits="0" name="rpmwarn" units="rpm">3000.0</pcVariable>
<pcVariable digits="0" name="rpmdang" units="rpm">5000.0</pcVariable>
<pcVariable digits="0" name="loadhigh">400.0</pcVariable>
<pcVariable name="wue_lpg">"No"</pcVariable>
<pcVariable digits="0" name="vehigh" units="%">255.0</pcVariable>
<pcVariable name="clt_exp">"Normal"</pcVariable>
<pcVariable name="scatterRuntimeEnabled">"Enabled"</pcVariable>
<pcVariable name="prefSpeedUnits">"MPH"</pcVariable>
<pcVariable name="prefLengthUnits">"m"</pcVariable>
<pcVariable name="tsSpeedSource">"GPS Speed"</pcVariable>
<pcVariable digits="0" name="tsPrimaryInjectorSize">0.0</pcVariable>
<pcVariable name="tsInjSizeConstant">"cc/min"</pcVariable>
<pcVariable name="tsLogPowerFields">"Log HP &amp; Tq"</pcVariable>
<pcVariable name="tsLogPerfFields">"Off"</pcVariable>
<pcVariable name="tsFuelConsumptionUnits">"US Gallons"</pcVariable>
<pcVariable name="tsDistanceUnits">"Miles Per Hour"</pcVariable>
<pcVariable digits="0" name="tsVehicleWeight">3450.0</pcVariable>
<pcVariable name="tsWeightUnits">"lbs"</pcVariable>
<pcVariable digits="2" name="tsVehicleDragCoef">0.34</pcVariable>
<pcVariable digits="0" name="tsTirePressure" units="psi">32.0</pcVariable>
<pcVariable digits="1" name="tsFrontalArea">19.3</pcVariable>
<pcVariable name="tsFrontalUnits">"sqft"</pcVariable>
<pcVariable digits="1" name="tsTireDiameter" units="in">25.5</pcVariable>
<pcVariable digits="2" name="tsTransGearRatio" units=":1">1.0</pcVariable>
<pcVariable digits="2" name="tsFinalDriveRatio" units=":1">3.7</pcVariable>
<pcVariable digits="0" name="tsEtRollOut" units="in">0.0</pcVariable>
<pcVariable cols="1" digits="1" name="wueAfrTargetOffset" rows="10" units=":1">
         -1.5 
         -1.1 
         -0.8 
         -0.6 
         -0.5 
         -0.4 
         -0.3 
         -0.2 
         -0.1 
         0.0 
      </pcVariable>
<pcVariable cols="1" digits="0" name="wueAnalRecommend" rows="10" units="%">
         170.0 
         165.0 
         160.0 
         151.0 
         139.0 
         114.0 
         108.0 
         104.0 
         102.0 
         100.0 
      </pcVariable>
</page>
<page number="0" size="1024">
<constant name="nCylinders">"4"</constant>
<constant digits="0" name="no_skip_pulses">3.0</constant>
<constant name="ICIgnCapture">"Falling Edge"</constant>
<constant name="engineType">"Even fire"</constant>
<constant name="spkout_hi_lo">"Going High (Inverted)"</constant>
<constant name="spkout_hi_lo2">"Going High"</constant>
<constant digits="1" name="max_coil_dur" units="ms">3.0</constant>
<constant digits="1" name="max_spk_dur" units="ms">1.0</constant>
<constant digits="0" name="crankingRPM" units="RPM">700.0</constant>
<constant digits="1" name="triggerOffset" units="deg">7.0</constant>
<constant digits="1" name="TpsBypassCLTRevlim" units="TPS %">90.0</constant>
<constant digits="1" name="map0" units="%">3.5</constant>
<constant digits="1" name="mapmax" units="%">416.5</constant>
<constant digits="1" name="clt0" units="°F">0.0</constant>
<constant digits="0" name="cltmult" units="%">100.0</constant>
<constant digits="1" name="mat0" units="°F">0.0</constant>
<constant digits="0" name="matmult" units="%">100.0</constant>
<constant digits="0" name="tpsMin" units="ADC">116.0</constant>
<constant digits="0" name="tpsMax" units="ADC">744.0</constant>
<constant digits="1" name="batt0" units="V">0.1</constant>
<constant digits="1" name="battmax" units="V">32.5</constant>
<constant digits="1" name="ego0" units="afr">0.0</constant>
<constant digits="0" name="egomult" units="%">100.0</constant>
<constant digits="1" name="baro0" units="kPa">9.3</constant>
<constant digits="1" name="baromax" units="kPa">260.9</constant>
<constant digits="1" name="bcor0" units="%">0.0</constant>
<constant digits="0" name="bcormult" units="%">0.0</constant>
<constant digits="0" name="iacfullopen" units="steps">250.0</constant>
<constant digits="2" name="reluctorteeth1">40.0</constant>
<constant name="IdleCtl">"PWM valve (2 or 3 wire)"</constant>
<constant name="IdleCtl_alg">"Open-loop (warmup)"</constant>
<constant name="IdleCtl_vss">"Use Engine State"</constant>
<constant name="IdleCtl_home">"Closed"</constant>
<constant digits="0" name="IACtstep" units="ms">3.0</constant>
<constant digits="0" name="IAC_tinitial_step" units="ms">5.0</constant>
<constant digits="0" name="IACminstep" units="steps">2.0</constant>
<constant digits="0" name="dwellduty" units="%">49.53</constant>
<constant digits="0" name="IACStart">160.0</constant>
<constant digits="1" name="IdleHyst" units="°F">5.0</constant>
<constant digits="0" name="IACcrankpos" units="steps">100.0</constant>
<constant digits="0" name="IACcrankxt" units="s">5.0</constant>
<constant name="IACcurlim">"Moving only"</constant>
<constant digits="2" name="reluctorteeth2">40.0</constant>
<constant digits="1" name="boosttol" units="kPa">40.0</constant>
<constant digits="1" name="OverBoostKpa2" units="kPa">100.0</constant>
<constant digits="0" name="fc_rpm_lower" units="rpm">1300.0</constant>
<constant name="OverBoostOption">"None"</constant>
<constant name="OverBoostOption_tol">"Off"</constant>
<constant name="hardware_spk">"Spark"</constant>
<constant name="hardware_fuel">"Inj A,B.."</constant>
<constant name="hardware_cam">"CMP"</constant>
<constant digits="1" name="OverBoostKpa" units="kPa">100.0</constant>
<constant digits="1" name="OverBoostHyst" units="kPa">10.0</constant>
<constant digits="1" name="N2Olaunchmaxmap" units="kPa">150.0</constant>
<constant digits="1" name="tpsThresh" units="%/s">20.0</constant>
<constant digits="0" name="mapThresh" units="kPa/s">999.0</constant>
<constant digits="0" name="taeColdA" units="%ReqFuel">20.0</constant>
<constant digits="0" name="taeColdM" units="%">130.0</constant>
<constant digits="2" name="taeTime" units="s">0.2</constant>
<constant digits="0" name="tpsasync_events" units="events">20.0</constant>
<constant digits="0" name="tdePct">100.0</constant>
<constant digits="1" name="floodClear" units="%">70.0</constant>
<constant digits="1" name="TPSOXLimit" units="%">70.0</constant>
<constant digits="0" name="tpsProportion" units="%">100.0</constant>
<constant name="baroCorr">"Initial MAP Reading"</constant>
<constant name="egoType">"Wide Band"</constant>
<constant digits="0" name="egoCount">16.0</constant>
<constant digits="0" name="egoDelta" units="%">1.0</constant>
<constant digits="0" name="oldegoLimit" units="%">15.0</constant>
<constant digits="3" name="EGOVtarget" units="Volts">0.44988</constant>
<constant name="tempUnits">"Coolant/MAT Tables in °F"</constant>
<constant digits="0" name="egonum">1.0</constant>
<constant digits="0" name="rtc_trim" units="ppm">0.0</constant>
<constant digits="1" name="fastIdleT" units="°F">140.0</constant>
<constant digits="1" name="egoTemp" units="°F">120.0</constant>
<constant digits="0" name="egoRPM" units="RPM">1300.0</constant>
<constant digits="2" name="reqFuel" units="ms">11.6</constant>
<constant digits="0" name="divider">2.0</constant>
<constant name="alternate">"Alternating"</constant>
<constant name="altcrank">"Every event"</constant>
<constant name="alternate_blend">"Off"</constant>
<constant digits="1" name="injPwmT" units="ms">1.040384</constant>
<constant digits="0" name="injPwmPd" units="us">66.0</constant>
<constant digits="0" name="injPwmP" units="%">75.0</constant>
<constant name="twoStroke">"Four-stroke"</constant>
<constant name="nInjectors">"4"</constant>
<constant digits="1" name="OddFireang">90.0</constant>
<constant digits="0" name="rpmLF">50.0</constant>
<constant digits="0" name="mapLF">80.0</constant>
<constant digits="0" name="tpsLF">80.0</constant>
<constant digits="0" name="egoLF">60.0</constant>
<constant digits="0" name="adcLF">90.0</constant>
<constant name="knk_pin_out">"Tach Out"</constant>
<constant digits="0" name="mafLF">50.0</constant>
<constant name="algorithm">"Speed Density"</constant>
<constant name="algorithm2">"Disabled"</constant>
<constant name="IgnAlgorithm">"Speed Density"</constant>
<constant name="IgnAlgorithm2">"Disabled"</constant>
<constant digits="0" name="AfrAlgorithm">1.0</constant>
<constant digits="1" name="dwelltime" units="ms">1.0</constant>
<constant digits="1" name="trigret_ang" units="deg">50.0</constant>
<constant name="RevLimOption_retard">"Progressive retard"</constant>
<constant name="RevLimOption_spkcut">"On"</constant>
<constant name="RevLimCLTbased">"Normal"</constant>
<constant name="RevLimOption_fuelprog">"Off"</constant>
<constant name="RevLimOption_fuelcut">"Off"</constant>
<constant digits="0" name="RevLimMaxRtd" units="deg">12.0</constant>
<constant digits="0" name="ego_startdelay" units="s">60.0</constant>
<constant name="can_poll2_gps">"Off"</constant>
<constant name="can_poll2_vss">"Listen"</constant>
<constant name="can_poll2_egolag">"Off"</constant>
<constant name="opt142_rtc">"On-board"</constant>
<constant name="opt142_gs_share">"Off"</constant>
<constant digits="1" name="injPwmT2" units="ms">1.040384</constant>
<constant digits="0" name="injPwmPd2" units="us">66.0</constant>
<constant digits="0" name="injPwmP2" units="%">75.0</constant>
<constant digits="0" name="can_ego_id">5.0</constant>
<constant digits="0" name="can_ego_table">7.0</constant>
<constant digits="0" name="can_ego_offset" units="bytes">153.0</constant>
<constant digits="1" name="baro_upper" units="kPa">105.0</constant>
<constant digits="1" name="baro_lower" units="kPa">80.0</constant>
<constant digits="1" name="baro_default" units="kPa">100.0</constant>
<constant name="can_poll2_ego2">"Disable"</constant>
<constant digits="0" name="launchcutzone" units="RPM">200.0</constant>
<constant digits="0" name="RevLimNormal2" units="RPM">7200.0</constant>
<constant digits="0" name="hw_latency" units="usec">40.0</constant>
<constant name="loadCombine">"multiplicitive"</constant>
<constant name="loadMult">"multiply"</constant>
<constant name="loadStoich">"include AFRtarget"</constant>
<constant name="loadCombineign">"additive"</constant>
<constant name="loadMult2">"don't multiply"</constant>
<constant name="loadopts_oldbaro">"Off"</constant>
<constant digits="0" name="baud">115200.0</constant>
<constant digits="2" name="MAPOXLimit" units="%">90.0</constant>
<constant digits="0" name="can_poll_id_rtc">5.0</constant>
<constant digits="0" name="mycan_id">0.0</constant>
<constant digits="0" name="mapsample_percent" units="%">50.0</constant>
<constant digits="0" name="can_poll_id_ports">5.0</constant>
<constant digits="0" name="can_poll_id">5.0</constant>
<constant digits="2" name="aeTaperTime" units="s">0.0</constant>
<constant digits="0" name="tpsasync2_events" units="events">0.0</constant>
<constant digits="0" name="aeEndPW" units="%ReqFuel">0.0</constant>
<constant name="egoAlgorithm">"Simple"</constant>
<constant name="egoAlgorithm_auth">"On"</constant>
<constant name="egoAlgorithm_delay_table">"Use IGN events"</constant>
<constant digits="0" name="egoKP" units="%">100.0</constant>
<constant digits="0" name="egoKI" units="%">20.0</constant>
<constant digits="0" name="egoKD" units="%">0.0</constant>
<constant digits="0" name="ac_idleup_vss_offpoint" units="MPH">39.81682</constant>
<constant digits="0" name="ac_idleup_vss_hyst" units="MPH">4.92118</constant>
<constant name="flexFuel">"Disabled"</constant>
<constant name="flexport">"Digital Switched In 1"</constant>
<constant cols="1" digits="0" name="fuelFreq" rows="2" units="Hz">
         50.0 
         150.0 
      </constant>
<constant digits="0" name="fuelFreq0" units="Hz">50.0</constant>
<constant digits="0" name="fuelFreq1" units="Hz">150.0</constant>
<constant cols="1" digits="0" name="fuelCorr" rows="2" units="%">
         100.0 
         163.0 
      </constant>
<constant digits="0" name="fuelCorr0" units="%">100.0</constant>
<constant digits="0" name="fuelCorr1" units="%">163.0</constant>
<constant name="dwellmode">"Standard Dwell"</constant>
<constant digits="0" name="pwmidle_shift_lower_rpm" units="rpm">8000.0</constant>
<constant digits="1" name="ac_idleup_tps_offpoint" units="%">70.0</constant>
<constant digits="1" name="ac_idleup_tps_hyst" units="%">10.0</constant>
<constant digits="1" name="fan_idleup_tps_offpoint" units="%">70.0</constant>
<constant digits="1" name="fan_idleup_tps_hyst" units="%">10.0</constant>
<constant digits="0" name="fan_idleup_vss_offpoint" units="MPH">70.01497</constant>
<constant name="knk_option">"Disabled"</constant>
<constant name="knk_option_an">"Analogue"</constant>
<constant name="knkDirection">"Low Input"</constant>
<constant name="knkpull">"Pull up"</constant>
<constant name="knk_option_wind">"At end"</constant>
<constant digits="1" name="knk_maxrtd" units="deg">10.0</constant>
<constant digits="1" name="knk_step1" units="deg">3.0</constant>
<constant digits="1" name="knk_step2" units="deg">1.0</constant>
<constant digits="1" name="knk_trtd" units="s">0.2</constant>
<constant digits="1" name="knk_tadv" units="s">2.0</constant>
<constant digits="1" name="knk_dtble_adv" units="deg">3.0</constant>
<constant digits="0" name="knk_ndet" units="knocks">2.0</constant>
<constant name="EAEOption">"Off"</constant>
<constant name="knkport">"Digital Switched In 3"</constant>
<constant digits="1" name="knk_maxmap" units="kPa">70.0</constant>
<constant digits="0" name="knk_lorpm" units="rpm">700.0</constant>
<constant digits="0" name="knk_hirpm" units="rpm">3500.0</constant>
<constant digits="0" name="triggerTeeth" units="teeth">36.0</constant>
<constant digits="0" name="No_Miss_Teeth" units="teeth">1.0</constant>
<constant digits="0" name="pwmidle_shift_open_time" units="s">0.0</constant>
<constant digits="1" name="Miss_ang" units="deg BTDC">80.0</constant>
<constant digits="1" name="ICISR_tmask" units="ms">0.1</constant>
<constant digits="0" name="ICISR_pmask" units="%">10.0</constant>
<constant digits="0" name="ae_lorpm" units="rpm">5500.0</constant>
<constant digits="0" name="ae_hirpm" units="rpm">6000.0</constant>
<constant cols="1" digits="1" name="fuelSpkDel" rows="2" units="deg">
         0.0 
         3.5 
      </constant>
<constant digits="1" name="fuelSpkDel0" units="deg">0.0</constant>
<constant digits="1" name="fuelSpkDel1" units="deg">3.5</constant>
<constant name="spk_conf2_gmtfi">"Off"</constant>
<constant name="spk_conf2_oddodd">"Alternate"</constant>
<constant name="spk_conf2_dwell">"Off"</constant>
<constant name="spk_conf2_dwelltbl">"Off"</constant>
<constant name="spk_conf2_dli">"Off"</constant>
<constant name="spk_config_campol">"Low"</constant>
<constant name="spk_config_camcrank">"Crank wheel"</constant>
<constant name="spk_config_trig2">"Single wheel with missing tooth"</constant>
<constant name="spk_config_trig2l">"Falling edge"</constant>
<constant name="spk_config_resetcam">"Cam"</constant>
<constant name="spk_mode0">"Miata 99-05"</constant>
<constant name="spk_mode3_trim">"Off"</constant>
<constant name="spk_mode3_tach3">"CMP"</constant>
<constant name="spk_mode3_hirespol">"Normal"</constant>
<constant name="spk_mode3_kick">"Off"</constant>
<constant name="spk_mode3">"Wasted spark"</constant>
<constant name="rtbaroport">"MAP"</constant>
<constant name="ego2port">"MAP"</constant>
<constant name="mapport">"MAP"</constant>
<constant name="mapport_t">"Voltage"</constant>
<constant name="mapport_f">"Digital Frequency In 1"</constant>
<constant name="knkport_an">"Analog In 3"</constant>
<constant name="OvrRunC">"Off"</constant>
<constant name="OvrRunC_progcut">"Off"</constant>
<constant name="OvrRunC_progret">"Off"</constant>
<constant name="OvrRunC_progign">"Off"</constant>
<constant name="OvrRunC_retign">"Off"</constant>
<constant digits="0" name="poll_level_tooth">0.0</constant>
<constant name="feature4_0igntrig">"Off"</constant>
<constant name="feature4_0maxdwl">"Off"</constant>
<constant name="feature4_0ftrig">"Off"</constant>
<constant name="feature4_0mindwl">"Off"</constant>
<constant name="timing_flags">"Use Table"</constant>
<constant name="use_prediction">"1st Deriv Prediction"</constant>
<constant digits="1" name="crank_dwell" units="ms">6.0</constant>
<constant name="tsw_pin_f">"Digital Switched In 3"</constant>
<constant digits="1" name="crank_timing" units="degrees">15.0</constant>
<constant digits="1" name="fixed_timing" units="degrees">10.0</constant>
<constant digits="0" name="tsf_rpm" units="rpm">6000.0</constant>
<constant digits="1" name="tsf_kpa" units="kPa">100.0</constant>
<constant digits="1" name="tsf_tps" units="%">80.0</constant>
<constant digits="0" name="tss_rpm" units="rpm">6001.0</constant>
<constant digits="1" name="tss_kpa" units="kPa">100.1</constant>
<constant digits="1" name="tss_tps" units="%">80.1</constant>
<constant name="f5_0_tsf">"Off"</constant>
<constant name="f5_0_tsf_opt">"Hardware"</constant>
<constant name="f5_0_tss">"Off"</constant>
<constant name="f5_0_tss_opt">"Hardware"</constant>
<constant name="tsw_pin_s">"Digital Switched In 3"</constant>
<constant digits="0" name="pwmidlecranktaper" units="s">9.0</constant>
<constant digits="1" name="knk_step_adv" units="deg">2.0</constant>
<constant digits="0" name="fc_rpm_upper" units="rpm">1400.0</constant>
<constant digits="1" name="fc_clt" units="°F">160.0</constant>
<constant digits="1" name="fc_delay" units="s">2.0</constant>
<constant name="tacho_opt3f">"Tach Out"</constant>
<constant digits="0" name="fc_ego_delay" units="s">0.0</constant>
<constant name="tacho_opt80">"On"</constant>
<constant name="tacho_optvar">"Fixed"</constant>
<constant name="tacho_opt40">"Normal"</constant>
<constant digits="1" name="tacho_scale" units="%">100.0</constant>
<constant name="feature3_tps">"Off"</constant>
<constant name="feature3_aseunit">"Cycles"</constant>
<constant name="feature3_maplog">"Off"</constant>
<constant name="feature3_3">"Off"</constant>
<constant name="feature3_pw4x">"Normal"</constant>
<constant name="feature3_n2oin">"On"</constant>
<constant name="feature3_matase">"Off"</constant>
<constant name="feature3_dwell">"Off"</constant>
<constant name="launch_opt_vss">"Off"</constant>
<constant name="launch_opt_vssgear">"Off"</constant>
<constant name="launch_opt_retard">"Off"</constant>
<constant name="launch_opt_bank">"Off"</constant>
<constant name="launch_opt_on">"Off"</constant>
<constant digits="0" name="launch_sft_zone" units="RPM">200.0</constant>
<constant digits="2" name="launch_sft_deg" units="deg">3.0</constant>
<constant digits="0" name="launch_hrd_lim" units="RPM">3000.0</constant>
<constant digits="0" name="launch_tps" units="%">10.0</constant>
<constant name="launchlimopt">"Spark Cut"</constant>
<constant name="launchlimopt_adv">"Basic"</constant>
<constant name="launchlimopt_cut">"Random Progressive"</constant>
<constant digits="0" name="launchvsstime" units="s">10.0</constant>
<constant digits="0" name="launchvss_maxgear">6.0</constant>
<constant name="launch_opt_pins">"Digital Switched In 1"</constant>
<constant digits="0" name="flats_arm" units="RPM">3000.0</constant>
<constant digits="1" name="launchvss_minvss" units="MPH">2.2369</constant>
<constant digits="2" name="flats_deg" units="deg">5.0</constant>
<constant digits="0" name="flats_hrd" units="RPM">4800.0</constant>
<constant digits="0" name="staged_pri_size" units="cc">265.0</constant>
<constant digits="0" name="staged_sec_size" units="cc">600.0</constant>
<constant name="staged_first_param">"Off"</constant>
<constant name="staged_second_param">"Off"</constant>
<constant name="staged_transition_on">"Off"</constant>
<constant name="staged_second_logic">"OR"</constant>
<constant name="staged_pw1_0">"Off"</constant>
<constant digits="0" name="staged_transition_events" units="ign events">0.0</constant>
<constant digits="0" name="staged_param_1" units="units">0.0</constant>
<constant digits="0" name="staged_param_2" units="units">0.0</constant>
<constant digits="0" name="staged_hyst_1" units="units">0.0</constant>
<constant digits="0" name="staged_hyst_2" units="units">0.0</constant>
<constant name="N2Oopt_01">"Both"</constant>
<constant name="N2Oopt_2">"Off"</constant>
<constant name="N2Oopt_3">"Off"</constant>
<constant name="N2Oopt_4">"Off"</constant>
<constant name="N2Oopt_5">"Off"</constant>
<constant name="N2Oopt2_prog_time">"RPM-based"</constant>
<constant name="N2Oopt2_prog">"On/Off"</constant>
<constant name="N2Oopt2_fuel">"Use N2O duty"</constant>
<constant name="N2Oopt2_prog_freq">"11.1Hz"</constant>
<constant name="N2Oopt2_prog_freqf">"Same"</constant>
<constant digits="0" name="N2ORpm" units="RPM">3000.0</constant>
<constant digits="0" name="N2ORpmMax" units="RPM">6000.0</constant>
<constant digits="1" name="N2OTps" units="%">80.0</constant>
<constant digits="1" name="N2OClt" units="°F">150.0</constant>
<constant digits="2" name="N2OAngle" units="deg">10.0</constant>
<constant digits="3" name="N2OPWLo" units="ms">6.0</constant>
<constant digits="3" name="N2OPWHi" units="ms">3.0</constant>
<constant digits="2" name="N2Odel_launch" units="s">0.0</constant>
<constant digits="2" name="N2Odel_flat" units="s">0.0</constant>
<constant digits="2" name="N2Oholdon" units="s">0.0</constant>
<constant digits="2" name="N2O2delay" units="s">0.5</constant>
<constant digits="0" name="N2O2Rpm" units="RPM">5000.0</constant>
<constant digits="0" name="N2O2RpmMax" units="RPM">6000.0</constant>
<constant digits="2" name="N2O2Angle" units="deg">1.0</constant>
<constant digits="3" name="N2O2PWLo" units="ms">2.0</constant>
<constant digits="3" name="N2O2PWHi" units="ms">1.0</constant>
<constant name="RotarySplitModeFD">"FC mode"</constant>
<constant name="RotarySplitModeNeg">"Not Allowed"</constant>
<constant digits="0" name="dlyct">4.0</constant>
<constant digits="1" name="dwelltime_trl" units="ms">3.0</constant>
<constant name="N2Oopt_pins">"Digital Switched 12V In"</constant>
<constant digits="1" name="RevLimRtdAng" units="deg">1.0</constant>
<constant digits="0" name="vss4_can_offset">0.0</constant>
<constant digits="0" name="RevLimNormal2_hyst" units="RPM">100.0</constant>
<constant name="pwmidleset_inv">"Normal, 0%=off"</constant>
<constant digits="0" name="trig_init">1.0</constant>
<constant digits="0" name="pwmidle_ms" units="ms">100.0</constant>
<constant digits="0" name="pwmidle_close_delay" units="s">3.0</constant>
<constant digits="1" name="pwmidle_open_duty" units="%">59.976</constant>
<constant digits="0" name="pwmidle_open_steps" units="steps">153.0</constant>
<constant digits="1" name="pwmidle_closed_duty" units="%">14.896</constant>
<constant digits="0" name="pwmidle_closed_steps" units="steps">38.0</constant>
<constant digits="0" name="pwmidle_pid_wait_timer" units="s">3.0</constant>
<constant name="pwmidle_freq_pin3">"Off"</constant>
<constant name="pwmidle_freq_koeo">"On"</constant>
<constant digits="0" name="ac_idleup_min_rpm" units="rpm">300.0</constant>
<constant name="pwmidle_flags_wot">"Off"</constant>
<constant digits="1" name="pwmidle_dp_adder" units="%">3.136</constant>
<constant digits="0" name="pwmidle_dp_adder_steps" units="steps">8.0</constant>
<constant digits="1" name="pwmidle_Kp_new" units="%">30.0</constant>
<constant digits="1" name="pwmidle_Ki_new" units="%">30.0</constant>
<constant digits="1" name="pwmidle_Kd_new" units="%">0.0</constant>
<constant name="pwmidle_freq_scale">"306Hz"</constant>
<constant name="pwmidle_freq_pin">"PWM / Idle Out 1"</constant>
<constant name="boost_ctl_settings_freq">"78Hz"</constant>
<constant name="boost_ctl_settings_on">"Off"</constant>
<constant name="boost_ctl_settings_cl">"Open-loop"</constant>
<constant name="boost_ctl_settings_invert_new">"Normal"</constant>
<constant name="boost_ctl_settings_dome">"Single Solenoid"</constant>
<constant name="boost_ctl_pins">"High Current Out 3"</constant>
<constant digits="0" name="boost_ctl_Kp" units="%">100.0</constant>
<constant digits="0" name="boost_ctl_Ki" units="%">0.0</constant>
<constant digits="0" name="boost_ctl_Kd" units="%">0.0</constant>
<constant digits="0" name="boost_ctl_closeduty" units="%">0.0</constant>
<constant digits="0" name="boost_ctl_openduty" units="%">100.0</constant>
<constant name="boost_ctl_pwm_scale">"12Hz"</constant>
<constant name="boost_ctl_pwm">"Slow"</constant>
<constant name="NoiseFilterOpts">"Off"</constant>
<constant name="NoiseFilterOpts1">"Off"</constant>
<constant name="NoiseFilterOpts2">"Off"</constant>
<constant name="NoiseFilterOpts3">"Off"</constant>
<constant digits="1" name="launchcuttiming" units="deg">9.0</constant>
<constant digits="0" name="pwmidle_max_rpm_new">259.0</constant>
<constant digits="0" name="pwmidle_targ_ramptime" units="s">3.0</constant>
<constant name="boost_ctl_pins_pwm">"High Current Out 3"</constant>
<constant name="vss_opt1">"Digital Frequency In 2"</constant>
<constant name="vss_opt2">"Digital Switched In 3"</constant>
<constant name="vss_opt3">"Digital Switched In 2"</constant>
<constant name="vss_opt4">"Off"</constant>
<constant name="secondtrigopts">"Off"</constant>
<constant name="secondtrigopts1">"Off"</constant>
<constant name="secondtrigopts2">"Off"</constant>
<constant name="secondtrigopts3">"Off"</constant>
<constant digits="0" name="TC5_required_width" units="uSec">416.0</constant>
<constant digits="0" name="egoLimit" units="%">10.0</constant>
<constant digits="1" name="stoich" units="AFR">14.7</constant>
<constant digits="2" name="MAPOXMin" units="%">20.0</constant>
<constant digits="1" name="IC2ISR_tmask" units="ms">0.2</constant>
<constant digits="0" name="IC2ISR_pmask" units="%">20.0</constant>
<constant name="afrload">"Use primary load (Algorithm)"</constant>
<constant name="eaeload">"Use primary load (Algorithm)"</constant>
<constant digits="0" name="fan_idleup_vss_hyst" units="MPH">4.92118</constant>
<constant name="log_style_led">"Off"</constant>
<constant digits="1" name="primedelay" units="s">0.0</constant>
<constant name="pwmidle_cl_opts_initvaluetable">"Use last value"</constant>
<constant name="pwmidle_cl_opts_initval_clt">"Use MAT"</constant>
<constant name="pwmidle_cl_opts_display_pid">"Basic"</constant>
<constant name="boost_ctl_flags">"Basic Mode"</constant>
<constant name="boost_ctl_flags2">"Basic Mode"</constant>
<constant name="idleveadv_to_pid_idleadv">"Use Engine State"</constant>
<constant name="idleveadv_to_pid_idleve">"Use Engine State"</constant>
<constant digits="1" name="boost_ctl_sensitivity">200.0</constant>
<constant digits="1" name="boost_ctl_sensitivity2">200.0</constant>
<constant digits="0" name="fuelcut_fuelon_upper_rpmdot" units="rpmdot">2000.0</constant>
<constant digits="0" name="fuelcut_fuelon_lower_rpmdot" units="rpmdot">100.0</constant>
<constant digits="3" name="staged_secondary_enrichment" units="ms">0.0</constant>
<constant digits="0" name="staged_primary_delay" units="ign events">0.0</constant>
<constant name="idleadvance_on">"Off"</constant>
<constant name="idleve_on">"On"</constant>
<constant name="idleadv_vsson">"Off"</constant>
<constant name="idle_special_ops_timing_assist">"Off"</constant>
<constant digits="1" name="idleadvance_clt" units="°F">140.0</constant>
<constant digits="0" name="idleadvance_delay" units="s">4.0</constant>
<constant cols="1" digits="1" name="idleadvance_curve" rows="4" units="deg">
         17.0 
         19.0 
         21.0 
         23.0 
      </constant>
<constant cols="1" digits="1" name="idleadvance_loads" rows="4" units="%">
         34.0 
         36.0 
         38.0 
         40.0 
      </constant>
<constant name="log_style2_but">"Digital Frequency In 3"</constant>
<constant name="log_style_block">"64 byte"</constant>
<constant name="log_style_gps">"Off"</constant>
<constant name="log_style_on2">"Always"</constant>
<constant name="log_style2_cont">"Start new log"</constant>
<constant name="log_style2_alwaysin">"Use detect switch"</constant>
<constant name="log_style2_samp">"Timed"</constant>
<constant name="log_style2_clg">"Off"</constant>
<constant name="log_style_ledspd">"Fastest"</constant>
<constant name="log_style2_ledspd">"Fastest"</constant>
<constant name="log_style3_adc">"INT_MAP"</constant>
<constant digits="0" name="log_length" units="mins">10.0</constant>
<constant digits="1" name="log_int" units="ms">19.968</constant>
<constant digits="0" name="log_rate">50.0801282</constant>
<constant digits="0" name="testval1">0.0</constant>
<constant digits="0" name="testval2">0.0</constant>
<constant digits="0" name="firea">1.0</constant>
<constant digits="0" name="fireb">3.0</constant>
<constant digits="0" name="firec">4.0</constant>
<constant digits="0" name="fired">2.0</constant>
<constant digits="0" name="firee">0.0</constant>
<constant digits="0" name="firef">0.0</constant>
<constant digits="0" name="fireg">0.0</constant>
<constant digits="0" name="fireh">0.0</constant>
<constant digits="0" name="firei">0.0</constant>
<constant digits="0" name="firej">0.0</constant>
<constant digits="0" name="firek">0.0</constant>
<constant digits="0" name="firel">0.0</constant>
<constant digits="0" name="firem">0.0</constant>
<constant digits="0" name="firen">0.0</constant>
<constant digits="0" name="fireo">0.0</constant>
<constant digits="0" name="firep">0.0</constant>
<constant name="sequential">"Fully Sequential"</constant>
<constant name="sequential_angle_spec">"End of squirt"</constant>
<constant name="sequential_trim_on_off">"Off"</constant>
<constant digits="0" name="boost_launch_duty" units="%">0.0</constant>
<constant digits="1" name="boost_launch_target" units="kPa">100.0</constant>
<constant name="boost_feats_tsw">"Off"</constant>
<constant name="boost_feats_launch">"Off"</constant>
<constant name="boost_feats_timed">"Off"</constant>
<constant name="launch_3step_in">"Off"</constant>
<constant digits="0" name="launch_var_low" units="rpm">3000.0</constant>
<constant digits="0" name="launch_var_up" units="rpm">5000.0</constant>
<constant digits="0" name="vssout_scale">300.0</constant>
<constant digits="2" name="launch_sft_deg3" units="deg">5.0</constant>
<constant digits="0" name="launch_hrd_lim3" units="RPM">4000.0</constant>
<constant digits="1" name="map_sample_duration" units="deg">10.0</constant>
<constant name="opentime_opt1_master">"Same"</constant>
<constant name="opentime_opt1">"Curve 1"</constant>
<constant name="opentime_opt2">"Curve 1"</constant>
<constant name="opentime_opt3">"Curve 1"</constant>
<constant name="opentime_opt4">"Curve 1"</constant>
<constant name="opentime_opt5">"Curve 1"</constant>
<constant name="opentime_opt6">"Curve 1"</constant>
<constant name="opentime_opt7">"Curve 1"</constant>
<constant name="opentime_opt8">"Curve 1"</constant>
<constant name="opentime_opta">"Curve 1"</constant>
<constant name="opentime_opta_pwm">"Off"</constant>
<constant name="opentime_optb">"Curve 1"</constant>
<constant name="opentime_optb_pwm">"Off"</constant>
<constant name="opentime_optb_own">"Off"</constant>
<constant name="opentime_opt11">"Curve 1"</constant>
<constant name="opentime_opt12">"Curve 1"</constant>
<constant name="opentime_opt13">"Curve 1"</constant>
<constant name="opentime_opt14">"Curve 1"</constant>
<constant name="opentime_opt15">"Curve 1"</constant>
<constant name="opentime_opt16">"Curve 1"</constant>
<constant name="smallpw_opt1_master">"Off"</constant>
<constant name="smallpw_opt1">"Curve 1"</constant>
<constant name="smallpw_opt2">"Curve 1"</constant>
<constant name="smallpw_opt3">"Curve 1"</constant>
<constant name="smallpw_opt4">"Curve 1"</constant>
<constant name="smallpw_opt5">"Curve 1"</constant>
<constant name="smallpw_opt6">"Curve 1"</constant>
<constant name="smallpw_opt7">"Curve 1"</constant>
<constant name="smallpw_opt8">"Curve 1"</constant>
<constant name="smallpw_opta">"Curve 1"</constant>
<constant name="smallpw_optb">"Curve 1"</constant>
<constant name="smallpw_opt11">"Curve 1"</constant>
<constant name="smallpw_opt12">"Curve 1"</constant>
<constant name="smallpw_opt13">"Curve 1"</constant>
<constant name="smallpw_opt14">"Curve 1"</constant>
<constant name="smallpw_opt15">"Curve 1"</constant>
<constant name="smallpw_opt16">"Curve 1"</constant>
<constant name="maxafr_opt1_on">"Off"</constant>
<constant name="maxafr_opt1_load">"MAP"</constant>
<constant name="maxafr_opt1_led">"Off"</constant>
<constant digits="1" name="maxafr_en_load" units="%">100.0</constant>
<constant digits="0" name="maxafr_en_rpm" units="rpm">2500.0</constant>
<constant digits="1" name="maxafr_en_time" units="s">0.5</constant>
<constant digits="2" name="maxafr_spkcut_time" units="s">0.5</constant>
<constant digits="1" name="maxafr_ret_tps" units="%">20.0</constant>
<constant digits="1" name="maxafr_ret_map" units="%">95.0</constant>
<constant digits="1" name="maxafr_ret_rpm" units="rpm">2000.0</constant>
<constant digits="3" name="launch_addfuel" units="ms">0.0</constant>
<constant digits="3" name="wheeldia1" units="m">0.656</constant>
<constant digits="3" name="wheeldia2" units="m">0.656</constant>
<constant digits="2" name="fdratio1" units=":1">4.11</constant>
<constant name="vss1_pos">"Pulses per mile"</constant>
<constant name="vss2_pos">"Wheel"</constant>
<constant name="launch_var_on">"Off"</constant>
<constant digits="0" name="flats_minvss" units="MPH">0.0</constant>
<constant name="vss1_an">"Analog In 3"</constant>
<constant digits="0" name="vss1_can_id">7.0</constant>
<constant name="tsw_pin_ob">"Off"</constant>
<constant digits="0" name="vss1_can_offset">4.0</constant>
<constant digits="0" name="vss2_can_offset">4.0</constant>
<constant digits="0" name="MapThreshXTD" units="-kpa/sec">40.0</constant>
<constant digits="0" name="MapThreshXTD2" units="-kpa/sec">60.0</constant>
<constant name="vss_opt0_1">"Digital"</constant>
<constant name="vss_opt0_2">"Off"</constant>
<constant name="vss_opt0_3">"Off"</constant>
<constant name="vss_opt0_4">"Off"</constant>
<constant name="ss_opt1">"Off"</constant>
<constant name="ss_opt1_spd">"Off"</constant>
<constant name="vss2_an">"Analog In 3"</constant>
<constant digits="0" name="ss1_pwmseq">1.0</constant>
<constant digits="0" name="ss2_pwmseq">1.0</constant>
<constant digits="0" name="gear_can_offset">0.0</constant>
<constant name="mapsample_opt1">"1"</constant>
<constant name="mapsample_opt2">"Use event average"</constant>
<constant name="map2port">"Off"</constant>
<constant name="n2o1n_pins">"High Current Out 1"</constant>
<constant name="n2o1f_pins">"High Current Out 1"</constant>
<constant name="n2o2n_pins">"High Current Out 2"</constant>
<constant name="n2o2f_pins">"High Current Out 2"</constant>
<constant digits="0" name="vss1_an_max" units="MPH">149.64861</constant>
<constant digits="0" name="vss2_an_max" units="MPH">149.64861</constant>
<constant name="tsw_pin_rf">"Off"</constant>
<constant name="tsw_pin_afr">"Off"</constant>
<constant name="tsw_pin_stoich">"Off"</constant>
<constant name="boost_vss">"Off"</constant>
<constant digits="2" name="ReqFuel_alt" units="ms">15.0</constant>
<constant digits="1" name="stoich_alt" units="AFR">14.7</constant>
<constant name="water_pins_pump">"Off"</constant>
<constant name="water_pins_valve">"Off"</constant>
<constant name="water_pins_in_shut">"Off"</constant>
<constant name="water_freq_on">"Off"</constant>
<constant name="water_freq">"13Hz"</constant>
<constant name="water_freq_type">"Off"</constant>
<constant digits="0" name="boost_vss_tps" units="%">0.0</constant>
<constant digits="0" name="water_tps" units="%">70.0</constant>
<constant digits="0" name="water_rpm" units="RPM">1500.0</constant>
<constant digits="1" name="water_map" units="kPa">90.0</constant>
<constant digits="1" name="water_mat" units="°F">60.0</constant>
<constant digits="1" name="boost_ctl_lowerlimit" units="kPa">100.0</constant>
<constant name="enable_pollADC">"Disable"</constant>
<constant name="enable_pollPWM">"Disable"</constant>
<constant name="enable_pollports_digin">"Disable"</constant>
<constant name="enable_pollports_digout">"Disable"</constant>
<constant name="enable_pwmout">"Disable"</constant>
<constant name="enable_pwmout255">"Disable"</constant>
<constant digits="0" name="poll_table_rtc">7.0</constant>
<constant digits="0" name="poll_tablePWM">7.0</constant>
<constant digits="0" name="poll_tableports">7.0</constant>
<constant digits="0" name="poll_offset_rtc" units="bytes">110.0</constant>
<constant digits="0" name="poll_offsetPWM" units="bytes">58.0</constant>
<constant digits="0" name="can_poll_digin_offset" units="bytes">77.0</constant>
<constant digits="0" name="can_poll_digout_offset" units="bytes">75.0</constant>
<constant name="egt_num">"Off"</constant>
<constant name="accXport">"Off"</constant>
<constant name="accYport">"Off"</constant>
<constant name="accZport">"Off"</constant>
<constant digits="0" name="accXcal1" units="ADC">217.0</constant>
<constant digits="0" name="accXcal2" units="ADC">483.0</constant>
<constant digits="0" name="accYcal1" units="ADC">217.0</constant>
<constant digits="0" name="accYcal2" units="ADC">483.0</constant>
<constant digits="0" name="accZcal1" units="ADC">217.0</constant>
<constant digits="0" name="accZcal2" units="ADC">483.0</constant>
<constant digits="0" name="accxyzLF" units="%">50.0</constant>
<constant name="egt1port">"CAN ADC09"</constant>
<constant name="egt2port">"CAN ADC10"</constant>
<constant name="egt3port">"CAN ADC11"</constant>
<constant name="egt4port">"CAN ADC12"</constant>
<constant name="egt5port">"CAN ADC13"</constant>
<constant name="egt6port">"CAN ADC14"</constant>
<constant name="egt7port">"CAN ADC15"</constant>
<constant name="egt8port">"CAN ADC16"</constant>
<constant name="egt9port">"CAN ADC17"</constant>
<constant name="egt10port">"CAN ADC18"</constant>
<constant name="egt11port">"CAN ADC19"</constant>
<constant name="egt12port">"CAN ADC20"</constant>
<constant name="egt13port">"CAN ADC21"</constant>
<constant name="egt14port">"CAN ADC22"</constant>
<constant name="egt15port">"CAN ADC23"</constant>
<constant name="egt16port">"CAN ADC24"</constant>
<constant name="egt_conf_action">"Off"</constant>
<constant name="egt_conf_shutdown">"Off"</constant>
<constant name="egt_conf_bank">"Both"</constant>
<constant name="egt_conf_percyl">"Off"</constant>
<constant digits="0" name="egtcal_temp0" units="°F">32.0</constant>
<constant digits="0" name="egtcal_tempmax" units="°F">2282.0</constant>
<constant digits="0" name="egt_warn" units="°F">1620.0</constant>
<constant digits="0" name="egt_max" units="°F">1710.0</constant>
<constant digits="2" name="egt_time" units="s">0.02</constant>
<constant digits="1" name="vss1_can_scale" units="%">4000.0</constant>
<constant digits="0" name="vss1_can_scale_pulse">40000.0</constant>
<constant digits="1" name="vss2_can_scale" units="%">1000.0</constant>
<constant digits="0" name="vss2_can_scale_pulse">10000.0</constant>
<constant digits="0" name="vss1_pwmseq">1.0</constant>
<constant digits="0" name="vss2_pwmseq">2.0</constant>
<constant name="MAFOption">"Analog In 3"</constant>
<constant name="MAFOption_t">"Voltage"</constant>
<constant digits="0" name="enginesize" units="cc">1839.0</constant>
<constant name="vssout_opt">"Off"</constant>
<constant digits="0" name="vss3_can_offset">0.0</constant>
<constant name="vss1_can_size">"8bit"</constant>
<constant name="vss2_can_size">"8bit"</constant>
<constant name="vssout_optunits">"Time"</constant>
<constant name="MAFOption_f">"Digital Frequency In 1"</constant>
<constant digits="0" name="canpwm_clk" units="MHz">24.0</constant>
<constant digits="0" name="canpwm_pre">16.0</constant>
<constant digits="0" name="canpwm_div">3.0</constant>
<constant digits="0" name="vss1_can_table">7.0</constant>
<constant name="feature7_mafmat">"Off"</constant>
<constant name="feature7_maftrim">"Off"</constant>
<constant name="feature7_aeevents">"Time"</constant>
<constant name="feature7_aetpswot">"Off"</constant>
<constant name="feature7_batchcrank">"Off"</constant>
<constant name="feature7_cranktaper">"Off"</constant>
<constant name="feature7_crtpunits">"Events"</constant>
<constant digits="0" name="vss1LF">50.0</constant>
<constant digits="0" name="vss2LF">50.0</constant>
<constant digits="0" name="ss1LF">50.0</constant>
<constant digits="0" name="ss2LF">50.0</constant>
<constant digits="2" name="egt_addfuel" units="ms">0.0</constant>
<constant digits="0" name="launch_fcut_rpm" units="RPM">9000.0</constant>
<constant digits="2" name="gear1ratio" units=":1">3.32</constant>
<constant digits="2" name="gear2ratio" units=":1">2.09</constant>
<constant digits="2" name="gear3ratio" units=":1">1.4</constant>
<constant digits="2" name="gear4ratio" units=":1">1.0</constant>
<constant digits="2" name="gear5ratio" units=":1">0.83</constant>
<constant digits="2" name="gear6ratio" units=":1">0.5</constant>
<constant name="gear_method">"Off"</constant>
<constant name="gear_port_an">"Off"</constant>
<constant digits="2" name="gear0v" units="V">4.89</constant>
<constant digits="2" name="gear1v" units="V">1.78</constant>
<constant digits="2" name="gear2v" units="V">2.25</constant>
<constant digits="2" name="gear3v" units="V">2.96</constant>
<constant digits="2" name="gear4v" units="V">3.64</constant>
<constant digits="2" name="gear5v" units="V">4.33</constant>
<constant digits="2" name="gear6v" units="V">4.72</constant>
<constant digits="0" name="gear_no">5.0</constant>
<constant digits="0" name="vssdotLF">50.0</constant>
<constant digits="0" name="vssdot_int" units="ms">200.0</constant>
<constant name="ac_idleup_io_in">"Digital Switched In 3"</constant>
<constant name="ac_idleup_settings_inv">"Normal"</constant>
<constant name="ac_idleup_settings">"On"</constant>
<constant name="ac_idleup_io_out">"Injector Out J"</constant>
<constant digits="0" name="ac_idleup_delay" units="ms">500.0</constant>
<constant digits="1" name="ac_idleup_adder_duty" units="%">8.624</constant>
<constant digits="0" name="ac_idleup_adder_steps" units="steps">22.0</constant>
<constant name="fanctl_settings_pin">"Injector Out I"</constant>
<constant digits="0" name="fanctl_idleup_delay" units="ms">100.0</constant>
<constant digits="1" name="fanctl_idleup_adder_duty" units="%">1.568</constant>
<constant digits="0" name="fanctl_idleup_adder_steps" units="steps">4.0</constant>
<constant digits="1" name="fanctl_ontemp" units="°F">200.0</constant>
<constant digits="1" name="fanctl_offtemp" units="°F">190.0</constant>
<constant name="canadc_opt1">"Off"</constant>
<constant name="canadc_opt2">"Off"</constant>
<constant name="canadc_opt3">"Off"</constant>
<constant name="canadc_opt4">"Off"</constant>
<constant name="canadc_opt5">"Off"</constant>
<constant name="canadc_opt6">"Off"</constant>
<constant name="fanctl_opt2_engineoff">"Yes"</constant>
<constant name="fan_ctl_settings_acfan">"Turn fan on"</constant>
<constant name="fanctl_opt2_tps">"Off"</constant>
<constant name="fanctl_opt2_vss">"Off"</constant>
<constant name="fanctl_settings_idleup">"Yes"</constant>
<constant name="fanctl_settings_on">"On"</constant>
<constant digits="0" name="canadc_id1">5.0</constant>
<constant digits="0" name="canadc_id2">5.0</constant>
<constant digits="0" name="canadc_id3">5.0</constant>
<constant digits="0" name="canadc_id4">5.0</constant>
<constant digits="0" name="canadc_id5">5.0</constant>
<constant digits="0" name="canadc_id6">5.0</constant>
<constant digits="0" name="canadc_tab1">7.0</constant>
<constant digits="0" name="canadc_tab2">7.0</constant>
<constant digits="0" name="canadc_tab3">7.0</constant>
<constant digits="0" name="canadc_tab4">7.0</constant>
<constant digits="0" name="canadc_tab5">7.0</constant>
<constant digits="0" name="canadc_tab6">7.0</constant>
<constant digits="0" name="canadc_off1">2.0</constant>
<constant digits="0" name="canadc_off2">10.0</constant>
<constant digits="0" name="canadc_off3">18.0</constant>
<constant digits="0" name="canadc_off4">26.0</constant>
<constant digits="0" name="canadc_off5">34.0</constant>
<constant digits="0" name="canadc_off6">42.0</constant>
<constant digits="0" name="ac_idleup_cl_targetadder" units="rpm">300.0</constant>
<constant digits="0" name="fan_idleup_cl_targetadder" units="rpm">0.0</constant>
<constant digits="1" name="boost_ctl_clt_threshold" units="°F">170.0</constant>
<constant name="ac_idleup_set2_tps">"On"</constant>
<constant name="ac_idleup_set2_vss">"On"</constant>
<constant name="ac_idleup_set2_rpm">"On"</constant>
<constant digits="1" name="ego_upper_bound" units="AFR">20.0</constant>
<constant digits="1" name="ego_lower_bound" units="AFR">9.0</constant>
<constant name="ss_opt2">"Off"</constant>
<constant name="ss_opt2_spd">"Off"</constant>
<constant digits="0" name="launch_maxvss" units="MPH">199.97886</constant>
<constant name="maf_range">"650g/s"</constant>
<constant digits="0" name="ac_delay_since_last_on" units="s">5.0</constant>
<constant digits="2" name="reluctorteeth3">0.01</constant>
<constant digits="2" name="reluctorteeth4">0.01</constant>
<constant digits="0" name="boost_gear_switch" units="gear">3.0</constant>
<constant name="staged_extended_opts_use_v3">"Use Inj A-H (if possible)"</constant>
<constant name="staged_extended_opts_simult">"Alternating (2 squirts)"</constant>
<constant name="staged_extended_opts_pw1off">"Off"</constant>
<constant digits="0" name="can_pwmout_id">5.0</constant>
<constant digits="0" name="can_pwmout_tab">7.0</constant>
<constant digits="0" name="can_pwmout_offset" units="bytes">94.0</constant>
<constant digits="3" name="n2o_timing_delay" units="s">0.04992</constant>
<constant digits="3" name="n2o_timing_taper" units="s">0.04992</constant>
<constant digits="1" name="idleve_clt" units="°F">140.0</constant>
<constant digits="0" name="idleve_delay" units="s">2.0</constant>
<constant digits="0" name="ac_idleup_cl_lockout_mapadder" units="%">0.0</constant>
<constant digits="0" name="UNALLOCATED_SPACE_0_0" units="RAW">
         9.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_1" rows="2" units="RAW">
         1.0 
         244.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_2" rows="3" units="RAW">
         50.0 
         70.0 
         25.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_0_3" units="RAW">
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_0_4" units="RAW">
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_0_5" units="RAW">
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_0_6" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_7" rows="4" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_8" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_0_9" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_10" rows="4" units="RAW">
         0.0 
         10.0 
         0.0 
         250.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_11" rows="2" units="RAW">
         0.0 
         10.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_12" rows="20" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_0_13" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_14" rows="6" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_15" rows="188" units="RAW">
         0.0 
         0.0 
         0.0 
         2.0 
         0.0 
         4.0 
         0.0 
         6.0 
         0.0 
         8.0 
         0.0 
         11.0 
         0.0 
         12.0 
         0.0 
         16.0 
         0.0 
         18.0 
         0.0 
         20.0 
         0.0 
         22.0 
         0.0 
         18.0 
         0.0 
         24.0 
         0.0 
         26.0 
         0.0 
         28.0 
         0.0 
         38.0 
         0.0 
         40.0 
         0.0 
         48.0 
         0.0 
         50.0 
         0.0 
         54.0 
         0.0 
         58.0 
         0.0 
         62.0 
         0.0 
         66.0 
         0.0 
         70.0 
         0.0 
         94.0 
         0.0 
         142.0 
         0.0 
         252.0 
         1.0 
         44.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         1.0 
         1.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         1.0 
         1.0 
         1.0 
         1.0 
         2.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_16" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_17" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_0_18" units="RAW">
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_0_19" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_20" rows="2" units="RAW">
         0.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_0_21" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
</page>
<page number="1" size="1024">
<constant name="pwm_testio">"19.5Hz"</constant>
<constant digits="1" name="duty_testio" units="%">25.0</constant>
<constant digits="0" name="testop_0">0.0</constant>
<constant name="testop_coil">"Off"</constant>
<constant name="testop_fp">"Off"</constant>
<constant name="testop_inj">"Off"</constant>
<constant name="testop_pwm">"Standard"</constant>
<constant digits="1" name="testdwell" units="ms">3.0</constant>
<constant digits="1" name="testint" units="ms">199.936</constant>
<constant digits="0" name="testrpm" units="RPM">600.1920615</constant>
<constant digits="3" name="testpw" units="ms">0.0</constant>
<constant digits="0" name="testinjcnt">0.0</constant>
<constant digits="1" name="testinjPwmT" units="ms">1.040384</constant>
<constant digits="0" name="testinjPwmPd" units="us">66.0</constant>
<constant digits="0" name="testinjPwmP" units="%">30.0</constant>
<constant name="testsel_inj">"InjA"</constant>
<constant name="testsel_coil">"CoilA"</constant>
<constant digits="0" name="dbgtooth" units="tooth">0.0</constant>
<constant digits="0" name="iacpostest" units="steps">30.0</constant>
<constant digits="0" name="iachometest" units="steps">160.0</constant>
<constant digits="0" name="iactest_0">0.0</constant>
<constant name="flashlock">"Unlocked"</constant>
<constant name="boost_ctl_settings_on2">"Off"</constant>
<constant name="boost_ctl_settings_cl2">"Open-loop"</constant>
<constant name="boost_ctl_pins2">"High Current Out 1"</constant>
<constant digits="0" name="boost_ctl_Kp2" units="%">0.0</constant>
<constant digits="0" name="boost_ctl_Ki2" units="%">0.0</constant>
<constant digits="0" name="boost_ctl_Kd2" units="%">0.0</constant>
<constant digits="0" name="boost_ctl_closeduty2" units="%">0.0</constant>
<constant digits="0" name="boost_ctl_openduty2" units="%">0.0</constant>
<constant name="boost_ctl_pins_pwm2">"High Current Out 3"</constant>
<constant digits="1" name="boost_ctl_lowerlimit2" units="kPa">100.0</constant>
<constant name="boost_ctl_sensor2">"Sensor 1"</constant>
<constant name="vss3_an">"Analog In 3"</constant>
<constant name="vss4_an">"Analog In 1"</constant>
<constant digits="0" name="vss3_pwmseq">1.0</constant>
<constant digits="0" name="vss4_pwmseq">1.0</constant>
<constant digits="0" name="u08_debug38">0.0</constant>
<constant name="u08_debug38_1">"Off"</constant>
<constant name="u08_debug38_2">"Useful data"</constant>
<constant name="egoport1">"Analog In 2"</constant>
<constant name="egoport2">"O2 In"</constant>
<constant name="egoport3">"O2 In"</constant>
<constant name="egoport4">"O2 In"</constant>
<constant name="egoport5">"O2 In"</constant>
<constant name="egoport6">"O2 In"</constant>
<constant name="egoport7">"O2 In"</constant>
<constant name="egoport8">"O2 In"</constant>
<constant name="egoport9">"O2 In"</constant>
<constant name="egoport10">"O2 In"</constant>
<constant name="egoport11">"O2 In"</constant>
<constant name="egoport12">"O2 In"</constant>
<constant name="egoport13">"O2 In"</constant>
<constant name="egoport14">"O2 In"</constant>
<constant name="egoport15">"O2 In"</constant>
<constant name="egoport16">"O2 In"</constant>
<constant name="egomap1">"EGO1"</constant>
<constant name="egomap2">"EGO1"</constant>
<constant name="egomap3">"EGO1"</constant>
<constant name="egomap4">"EGO1"</constant>
<constant name="egomap5">"EGO1"</constant>
<constant name="egomap6">"EGO1"</constant>
<constant name="egomap7">"EGO1"</constant>
<constant name="egomap8">"EGO1"</constant>
<constant name="egomap9">"EGO1"</constant>
<constant name="egomap10">"EGO1"</constant>
<constant name="egomap11">"EGO1"</constant>
<constant name="egomap12">"EGO1"</constant>
<constant name="egomap13">"EGO1"</constant>
<constant name="egomap14">"EGO1"</constant>
<constant name="egomap15">"EGO1"</constant>
<constant name="egomap16">"EGO1"</constant>
<constant name="egomap1t">"1"</constant>
<constant name="egomap2t">"1"</constant>
<constant name="egomap3t">"1"</constant>
<constant name="egomap4t">"1"</constant>
<constant name="egomap5t">"1"</constant>
<constant name="egomap6t">"1"</constant>
<constant name="egomap7t">"1"</constant>
<constant name="egomap8t">"1"</constant>
<constant name="egomap9t">"1"</constant>
<constant name="egomap10t">"1"</constant>
<constant name="egomap11t">"1"</constant>
<constant name="egomap12t">"1"</constant>
<constant name="egomap13t">"1"</constant>
<constant name="egomap14t">"1"</constant>
<constant name="egomap15t">"1"</constant>
<constant name="egomap16t">"1"</constant>
<constant name="tc_opt_on">"Off"</constant>
<constant name="tc_opt_method">"Switch input"</constant>
<constant name="tc_opt_slipcurve">"Fixed value"</constant>
<constant name="tc_opt_n2o">"On/Off"</constant>
<constant name="tc_opt_bank">"Both"</constant>
<constant digits="0" name="tc_slipthresh" units="%">5.0</constant>
<constant digits="1" name="tc_minvss" units="MPH">2.01321</constant>
<constant digits="1" name="tc_maxvss" units="MPH">89.476</constant>
<constant digits="1" name="tc_mintps" units="%">20.0</constant>
<constant name="tc_enin">"Off"</constant>
<constant name="knock_bpass">"4.95"</constant>
<constant name="knock_conf_num">"1"</constant>
<constant name="knock_conf_debug">"Off"</constant>
<constant name="knock_conf_percylact">"Off"</constant>
<constant name="knock_conf_launch">"Off"</constant>
<constant name="knock_conf_percyl">"Off"</constant>
<constant name="knock_int">"150"</constant>
<constant digits="2" name="ff_tpw0" units="ms">1.0</constant>
<constant digits="2" name="ff_tpw1" units="ms">5.0</constant>
<constant digits="1" name="ff_temp0" units="°F">-40.0</constant>
<constant digits="1" name="ff_temp1" units="°F">257.0</constant>
<constant name="fueltemp1">"Off"</constant>
<constant name="fueltemp1_corr">"Off"</constant>
<constant name="tc_knob">"Off"</constant>
<constant digits="1" name="maf_freq0" units="Hz">37.5</constant>
<constant digits="1" name="maf_freq1" units="Hz">6250.0</constant>
<constant digits="1" name="map_freq0" units="Hz">32.0</constant>
<constant digits="1" name="map_freq1" units="Hz">75.0</constant>
<constant name="knock_gain01">"1.000"</constant>
<constant name="knock_gain02">"1.000"</constant>
<constant name="knock_gain03">"1.000"</constant>
<constant name="knock_gain04">"1.000"</constant>
<constant name="knock_gain05">"1.000"</constant>
<constant name="knock_gain06">"1.000"</constant>
<constant name="knock_gain07">"1.000"</constant>
<constant name="knock_gain08">"1.000"</constant>
<constant name="knock_gain09">"1.000"</constant>
<constant name="knock_gain10">"1.000"</constant>
<constant name="knock_gain11">"1.000"</constant>
<constant name="knock_gain12">"1.000"</constant>
<constant name="knock_gain13">"1.000"</constant>
<constant name="knock_gain14">"1.000"</constant>
<constant name="knock_gain15">"1.000"</constant>
<constant name="knock_gain16">"1.000"</constant>
<constant name="knock_sens01">"1"</constant>
<constant name="knock_sens02">"1"</constant>
<constant name="knock_sens03">"1"</constant>
<constant name="knock_sens04">"1"</constant>
<constant name="knock_sens05">"1"</constant>
<constant name="knock_sens06">"1"</constant>
<constant name="knock_sens07">"1"</constant>
<constant name="knock_sens08">"1"</constant>
<constant name="knock_sens09">"1"</constant>
<constant name="knock_sens10">"1"</constant>
<constant name="knock_sens11">"1"</constant>
<constant name="knock_sens12">"1"</constant>
<constant name="knock_sens13">"1"</constant>
<constant name="knock_sens14">"1"</constant>
<constant name="knock_sens15">"1"</constant>
<constant name="knock_sens16">"1"</constant>
<constant digits="0" name="s16_debug">0.0</constant>
<constant digits="0" name="u08_debug134">0.0</constant>
<constant name="AE_options">"Time-based AE"</constant>
<constant digits="1" name="accel_blend_percent" units="%">100.0</constant>
<constant digits="0" name="accel_tpsdot_threshold" units="%/sec">30.0</constant>
<constant digits="0" name="accel_mapdot_threshold" units="kpa/sec">100.0</constant>
<constant digits="0" name="ae_lorpm2" units="rpm">6001.0</constant>
<constant digits="0" name="ae_hirpm2" units="rpm">6001.0</constant>
<constant digits="1" name="accel_blend_percent2" units="%">100.0</constant>
<constant digits="0" name="accel_tpsdot_threshold2" units="%/sec">50.1</constant>
<constant digits="0" name="accel_mapdot_threshold2" units="kpa/sec">101.0</constant>
<constant digits="1" name="tpsThresh2" units="%/s">200.0</constant>
<constant digits="0" name="mapThresh2" units="kPa/s">100.0</constant>
<constant digits="0" name="aeEndPW2" units="%ReqFuel">0.0</constant>
<constant digits="0" name="taeColdA2" units="%ReqFuel">20.0</constant>
<constant digits="0" name="taeColdM2" units="%">130.0</constant>
<constant digits="2" name="taeTime2" units="s">0.2</constant>
<constant digits="0" name="taeTime_events2" units="events">20.0</constant>
<constant digits="0" name="tdePct2">100.0</constant>
<constant digits="2" name="aeTaperTime2" units="s">0.0</constant>
<constant digits="0" name="aeTaperTime_events2" units="events">0.0</constant>
<constant digits="0" name="tpsProportion2" units="%">100.0</constant>
<constant digits="1" name="accel_CLT_multiplier2" units="%">100.0</constant>
<constant name="tc_led_out">"Off"</constant>
<constant name="tc_opt_driven">"VSS1"</constant>
<constant name="tc_opt_undriven">"VSS2"</constant>
<constant digits="1" name="accel_CLT_multiplier" units="%">100.0</constant>
<constant cols="1" digits="0" name="cl_idle_timing_target_deltas" rows="8" units="rpm">
         -400.0 
         -100.0 
         -75.0 
         -50.0 
         0.0 
         50.0 
         100.0 
         300.0 
      </constant>
<constant cols="1" digits="0" name="cl_idle_timing_advance_deltas" rows="8" units="deg">
         2.0 
         3.0 
         2.0 
         1.0 
         0.0 
         -1.0 
         -1.0 
         -2.0 
      </constant>
<constant name="ltt_opt_on">"Off"</constant>
<constant name="ltt_opt_mode">"Timed"</constant>
<constant name="ltt_opt_feedback">"Off"</constant>
<constant name="ltt_but_in">"Digital Switched In 3"</constant>
<constant digits="0" name="ltt_int" units="min">30.0</constant>
<constant name="ltt_led_out">"Off"</constant>
<constant digits="1" name="ltt_thresh" units="%">100.0</constant>
<constant digits="1" name="tc_minmap" units="kPa">0.0</constant>
<constant name="can_bcast1_on">"Off"</constant>
<constant name="can_bcast1_280x4">"Off"</constant>
<constant name="can_bcast1_280x1">"Off"</constant>
<constant name="can_bcast1_289">"Off"</constant>
<constant name="can_bcast1_316">"Off"</constant>
<constant name="can_bcast1_329">"Off"</constant>
<constant name="can_bcast1_561">"Off"</constant>
<constant name="can_bcast1_361">"Off"</constant>
<constant name="can_bcast2_041">"Off"</constant>
<constant name="can_bcast2_he351">"Off"</constant>
<constant name="can_bcast2_23d">"Off"</constant>
<constant name="can_bcast2_xxx">"Off"</constant>
<constant digits="1" name="can_bcast_int" units="ms">249.984</constant>
<constant name="timedout1_in">"Off"</constant>
<constant name="timedout1_out">"High Current Out 2"</constant>
<constant digits="3" name="timedout1_offdelay" units="s">0.5</constant>
<constant name="tstop_out">"Off"</constant>
<constant name="can_enable_on">"On"</constant>
<constant name="can_enable_alcan">"Off"</constant>
<constant name="can_enable_baud">"500k"</constant>
<constant digits="3" name="tstop_delay" units="s">1.0</constant>
<constant digits="3" name="tstop_hold" units="s">0.5</constant>
<constant digits="1" name="oddfireangs1">60.0</constant>
<constant digits="1" name="oddfireangs2">60.0</constant>
<constant digits="1" name="oddfireangs3">60.0</constant>
<constant digits="1" name="oddfireangs4">60.0</constant>
<constant digits="1" name="oddfireangs5">60.0</constant>
<constant digits="1" name="oddfireangs6">60.0</constant>
<constant name="cel_opt_on">"On"</constant>
<constant name="cel_opt_stat">"Off"</constant>
<constant name="cel_opt_adc">"Fluctuation"</constant>
<constant name="cel_opt_flash">"Solid"</constant>
<constant name="cel_opt_when">"On"</constant>
<constant name="cel_port">"Digital Frequency In 1"</constant>
<constant digits="1" name="afr_min" units="AFR">8.5</constant>
<constant digits="1" name="afr_max" units="AFR">22.0</constant>
<constant digits="0" name="afr_var_upper">2000.0</constant>
<constant digits="0" name="afr_var_lower">10.0</constant>
<constant digits="0" name="map_minadc">0.0</constant>
<constant digits="0" name="map_maxadc">1023.0</constant>
<constant digits="0" name="map_var_upper">7000.0</constant>
<constant digits="0" name="mat_minadc">5.0</constant>
<constant digits="0" name="mat_maxadc">1018.0</constant>
<constant digits="0" name="mat_var_upper">1500.0</constant>
<constant digits="0" name="clt_minadc">5.0</constant>
<constant digits="0" name="clt_maxadc">1023.0</constant>
<constant digits="0" name="clt_var_upper">1000.0</constant>
<constant digits="0" name="tps_minadc">0.0</constant>
<constant digits="0" name="tps_maxadc">1023.0</constant>
<constant digits="0" name="tps_var_upper">7000.0</constant>
<constant digits="1" name="batt_minv">7.0</constant>
<constant digits="1" name="batt_maxv">23.0</constant>
<constant digits="0" name="batt_var_upper">15.0</constant>
<constant name="cel_opt2_map">"Off"</constant>
<constant name="cel_opt2_mat">"Off"</constant>
<constant name="cel_opt2_clt">"Off"</constant>
<constant name="cel_opt2_tps">"Off"</constant>
<constant name="cel_opt2_batt">"Off"</constant>
<constant name="cel_opt2_afr0">"Off"</constant>
<constant name="cel_opt2_sync">"Off"</constant>
<constant name="cel_opt2_egt">"Off"</constant>
<constant name="cel_action1_map">"Off"</constant>
<constant name="cel_action1_mat">"Off"</constant>
<constant name="cel_action1_clt">"Off"</constant>
<constant name="cel_action1_tps">"Off"</constant>
<constant name="cel_action1_batt">"Off"</constant>
<constant name="cel_action1_ego">"Off"</constant>
<constant name="cel_action1_sync">"Off"</constant>
<constant name="cel_action1_map_an">"Off"</constant>
<constant digits="1" name="cel_clt_cold" units="°F">-40.0</constant>
<constant digits="1" name="cel_clt_warm" units="°F">212.0</constant>
<constant digits="1" name="cel_warmtime" units="mins">5.14794</constant>
<constant digits="1" name="cel_mat_default" units="°F">100.0</constant>
<constant digits="0" name="cel_revlim" units="RPM">3000.0</constant>
<constant digits="1" name="cel_overboost" units="kPa">105.0</constant>
<constant digits="0" name="cel_boost_duty" units="%">0.0</constant>
<constant digits="0" name="cel_boost_duty2" units="%">0.0</constant>
<constant digits="0" name="cel_synctol">1.0</constant>
<constant name="cel_opt3_flex">"Off"</constant>
<constant digits="1" name="cel_retard" units="deg">0.0</constant>
<constant digits="0" name="map_var_lower">0.0</constant>
<constant digits="1" name="egt_minvalid" units="°F">-40.0</constant>
<constant digits="1" name="egt_maxvalid" units="°F">2700.0</constant>
<constant digits="0" name="egt_var_upper">10000.0</constant>
<constant digits="0" name="egt_var_lower">0.0</constant>
<constant digits="0" name="cel_runtime" units="s">20.0</constant>
<constant name="cel_action2_flex">"Off"</constant>
<constant name="cel_action2_egt">"Off"</constant>
<constant name="cel_action2_oil">"Off"</constant>
<constant name="blend_opt1">"TPS"</constant>
<constant name="blend_opt2">"TPS"</constant>
<constant name="blend_opt3">"TPS"</constant>
<constant name="blend_opt4">"TPS"</constant>
<constant name="blend_opt5">"TPS"</constant>
<constant name="blend_opt6">"TPS"</constant>
<constant name="blend_opt7">"TPS"</constant>
<constant name="fp_opt_mode">"On/Off"</constant>
<constant name="fp_opt_reg">"Vac referenced"</constant>
<constant name="fp_opt_inv">"Normal"</constant>
<constant name="fp_opt_safety">"Off"</constant>
<constant name="fp_out1">"Fuel Pump"</constant>
<constant digits="1" name="rail_pressure_psig" units="psi.g">42.917336</constant>
<constant digits="1" name="rail_pressure_kpag" units="kPa.g">295.9</constant>
<constant digits="1" name="fp_Kp" units="%">10.0</constant>
<constant digits="1" name="fp_Ki" units="%">5.0</constant>
<constant digits="1" name="fp_Kd" units="%">3.0</constant>
<constant digits="1" name="fp_prime_duty" units="%">39.2</constant>
<constant name="fp_press_in">"Off"</constant>
<constant name="fp_press_type">"Gauge"</constant>
<constant name="fp_freq">"125Hz"</constant>
<constant name="alternator_opt_mode">"High-speed feedback field control"</constant>
<constant name="alternator_freq">"250Hz"</constant>
<constant name="alternator_controlout">"PWM Out 3"</constant>
<constant name="alternator_control_inv">"Inverted"</constant>
<constant name="alternator_lampout">"Off"</constant>
<constant digits="1" name="alternator_Kp" units="%">90.0</constant>
<constant digits="1" name="alternator_Ki" units="%">150.0</constant>
<constant digits="1" name="alternator_Kd" units="%">1.0</constant>
<constant digits="1" name="alternator_startdelay" units="s">0.5</constant>
<constant digits="1" name="alternator_ramptime" units="s">1.0</constant>
<constant digits="1" name="alternator_wot" units="%">101.0</constant>
<constant digits="1" name="alternator_wotv" units="V">12.5</constant>
<constant digits="1" name="alternator_overrv" units="V">14.8</constant>
<constant digits="0" name="alternator_wottimeout" units="s">20.0</constant>
<constant name="alternator_tempin">"Off"</constant>
<constant name="alternator_freq_monin">"Off"</constant>
<constant name="alternator_freq_moninv">"Normal"</constant>
<constant digits="1" name="alternator_targv" units="V">14.5</constant>
<constant digits="0" name="alternator_ctl_ms" units="ms">9.984</constant>
<constant digits="0" name="fp_ctl_ms" units="ms">19.968</constant>
<constant name="alternator_freq_currin">"Off"</constant>
<constant name="alternator_freq_currinv">"Normal"</constant>
<constant digits="0" name="alternator_chargetime" units="min">1.0</constant>
<constant digits="1" name="alternator_targvr" units="V">14.0</constant>
<constant digits="1" name="alternator_diff" units="V">1.0</constant>
<constant digits="0" name="alternator_maxload" units="%">90.0</constant>
<constant name="hpte_opt_on">"Off"</constant>
<constant digits="1" name="hpte_load" units="%">90.0</constant>
<constant digits="0" name="hpte_rpm" units="rpm">900.0</constant>
<constant name="shiftlight_opt_pins">"Off"</constant>
<constant name="shiftlight_opt_gear">"Off"</constant>
<constant digits="1" name="fc_trans_time_ret" units="s">0.5</constant>
<constant digits="0" name="shiftlight_limit1" units="rpm">6200.0</constant>
<constant digits="0" name="shiftlight_limit2" units="rpm">6500.0</constant>
<constant digits="0" name="shiftlight_limit3" units="rpm">6500.0</constant>
<constant digits="0" name="shiftlight_limit4" units="rpm">6500.0</constant>
<constant digits="0" name="shiftlight_limit5" units="rpm">6500.0</constant>
<constant digits="0" name="shiftlight_limit6" units="rpm">6500.0</constant>
<constant digits="0" name="ltt_samp_time" units="s">30.0</constant>
<constant digits="0" name="ltt_agg">50.0</constant>
<constant name="oilpress_in">"Off"</constant>
<constant name="oilpress_in_safety">"Off"</constant>
<constant name="oilpress_out">"Off"</constant>
<constant digits="0" name="fuelcalctime" units="ms">99.968</constant>
<constant digits="0" name="alternator_sensitivity">4.0</constant>
<constant digits="0" name="idleminvss" units="MPH">0.0</constant>
<constant digits="1" name="flex_baseline" units="%">0.0</constant>
<constant digits="1" name="fc_transition_time" units="s">0.5</constant>
<constant digits="2" name="fc_ae_time" units="s">0.0</constant>
<constant digits="2" name="fc_timing" units="deg">36.0</constant>
<constant digits="0" name="fc_ae_pct" units="%ReqFuel">0.0</constant>
<constant digits="1" name="fp_off_duty" units="%">0.0</constant>
<constant digits="1" name="fp_min_duty" units="%">0.0</constant>
<constant digits="1" name="fp_max_duty" units="%">99.96</constant>
<constant name="tcs_in">"Off"</constant>
<constant digits="0" name="tcs_moves">1.0</constant>
<constant digits="3" name="tcs_offtime" units="s">0.05</constant>
<constant digits="3" name="tcs_ontime" units="s">0.1</constant>
<constant digits="1" name="boost_geartarg1" units="kPa">100.0</constant>
<constant digits="1" name="boost_geartarg2" units="kPa">100.0</constant>
<constant digits="1" name="boost_geartarg3" units="kPa">100.0</constant>
<constant digits="1" name="boost_geartarg4" units="kPa">100.0</constant>
<constant digits="1" name="boost_geartarg5" units="kPa">100.0</constant>
<constant digits="1" name="boost_geartarg6" units="kPa">100.0</constant>
<constant digits="1" name="fp_drop_psig" units="psi.g">4.3512</constant>
<constant digits="1" name="fp_drop_kpag" units="kPa.g">30.0</constant>
<constant digits="1" name="fp_drop_load" units="%">90.0</constant>
<constant digits="0" name="fp_drop_rpm" units="rpm">1500.0</constant>
<constant digits="2" name="fp_drop_time" units="s">1.0</constant>
<constant digits="0" name="pwm_opt_load_a_offset">26.0</constant>
<constant digits="0" name="pwm_opt_load_b_offset">18.0</constant>
<constant digits="0" name="pwm_opt_load_c_offset">18.0</constant>
<constant digits="0" name="pwm_opt_load_d_offset">18.0</constant>
<constant digits="0" name="pwm_opt_load_e_offset">18.0</constant>
<constant digits="0" name="pwm_opt_load_f_offset">18.0</constant>
<constant digits="0" name="pwm_opt_load_a_size">2.0</constant>
<constant digits="0" name="pwm_opt_load_b_size">2.0</constant>
<constant digits="0" name="pwm_opt_load_c_size">2.0</constant>
<constant digits="0" name="pwm_opt_load_d_size">2.0</constant>
<constant digits="0" name="pwm_opt_load_e_size">2.0</constant>
<constant digits="0" name="pwm_opt_load_f_size">2.0</constant>
<constant digits="0" name="can_gps_id">5.0</constant>
<constant digits="0" name="can_gps_table">7.0</constant>
<constant digits="0" name="can_gps_offset" units="bytes">128.0</constant>
<constant digits="1" name="spkadj_max" units="deg">2.0</constant>
<constant digits="1" name="spkadj_min" units="deg">-15.0</constant>
<constant digits="0" name="can_outpc_msg">1520.0</constant>
<constant name="can_outpc_gp00_master">"Off"</constant>
<constant name="can_outpc_gp00">"Off"</constant>
<constant name="can_outpc_gp01">"Off"</constant>
<constant name="can_outpc_gp02">"Off"</constant>
<constant name="can_outpc_gp03">"Off"</constant>
<constant name="can_outpc_gp04">"Off"</constant>
<constant name="can_outpc_gp05">"Off"</constant>
<constant name="can_outpc_gp06">"Off"</constant>
<constant name="can_outpc_gp07">"Off"</constant>
<constant name="can_outpc_gp08">"Off"</constant>
<constant name="can_outpc_gp09">"Off"</constant>
<constant name="can_outpc_gp10">"Off"</constant>
<constant name="can_outpc_gp11">"Off"</constant>
<constant name="can_outpc_gp12">"Off"</constant>
<constant name="can_outpc_gp13">"Off"</constant>
<constant name="can_outpc_gp14">"Off"</constant>
<constant name="can_outpc_gp15">"Off"</constant>
<constant name="can_outpc_gp16">"Off"</constant>
<constant name="can_outpc_gp17">"Off"</constant>
<constant name="can_outpc_gp18">"Off"</constant>
<constant name="can_outpc_gp19">"Off"</constant>
<constant name="can_outpc_gp20">"Off"</constant>
<constant name="can_outpc_gp21">"Off"</constant>
<constant name="can_outpc_gp22">"Off"</constant>
<constant name="can_outpc_gp23">"Off"</constant>
<constant name="can_outpc_gp24">"Off"</constant>
<constant name="can_outpc_gp25">"Off"</constant>
<constant name="can_outpc_gp26">"Off"</constant>
<constant name="can_outpc_gp27">"Off"</constant>
<constant name="can_outpc_gp28">"Off"</constant>
<constant name="can_outpc_gp29">"Off"</constant>
<constant name="can_outpc_gp30">"Off"</constant>
<constant name="can_outpc_gp31">"Off"</constant>
<constant name="can_outpc_gp32">"Off"</constant>
<constant name="can_outpc_gp33">"Off"</constant>
<constant name="can_outpc_gp34">"Off"</constant>
<constant name="can_outpc_gp35">"Off"</constant>
<constant name="can_outpc_gp36">"Off"</constant>
<constant name="can_outpc_gp37">"Off"</constant>
<constant name="can_outpc_gp38">"Off"</constant>
<constant name="can_outpc_gp39">"Off"</constant>
<constant name="can_outpc_gp40">"Off"</constant>
<constant name="can_outpc_gp41">"Off"</constant>
<constant name="can_outpc_gp42">"Off"</constant>
<constant name="can_outpc_gp43">"Off"</constant>
<constant name="can_outpc_gp44">"Off"</constant>
<constant name="can_outpc_gp45">"Off"</constant>
<constant name="can_outpc_gp46">"Off"</constant>
<constant name="can_outpc_gp47">"Off"</constant>
<constant name="can_outpc_gp48">"Off"</constant>
<constant name="can_outpc_gp49">"Off"</constant>
<constant name="can_outpc_gp50">"Off"</constant>
<constant name="can_outpc_gp51">"Off"</constant>
<constant name="can_outpc_gp52">"Off"</constant>
<constant name="can_outpc_gp53">"Off"</constant>
<constant name="can_outpc_gp54">"Off"</constant>
<constant name="can_outpc_gp55">"Off"</constant>
<constant name="can_outpc_gp56">"Off"</constant>
<constant name="can_outpc_gp57">"Off"</constant>
<constant name="can_outpc_gp58">"Off"</constant>
<constant name="can_outpc_gp59">"Off"</constant>
<constant name="can_outpc_gp60">"Off"</constant>
<constant name="can_outpc_gp61">"Off"</constant>
<constant name="can_outpc_gp62">"Off"</constant>
<constant name="can_outpc_gp63">"Off"</constant>
<constant name="can_rcv_opt_on">"Off"</constant>
<constant digits="0" name="engine_state_accel_slow_thresh" units="rpm/sec">800.0</constant>
<constant digits="0" name="engine_state_decel_slow_thresh" units="rpm/sec">-800.0</constant>
<constant digits="1" name="engine_state_tps_closed_thresh" units="%">1.0</constant>
<constant digits="1" name="engine_state_overrun_map_thresh" units="kPa">20.0</constant>
<constant digits="0" name="engine_state_overrun_rpm_thresh" units="rpm">1200.0</constant>
<constant name="engine_state_flags_use_vss">"Off"</constant>
<constant digits="2" name="vss_samp_int" units="ms">50.0</constant>
<constant digits="0" name="engine_state_vss_thresh" units="MPH">0.0</constant>
<constant digits="1" name="engine_state_tps_wot_thresh" units="%">95.0</constant>
<constant digits="2" name="oilpress_time" units="s">0.1</constant>
<constant name="dummyfield">""</constant>
<constant name="staged_out2">"Off"</constant>
<constant name="staged_out2_inv">"Normal"</constant>
<constant digits="1" name="staged_out2_time" units="s">0.4</constant>
<constant digits="0" name="u16_debug640">0.0</constant>
<constant name="staged_out1">"Off"</constant>
<constant name="staged_out1_inv">"Normal"</constant>
<constant name="log_style4_opt">"RPM"</constant>
<constant digits="0" name="log_trig_rpm" units="RPM">1200.0</constant>
<constant digits="0" name="log_trig_tps" units="%">5.0</constant>
<constant digits="0" name="baudhigh">115200.0</constant>
<constant digits="0" name="fuelCorr_default" units="%">163.0</constant>
<constant name="sdpulse_out">"Off"</constant>
<constant digits="1" name="fuelSpkDel_default" units="deg">0.0</constant>
<constant digits="1" name="map_phase_thresh" units="kPa">70.0</constant>
<constant digits="1" name="flex_pct0" units="%">0.0</constant>
<constant digits="1" name="flex_pct1" units="%">100.0</constant>
<constant name="sensor01_source">"Off"</constant>
<constant name="sensor02_source">"Off"</constant>
<constant name="sensor03_source">"Off"</constant>
<constant name="sensor04_source">"Off"</constant>
<constant name="sensor05_source">"Off"</constant>
<constant name="sensor06_source">"Off"</constant>
<constant name="sensor07_source">"Off"</constant>
<constant name="sensor08_source">"Off"</constant>
<constant name="sensor09_source">"Off"</constant>
<constant name="sensor10_source">"Off"</constant>
<constant name="sensor11_source">"Off"</constant>
<constant name="sensor12_source">"Off"</constant>
<constant name="sensor13_source">"Off"</constant>
<constant name="sensor14_source">"Off"</constant>
<constant name="sensor15_source">"Off"</constant>
<constant name="sensor16_source">"ECU temp"</constant>
<constant name="sensor01_trans">"Raw"</constant>
<constant name="sensor02_trans">"Raw"</constant>
<constant name="sensor03_trans">"Raw"</constant>
<constant name="sensor04_trans">"Raw"</constant>
<constant name="sensor05_trans">"Raw"</constant>
<constant name="sensor06_trans">"Raw"</constant>
<constant name="sensor07_trans">"Raw"</constant>
<constant name="sensor08_trans">"Raw"</constant>
<constant name="sensor09_trans">"Raw"</constant>
<constant name="sensor10_trans">"Raw"</constant>
<constant name="sensor11_trans">"Raw"</constant>
<constant name="sensor12_trans">"Raw"</constant>
<constant name="sensor13_trans">"Raw"</constant>
<constant name="sensor14_trans">"Raw"</constant>
<constant name="sensor15_trans">"Raw"</constant>
<constant name="sensor16_trans">"Beta calibration"</constant>
<constant digits="1" name="sensor01_val0">0.0</constant>
<constant digits="1" name="sensor02_val0">0.0</constant>
<constant digits="1" name="sensor03_val0">0.0</constant>
<constant digits="1" name="sensor04_val0">0.0</constant>
<constant digits="1" name="sensor05_val0">0.0</constant>
<constant digits="1" name="sensor06_val0">0.0</constant>
<constant digits="1" name="sensor07_val0">0.0</constant>
<constant digits="1" name="sensor08_val0">0.0</constant>
<constant digits="1" name="sensor09_val0">0.0</constant>
<constant digits="1" name="sensor10_val0">0.0</constant>
<constant digits="1" name="sensor11_val0">0.0</constant>
<constant digits="1" name="sensor12_val0">0.0</constant>
<constant digits="1" name="sensor13_val0">0.0</constant>
<constant digits="1" name="sensor14_val0">0.0</constant>
<constant digits="1" name="sensor15_val0">0.0</constant>
<constant digits="1" name="sensor16_val0">-11.0</constant>
<constant digits="1" name="sensor01_max">102.3</constant>
<constant digits="1" name="sensor02_max">102.3</constant>
<constant digits="1" name="sensor03_max">102.3</constant>
<constant digits="1" name="sensor04_max">102.3</constant>
<constant digits="1" name="sensor05_max">102.3</constant>
<constant digits="1" name="sensor06_max">102.3</constant>
<constant digits="1" name="sensor07_max">102.3</constant>
<constant digits="1" name="sensor08_max">102.3</constant>
<constant digits="1" name="sensor09_max">102.3</constant>
<constant digits="1" name="sensor10_max">102.3</constant>
<constant digits="1" name="sensor11_max">102.3</constant>
<constant digits="1" name="sensor12_max">102.3</constant>
<constant digits="1" name="sensor13_max">102.3</constant>
<constant digits="1" name="sensor14_max">102.3</constant>
<constant digits="1" name="sensor15_max">102.3</constant>
<constant digits="1" name="sensor16_max">102.3</constant>
<constant digits="0" name="sensor01LF">100.0</constant>
<constant digits="0" name="sensor02LF">100.0</constant>
<constant digits="0" name="sensor03LF">100.0</constant>
<constant digits="0" name="sensor04LF">100.0</constant>
<constant digits="0" name="sensor05LF">100.0</constant>
<constant digits="0" name="sensor06LF">100.0</constant>
<constant digits="0" name="sensor07LF">100.0</constant>
<constant digits="0" name="sensor08LF">100.0</constant>
<constant digits="0" name="sensor09LF">100.0</constant>
<constant digits="0" name="sensor10LF">100.0</constant>
<constant digits="0" name="sensor11LF">100.0</constant>
<constant digits="0" name="sensor12LF">100.0</constant>
<constant digits="0" name="sensor13LF">100.0</constant>
<constant digits="0" name="sensor14LF">100.0</constant>
<constant digits="0" name="sensor15LF">100.0</constant>
<constant digits="0" name="sensor16LF">100.0</constant>
<constant name="sensor_temp">"degF"</constant>
<constant digits="3" name="injOpen1" units="ms">1.0</constant>
<constant digits="3" name="injOpen2" units="ms">1.0</constant>
<constant digits="3" name="injOpen3" units="ms">1.0</constant>
<constant digits="3" name="injOpen4" units="ms">1.0</constant>
<constant digits="3" name="injOpen5" units="ms">1.0</constant>
<constant digits="3" name="injOpen6" units="ms">1.0</constant>
<constant digits="3" name="injOpen7" units="ms">1.0</constant>
<constant digits="3" name="injOpen8" units="ms">1.0</constant>
<constant digits="3" name="injOpena" units="ms">1.0</constant>
<constant digits="3" name="injOpenb" units="ms">1.0</constant>
<constant digits="3" name="injOpen11" units="ms">1.0</constant>
<constant digits="3" name="injOpen12" units="ms">1.0</constant>
<constant digits="3" name="injOpen13" units="ms">1.0</constant>
<constant digits="3" name="injOpen14" units="ms">1.0</constant>
<constant digits="3" name="injOpen15" units="ms">1.0</constant>
<constant digits="3" name="injOpen16" units="ms">1.0</constant>
<constant digits="3" name="injOpen17" units="ms">1.0</constant>
<constant digits="3" name="injOpen18" units="ms">1.0</constant>
<constant name="shift_cut_on">"Off"</constant>
<constant name="shift_cut_auto">"Button"</constant>
<constant name="shift_cut_gear">"Off"</constant>
<constant name="shift_cut_fuel">"Off"</constant>
<constant name="shift_cut_in">"Digital Switched In 3"</constant>
<constant name="shift_cut_out">"Stepper Out 1"</constant>
<constant digits="0" name="shift_cut_rpm" units="RPM">8000.0</constant>
<constant digits="0" name="shift_cut_tps" units="%">75.0</constant>
<constant digits="2" name="shift_cut_delay" units="s">0.1024</constant>
<constant digits="2" name="shift_cut_time" units="s">0.08192</constant>
<constant digits="2" name="shift_cut_add12" units="s">0.03072</constant>
<constant digits="2" name="shift_cut_add23" units="s">0.0</constant>
<constant digits="2" name="shift_cut_add34" units="s">0.0</constant>
<constant digits="2" name="shift_cut_add45" units="s">0.0</constant>
<constant digits="2" name="shift_cut_add56" units="s">0.0</constant>
<constant digits="2" name="shift_cut_soldelay" units="s">0.1024</constant>
<constant digits="0" name="shift_cut_rpm12" units="RPM">6000.0</constant>
<constant digits="0" name="shift_cut_rpm23" units="RPM">6000.0</constant>
<constant digits="0" name="shift_cut_rpm34" units="RPM">6000.0</constant>
<constant digits="0" name="shift_cut_rpm45" units="RPM">6000.0</constant>
<constant digits="0" name="shift_cut_rpm56" units="RPM">6000.0</constant>
<constant digits="2" name="shift_cut_reshift" units="s">0.50176</constant>
<constant name="pwm_opt_on_a">"Off"</constant>
<constant name="pwm_opt_freq_a">"250Hz"</constant>
<constant name="pwm_opt_load_a">"TPS"</constant>
<constant name="pwm_opt_on_b">"Off"</constant>
<constant name="pwm_opt_freq_b">"13Hz"</constant>
<constant name="pwm_opt_load_b">"MAP"</constant>
<constant name="pwm_opt_on_c">"Off"</constant>
<constant name="pwm_opt_freq_c">"13Hz"</constant>
<constant name="pwm_opt_load_c">"MAP"</constant>
<constant name="pwm_opt_on_d">"Off"</constant>
<constant name="pwm_opt_freq_d">"13Hz"</constant>
<constant name="pwm_opt_load_d">"MAP"</constant>
<constant name="pwm_opt_on_e">"Off"</constant>
<constant name="pwm_opt_freq_e">"13Hz"</constant>
<constant name="pwm_opt_load_e">"MAP"</constant>
<constant name="pwm_opt_on_f">"Off"</constant>
<constant name="pwm_opt_freq_f">"13Hz"</constant>
<constant name="pwm_opt_load_f">"MAP"</constant>
<constant name="pwm_opt2_a">"PWM Out 3"</constant>
<constant name="pwm_opt2_b">"Stepper Out 1"</constant>
<constant name="pwm_opt2_c">"Stepper Out 1"</constant>
<constant name="pwm_opt2_d">"Stepper Out 1"</constant>
<constant name="pwm_opt2_e">"Stepper Out 1"</constant>
<constant name="pwm_opt2_f">"Stepper Out 1"</constant>
<constant digits="0" name="pwm_onabove_a" units="%">60.0</constant>
<constant digits="0" name="pwm_onabove_b" units="%">60.0</constant>
<constant digits="0" name="pwm_onabove_c" units="%">60.0</constant>
<constant digits="0" name="pwm_onabove_d" units="%">60.0</constant>
<constant digits="0" name="pwm_onabove_e" units="%">60.0</constant>
<constant digits="0" name="pwm_onabove_f" units="%">60.0</constant>
<constant digits="0" name="pwm_offbelow_a" units="%">40.0</constant>
<constant digits="0" name="pwm_offbelow_b" units="%">40.0</constant>
<constant digits="0" name="pwm_offbelow_c" units="%">40.0</constant>
<constant digits="0" name="pwm_offbelow_d" units="%">40.0</constant>
<constant digits="0" name="pwm_offbelow_e" units="%">40.0</constant>
<constant digits="0" name="pwm_offbelow_f" units="%">40.0</constant>
<constant name="dualfuel_sw_on">"Off"</constant>
<constant name="dualfuel_sw_fuel">"Off"</constant>
<constant name="dualfuel_sw_spk">"Off"</constant>
<constant name="dualfuel_sw_afr">"Off"</constant>
<constant name="dualfuel_sw_rf">"Off"</constant>
<constant name="dualfuel_sw_stoich">"Off"</constant>
<constant name="dualfuel_sw_wue">"Off"</constant>
<constant name="dualfuel_sw_ase">"Off"</constant>
<constant name="dualfuel_sw2_prime">"Off"</constant>
<constant name="dualfuel_sw2_crank">"Off"</constant>
<constant name="dualfuel_sw2_injp">"Off"</constant>
<constant name="dualfuel_sw2_smpw">"Off"</constant>
<constant name="dualfuel_sw2_ob">"Off"</constant>
<constant name="dualfuel_sw2_boosw">"Off"</constant>
<constant name="dualfuel_sw2_ae">"Off"</constant>
<constant name="opentime2_opt1_master">"Same"</constant>
<constant name="opentime2_opt1">"Curve 1"</constant>
<constant name="opentime2_opt2">"Curve 1"</constant>
<constant name="opentime2_opt3">"Curve 1"</constant>
<constant name="opentime2_opt4">"Curve 1"</constant>
<constant name="opentime2_opt5">"Curve 1"</constant>
<constant name="opentime2_opt6">"Curve 1"</constant>
<constant name="opentime2_opt7">"Curve 1"</constant>
<constant name="opentime2_opt8">"Curve 1"</constant>
<constant name="opentime2_opta">"Curve 1"</constant>
<constant name="opentime2_opta_pwm">"Off"</constant>
<constant name="opentime2_optb">"Curve 1"</constant>
<constant name="opentime2_optb_pwm">"Off"</constant>
<constant name="opentime2_optb_own">"Off"</constant>
<constant name="opentime2_opt11">"Curve 1"</constant>
<constant name="opentime2_opt12">"Curve 1"</constant>
<constant name="opentime2_opt13">"Curve 1"</constant>
<constant name="opentime2_opt14">"Curve 1"</constant>
<constant name="opentime2_opt15">"Curve 1"</constant>
<constant name="opentime2_opt16">"Curve 1"</constant>
<constant name="smallpw2_opt1_master">"Off"</constant>
<constant name="smallpw2_opt1">"Curve 1"</constant>
<constant name="smallpw2_opt2">"Curve 1"</constant>
<constant name="smallpw2_opt3">"Curve 1"</constant>
<constant name="smallpw2_opt4">"Curve 1"</constant>
<constant name="smallpw2_opt5">"Curve 1"</constant>
<constant name="smallpw2_opt6">"Curve 1"</constant>
<constant name="smallpw2_opt7">"Curve 1"</constant>
<constant name="smallpw2_opt8">"Curve 1"</constant>
<constant name="smallpw2_opta">"Curve 1"</constant>
<constant name="smallpw2_optb">"Curve 1"</constant>
<constant name="smallpw2_opt11">"Curve 1"</constant>
<constant name="smallpw2_opt12">"Curve 1"</constant>
<constant name="smallpw2_opt13">"Curve 1"</constant>
<constant name="smallpw2_opt14">"Curve 1"</constant>
<constant name="smallpw2_opt15">"Curve 1"</constant>
<constant name="smallpw2_opt16">"Curve 1"</constant>
<constant name="dualfuel_pin">"Digital Switched In 3"</constant>
<constant name="dualfuel_opt_temp">"Off"</constant>
<constant name="dualfuel_opt_press">"Off"</constant>
<constant name="dualfuel_opt_mode">"Switching"</constant>
<constant name="dualfuel_opt_out">"Shared outputs+relay"</constant>
<constant digits="3" name="inj2Open1" units="ms">1.0</constant>
<constant digits="3" name="inj2Open2" units="ms">1.0</constant>
<constant digits="3" name="inj2Open3" units="ms">1.0</constant>
<constant digits="3" name="inj2Open4" units="ms">1.0</constant>
<constant digits="3" name="inj2Open5" units="ms">1.0</constant>
<constant digits="3" name="inj2Open6" units="ms">1.0</constant>
<constant digits="3" name="inj2Open7" units="ms">1.0</constant>
<constant digits="3" name="inj2Open8" units="ms">1.0</constant>
<constant digits="3" name="inj2Opena" units="ms">1.0</constant>
<constant digits="3" name="inj2Openb" units="ms">1.0</constant>
<constant digits="3" name="inj2Open11" units="ms">1.0</constant>
<constant digits="3" name="inj2Open12" units="ms">1.0</constant>
<constant digits="3" name="inj2Open13" units="ms">1.0</constant>
<constant digits="3" name="inj2Open14" units="ms">1.0</constant>
<constant digits="3" name="inj2Open15" units="ms">1.0</constant>
<constant digits="3" name="inj2Open16" units="ms">1.0</constant>
<constant digits="3" name="inj2Open17" units="ms">1.0</constant>
<constant digits="3" name="inj2Open18" units="ms">1.0</constant>
<constant digits="1" name="inj2PwmT" units="ms">1.040384</constant>
<constant digits="0" name="inj2PwmPd" units="us">66.0</constant>
<constant digits="0" name="inj2PwmP" units="%">75.0</constant>
<constant digits="1" name="inj2PwmT2" units="ms">1.040384</constant>
<constant digits="0" name="inj2PwmPd2" units="us">66.0</constant>
<constant digits="0" name="inj2PwmP2" units="%">75.0</constant>
<constant name="dualfuel_temp_sens">"Off"</constant>
<constant name="dualfuel_press_sens">"Off"</constant>
<constant name="dualfuel_press_type">"Gauge"</constant>
<constant name="pwm_opt_curve_a">"Table"</constant>
<constant name="pwm_opt_curve_b">"Table"</constant>
<constant name="pwm_opt_curve_c">"Table"</constant>
<constant name="pwm_opt_curve_d">"Table"</constant>
<constant name="pwm_opt_curve_e">"Table"</constant>
<constant name="pwm_opt_curve_f">"Table"</constant>
<constant digits="1" name="ITB_load_mappoint" units="% baro">90.0</constant>
<constant digits="0" name="ITB_load_idletpsthresh" units="%">1.0</constant>
<constant cols="1" digits="1" name="idle_voltage_comp_voltage" rows="6" units="V">
         9.0 
         10.5 
         12.0 
         13.5 
         15.0 
         16.0 
      </constant>
<constant cols="1" digits="1" name="idle_voltage_comp_delta" rows="6" units="%">
         5.488 
         3.92 
         2.352 
         0.0 
         -2.744 
         -4.312 
      </constant>
<constant digits="0" name="ac_idleup_max_rpm" units="rpm">5000.0</constant>
<constant name="llstg_in">"Off"</constant>
<constant name="llstg_out">"Stepper Out 1"</constant>
<constant digits="3" name="kickdelay" units="ms">1.0</constant>
<constant digits="0" name="log_trig_map" units="%">120.0</constant>
<constant digits="1" name="flexpct_default" units="%">1.0</constant>
<constant digits="0" name="UNALLOCATED_SPACE_1_0" units="RAW">
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_1_1" units="RAW">
         25.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_1_2" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_1_3" rows="37" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_1_4" units="RAW">
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_1_5" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_1_6" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_1_7" rows="2" units="RAW">
         1.0 
         144.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_1_8" rows="2" units="RAW">
         254.0 
         112.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_1_9" rows="61" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_1_10" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_1_11" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_1_12" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_1_13" rows="8" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_1_14" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_1" rows="30" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
</page>
<page number="2" size="1024">
<constant cols="8" digits="1" name="boost_ctl_load_targets" rows="8" units="kPa">
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
      </constant>
<constant cols="1" digits="1" name="boost_ctl_loadtarg_tps_bins" rows="8" units="%">
         0.0 
         20.0 
         40.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="boost_ctl_loadtarg_rpm_bins" rows="8" units="rpm">
         200.0 
         400.0 
         600.0 
         800.0 
         1000.0 
         2000.0 
         3000.0 
         4000.0 
      </constant>
<constant cols="8" digits="0" name="boost_ctl_pwm_targets" rows="8" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="1" name="boost_ctl_pwmtarg_tps_bins" rows="8" units="%">
         0.0 
         20.0 
         40.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="boost_ctl_pwmtarg_rpm_bins" rows="8" units="rpm">
         500.0 
         1000.0 
         2000.0 
         3000.0 
         4000.0 
         5000.0 
         6000.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="primePWTable" rows="10" units="ms">
         6.0 
         5.6 
         5.2 
         4.8 
         4.4 
         4.0 
         3.6 
         3.2 
         2.6 
         2.0 
      </constant>
<constant cols="1" digits="0" name="crankPctTable" rows="10" units="%">
         326.0 
         301.0 
         276.0 
         251.0 
         226.0 
         201.0 
         176.0 
         151.0 
         126.0 
         101.0 
      </constant>
<constant cols="1" digits="0" name="asePctTable" rows="10" units="%">
         45.0 
         43.0 
         41.0 
         39.0 
         37.0 
         35.0 
         33.0 
         31.0 
         30.0 
         29.0 
      </constant>
<constant cols="1" digits="0" name="aseCntTable" rows="10" units="cycles">
         350.0 
         330.0 
         310.0 
         290.0 
         270.0 
         250.0 
         230.0 
         210.0 
         180.0 
         150.0 
      </constant>
<constant cols="1" digits="1" name="matTemps" rows="6" units="°F">
         160.0 
         180.0 
         200.0 
         220.0 
         240.0 
         260.0 
      </constant>
<constant cols="1" digits="1" name="matRetard" rows="6" units="deg">
         0.0 
         0.0 
         2.0 
         4.0 
         6.0 
         8.0 
      </constant>
<constant cols="1" digits="0" name="EAEAWCRPMbins" rows="12" units="rpm">
         800.0 
         1000.0 
         1500.0 
         2000.0 
         2500.0 
         3000.0 
         3500.0 
         4000.0 
         4500.0 
         5000.0 
         5500.0 
         6000.0 
      </constant>
<constant cols="1" digits="0" name="EAESOCRPMbins" rows="12" units="rpm">
         800.0 
         1000.0 
         1500.0 
         2000.0 
         2500.0 
         3000.0 
         3500.0 
         4000.0 
         4500.0 
         5000.0 
         5500.0 
         6000.0 
      </constant>
<constant cols="1" digits="0" name="EAEAWCKPAbins" rows="12" units="kPa">
         30.0 
         35.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="EAESOCKPAbins" rows="12" units="kPa">
         30.0 
         35.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="EAEBAWC" rows="12" units="%">
         22.0 
         28.0 
         30.0 
         32.0 
         38.0 
         40.0 
         42.0 
         48.0 
         50.0 
         52.0 
         58.0 
         60.0 
      </constant>
<constant cols="1" digits="1" name="EAEBSOC" rows="12" units="%">
         2.2 
         2.8 
         3.0 
         3.2 
         3.8 
         4.0 
         4.2 
         4.8 
         5.0 
         5.2 
         5.8 
         6.0 
      </constant>
<constant cols="1" digits="0" name="EAEAWN" rows="12" units="%">
         100.0 
         95.0 
         90.0 
         85.0 
         80.0 
         75.0 
         70.0 
         65.0 
         60.0 
         55.0 
         50.0 
         45.0 
      </constant>
<constant cols="1" digits="0" name="EAESON" rows="12" units="%">
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         85.0 
         90.0 
         95.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="EAEAWW" rows="12" units="%">
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="EAESOW" rows="12" units="%">
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="baroCorrVals" rows="9" units="kPa">
         65.0 
         70.0 
         75.0 
         80.0 
         85.0 
         90.0 
         95.0 
         100.0 
         105.0 
      </constant>
<constant cols="1" digits="1" name="matCorrTemps2" rows="9" units="°F">
         -40.0 
         -4.0 
         32.0 
         59.0 
         86.0 
         113.0 
         140.0 
         194.0 
         248.0 
      </constant>
<constant cols="1" digits="1" name="temp_table_p5" rows="10" units="°F">
         10.0 
         30.0 
         50.0 
         70.0 
         90.0 
         110.0 
         130.0 
         150.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="1" name="EAEAWWCLTbins" rows="12" units="deg">
         0.0 
         20.0 
         40.0 
         60.0 
         80.0 
         100.0 
         120.0 
         130.0 
         140.0 
         160.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="1" name="EAESOWCLTbins" rows="12" units="deg">
         0.0 
         20.0 
         40.0 
         60.0 
         80.0 
         100.0 
         120.0 
         130.0 
         140.0 
         160.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="0" name="pwmidle_target_rpms" rows="8" units="rpms">
         1200.0 
         1200.0 
         1200.0 
         1200.0 
         1100.0 
         1000.0 
         900.0 
         900.0 
      </constant>
<constant cols="1" digits="1" name="pwmidle_clt_temps" rows="8" units="°F">
         70.0 
         80.0 
         90.0 
         100.0 
         110.0 
         120.0 
         130.0 
         140.0 
      </constant>
<constant cols="1" digits="1" name="RevLimLookup" rows="8" units="°F">
         32.0 
         68.0 
         100.0 
         120.0 
         140.0 
         160.0 
         180.0 
         200.0 
      </constant>
<constant cols="1" digits="0" name="RevLimRpm1" rows="8" units="RPM">
         2500.0 
         3000.0 
         4000.0 
         4500.0 
         5000.0 
         5500.0 
         6000.0 
         6000.0 
      </constant>
<constant cols="8" digits="1" name="RotarySplitTable" rows="8" units="deg">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="RotarySplitLoad" rows="8" units="kPa">
         30.0 
         40.0 
         50.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="RotarySplitRPM" rows="8" units="RPM">
         800.0 
         1200.0 
         2000.0 
         3000.0 
         4000.0 
         5000.0 
         6000.0 
         7000.0 
      </constant>
<constant cols="1" digits="0" name="NoiseFilterRpm" rows="4" units="RPM">
         500.0 
         2500.0 
         5500.0 
         7500.0 
      </constant>
<constant cols="1" digits="1" name="NoiseFilterLen" rows="4" units="usec">
         200.0 
         40.0 
         18.0 
         13.0 
      </constant>
<constant cols="1" digits="0" name="VariableLagTPSBins" rows="4" units="%/sec">
         3.0 
         10.0 
         20.0 
         50.0 
      </constant>
<constant cols="1" digits="0" name="VariableLagMapLags" rows="4" units="Lag">
         50.0 
         50.0 
         50.0 
         50.0 
      </constant>
<constant cols="1" digits="1" name="pwmidle_crank_dutyorsteps_duty" rows="4" units="%">
         59.584 
         49.784 
         45.864 
         45.08 
      </constant>
<constant cols="1" digits="0" name="pwmidle_crank_dutyorsteps_steps" rows="4" units="steps">
         152.0 
         127.0 
         117.0 
         115.0 
      </constant>
<constant cols="1" digits="1" name="pwmidle_crank_clt_temps" rows="4" units="°F">
         30.0 
         100.0 
         130.0 
         175.0 
      </constant>
<constant cols="1" digits="1" name="matclt_pct" rows="6" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="matclt_flow" rows="6" units="load*rpm">
         50000.0 
         170000.0 
         290000.0 
         410000.0 
         530000.0 
         650000.0 
      </constant>
<constant digits="0" name="user_value1">0.0</constant>
<constant digits="0" name="user_value2">0.0</constant>
<constant name="user_conf0">"Off"</constant>
<constant name="user_conf1">"Mode 0"</constant>
<constant cols="1" digits="1" name="baroCorrDelta" rows="9" units="%">
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="matCorrDelta2" rows="9" units="%">
         125.7 
         115.8 
         107.3 
         101.7 
         96.7 
         90.7 
         87.1 
         81.2 
         74.6 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_2_0" rows="20" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_2_1" rows="24" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_2_2" rows="11" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_2" rows="14" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
</page>
<page number="3" size="1024">
<constant cols="6" digits="1" name="inj_trima" rows="6" units="%">
         0.0 0.0 0.0 3.0 3.0 4.0 
         0.0 0.0 0.0 3.0 3.0 4.0 
         0.0 0.0 0.0 3.0 3.0 4.0 
         0.0 0.0 0.0 3.0 4.0 5.0 
         1.0 1.0 1.0 4.0 5.0 6.0 
         2.0 2.0 2.0 5.0 6.0 7.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimb" rows="6" units="%">
         1.0 1.0 1.0 4.0 4.0 5.0 
         1.0 1.0 1.0 4.0 4.0 5.0 
         1.0 1.0 1.0 4.0 4.0 5.0 
         1.0 1.0 1.0 4.0 5.0 6.0 
         2.0 2.0 2.0 5.0 6.0 7.0 
         3.0 3.0 3.0 6.0 7.0 8.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimc" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 3.0 3.0 3.0 0.0 
         0.0 0.0 3.0 3.0 3.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimd" rows="6" units="%">
         -3.0 -3.0 -3.0 0.0 0.0 1.0 
         -3.0 -3.0 -3.0 0.0 0.0 1.0 
         -3.0 -3.0 -3.0 0.0 0.0 1.0 
         -3.0 -3.0 -3.0 0.0 1.0 2.0 
         -2.0 -2.0 -2.0 1.0 2.0 3.0 
         -1.0 -1.0 -1.0 2.0 3.0 4.0 
      </constant>
<constant cols="6" digits="1" name="inj_trime" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimf" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimg" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimh" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimi" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimj" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimk" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_triml" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimm" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimn" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimo" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="inj_trimp" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="inj_trim_rpm" rows="6" units="rpm">
         500.0 
         1000.0 
         2000.0 
         4000.0 
         6000.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="inj_trim_load" rows="6" units="kPa">
         20.0 
         50.0 
         80.0 
         100.0 
         150.0 
         200.0 
      </constant>
<constant cols="12" digits="1" name="inj_timing" rows="12" units="deg">
         90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 
         90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 
         90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 
         90.0 90.0 90.0 90.0 90.4 90.9 91.3 91.7 92.6 93.4 93.9 94.3 
         90.0 90.0 90.0 90.0 90.6 91.3 91.9 92.6 93.9 95.1 95.8 96.4 
         90.0 90.0 90.0 90.0 90.9 91.7 92.6 93.4 95.1 96.9 97.7 98.6 
         90.0 90.0 90.0 90.0 91.3 92.6 93.9 95.1 97.7 100.3 101.6 102.9 
         90.0 90.0 90.0 90.0 91.7 93.4 95.1 96.9 100.3 103.7 105.4 107.1 
         90.0 90.0 90.0 90.0 91.9 93.9 95.8 97.7 101.6 105.4 107.4 109.3 
         90.0 90.0 90.0 90.0 92.1 94.3 96.4 98.6 102.9 107.1 109.3 111.4 
         90.0 90.0 90.0 90.0 92.6 95.1 97.7 100.3 105.4 110.6 113.1 115.7 
         90.0 90.0 90.0 90.0 93.0 96.0 99.0 102.0 108.0 114.0 117.0 120.0 
      </constant>
<constant cols="1" digits="0" name="inj_timing_rpm" rows="12" units="rpm">
         300.0 
         1000.0 
         1500.0 
         2000.0 
         2500.0 
         3000.0 
         3500.0 
         4000.0 
         5000.0 
         6000.0 
         6500.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="inj_timing_load" rows="12" units="%">
         20.0 
         25.0 
         30.0 
         40.0 
         45.0 
         50.0 
         60.0 
         70.0 
         75.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="maxafr1_load" rows="6" units="%">
         85.0 
         90.0 
         150.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="1" digits="0" name="maxafr1_rpm" rows="6" units="rpm">
         500.0 
         1000.0 
         1500.0 
         2000.0 
         2500.0 
         8000.0 
      </constant>
<constant cols="6" digits="1" name="maxafr1_diff" rows="6" units="AFR">
         1.0 1.0 1.0 1.0 1.0 1.0 
         0.7 0.7 0.7 0.7 0.7 0.7 
         0.5 0.5 0.5 0.5 0.5 0.5 
         0.3 0.3 0.3 0.3 0.3 0.3 
         0.3 0.3 0.3 0.3 0.3 0.3 
         0.3 0.3 0.3 0.3 0.3 0.3 
      </constant>
<constant cols="1" digits="1" name="dwellrpm_dwell" rows="6" units="ms">
         3.0 
         3.0 
         3.0 
         3.0 
         3.0 
         3.0 
      </constant>
<constant cols="1" digits="0" name="dwellrpm_rpm" rows="6" units="RPM">
         500.0 
         1000.0 
         2000.0 
         3000.0 
         5000.0 
         8000.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_3" rows="10" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
</page>
<page number="4" size="1024">
<constant cols="8" digits="1" name="boost_ctl_load_targets2" rows="8" units="kPa">
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
      </constant>
<constant cols="1" digits="1" name="boost_ctl_loadtarg_tps_bins2" rows="8" units="%">
         0.0 
         20.0 
         40.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="boost_ctl_loadtarg_rpm_bins2" rows="8" units="rpm">
         200.0 
         400.0 
         600.0 
         800.0 
         1000.0 
         2000.0 
         3000.0 
         4000.0 
      </constant>
<constant cols="8" digits="0" name="boost_ctl_pwm_targets2" rows="8" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="1" name="boost_ctl_pwmtarg_tps_bins2" rows="8" units="%">
         0.0 
         20.0 
         40.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="boost_ctl_pwmtarg_rpm_bins2" rows="8" units="rpm">
         500.0 
         1000.0 
         2000.0 
         3000.0 
         4000.0 
         5000.0 
         6000.0 
         7000.0 
      </constant>
<constant cols="1" digits="0" name="boost_timed_pct" rows="6" units="%">
         0.0 
         20.0 
         40.0 
         60.0 
         80.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="boost_timed_time" rows="6" units="s">
         0.0 
         1.0 
         2.0 
         3.0 
         4.0 
         5.0 
      </constant>
<constant cols="1" digits="0" name="boostvss_duty" rows="6" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="boostvss_target" rows="6" units="kPa">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="boostvss_speed" rows="6" units="MPH">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="map_sample_rpms" rows="8" units="rpm">
         800.0 
         1500.0 
         3000.0 
         4000.0 
         5000.0 
         6000.0 
         7000.0 
         8000.0 
      </constant>
<constant cols="1" digits="1" name="map_sample_timing" rows="8" units="deg">
         45.0 
         45.0 
         45.0 
         45.0 
         45.0 
         45.0 
         45.0 
         45.0 
      </constant>
<constant cols="12" digits="1" name="afrTable1" rows="12" units="AFR">
         14.5 14.5 14.5 14.5 14.7 14.7 14.7 14.7 14.7 14.2 14.1 14.0 
         14.5 14.5 14.5 14.5 14.7 14.7 14.7 14.7 14.7 13.9 13.8 13.7 
         14.5 14.5 14.5 14.5 14.6 14.6 14.6 14.2 14.2 14.0 14.0 14.0 
         14.2 14.2 14.2 14.2 14.4 14.4 14.4 14.2 14.2 14.2 14.2 14.2 
         13.4 13.4 13.4 13.4 13.4 13.4 13.4 13.4 13.4 13.4 13.4 13.4 
         12.6 12.6 12.6 12.6 12.6 12.6 12.6 12.6 12.6 12.6 12.6 12.6 
         12.5 12.5 12.5 12.5 12.5 12.5 12.5 12.5 12.5 12.5 12.5 12.5 
         12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 
         12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 12.2 
         12.0 12.0 12.0 12.0 12.0 12.0 12.0 12.0 12.0 12.0 12.0 12.0 
         11.8 11.8 11.8 11.8 11.8 11.8 11.8 11.8 11.8 11.8 11.8 11.8 
         11.6 11.6 11.6 11.6 11.6 11.6 11.6 11.6 11.6 11.6 11.6 11.6 
      </constant>
<constant cols="12" digits="1" name="afrTable2" rows="12" units="AFR">
         13.0 13.5 16.0 16.0 16.0 14.9 14.3 13.2 13.1 13.2 13.1 13.0 
         13.4 13.9 15.5 15.5 15.4 14.9 14.1 13.0 12.9 12.8 12.7 12.7 
         13.5 14.0 14.7 14.6 14.5 14.3 13.6 13.0 12.9 12.8 12.7 12.6 
         13.6 14.1 14.3 14.2 14.1 13.9 13.4 12.9 12.8 12.7 12.6 12.6 
         13.4 13.4 13.9 13.7 13.6 13.6 13.1 12.7 12.6 12.6 12.6 12.6 
         13.0 13.0 13.1 13.0 13.0 12.9 13.0 12.5 12.5 12.5 12.5 12.5 
         13.0 12.9 12.9 12.8 12.8 12.7 12.6 12.5 12.5 12.5 12.5 12.4 
         13.0 12.9 12.9 12.8 12.8 12.7 12.6 12.5 12.5 12.5 12.3 12.3 
         12.9 12.8 12.8 12.7 12.7 12.6 12.5 12.5 12.5 12.2 12.2 12.2 
         12.3 12.3 12.3 12.2 12.2 12.1 12.1 12.0 12.0 11.8 11.8 11.8 
         11.7 11.6 11.6 11.6 11.6 11.6 11.5 11.5 11.5 11.4 11.4 11.4 
         11.0 11.0 11.0 11.0 11.0 11.0 11.0 11.0 11.0 11.0 11.0 11.0 
      </constant>
<constant cols="1" digits="0" name="wueBins" rows="10" units="%">
         170.0 
         165.0 
         160.0 
         151.0 
         139.0 
         114.0 
         108.0 
         104.0 
         102.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="iacstepTable" rows="10" units="steps">
         160.0 
         150.0 
         140.0 
         130.0 
         120.0 
         105.0 
         90.0 
         75.0 
         60.0 
         40.0 
      </constant>
<constant cols="1" digits="0" name="arpm_table1" rows="12" units="RPM">
         500.0 
         800.0 
         1100.0 
         1400.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
      </constant>
<constant cols="1" digits="0" name="arpm_table2" rows="12" units="RPM">
         500.0 
         800.0 
         1100.0 
         1400.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
      </constant>
<constant cols="1" digits="1" name="amap_table1" rows="12" units="kPa">
         30.0 
         45.0 
         60.0 
         75.0 
         87.0 
         100.0 
         120.0 
         145.0 
         160.0 
         175.0 
         187.0 
         200.0 
      </constant>
<constant cols="1" digits="1" name="amap_table2" rows="12" units="kPa">
         30.0 
         40.0 
         50.0 
         55.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="1" digits="1" name="tempTable" rows="10" units="°F">
         -40.0 
         -20.0 
         0.0 
         18.0 
         35.2 
         60.0 
         100.5 
         136.0 
         158.0 
         171.6 
      </constant>
<constant cols="1" digits="1" name="dwellvolts" rows="6" units="V">
         6.0 
         8.0 
         10.0 
         12.0 
         14.0 
         16.0 
      </constant>
<constant cols="1" digits="0" name="dwellcorr" rows="6" units="%">
         500.0 
         248.0 
         168.0 
         128.0 
         102.0 
         88.0 
      </constant>
<constant cols="1" digits="1" name="cold_adv_table" rows="10" units="deg">
         6.0 
         5.0 
         4.0 
         3.0 
         2.0 
         1.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="ipwmTable" rows="10" units="%">
         50.176 
         50.176 
         50.176 
         47.432 
         43.512 
         38.416 
         35.28 
         31.752 
         30.184 
         29.792 
      </constant>
<constant cols="1" digits="1" name="opentimepct0" rows="6" units="%">
         96.0 
         98.0 
         100.0 
         100.0 
         100.0 
         106.0 
      </constant>
<constant cols="1" digits="1" name="opentimepct1" rows="6" units="%">
         220.0 
         172.0 
         124.0 
         76.0 
         28.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="opentimepct2" rows="6" units="%">
         220.0 
         172.0 
         124.0 
         76.0 
         28.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="opentimepct3" rows="6" units="%">
         220.0 
         172.0 
         124.0 
         76.0 
         28.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="opentimev" rows="6" units="V">
         7.2 
         9.6 
         12.0 
         14.4 
         16.8 
         19.2 
      </constant>
<constant cols="1" digits="3" name="smallpw0" rows="6" units="ms">
         0.0 
         0.4 
         0.8 
         1.2 
         1.6 
         2.0 
      </constant>
<constant cols="1" digits="3" name="smallpw1" rows="6" units="ms">
         0.0 
         0.4 
         0.8 
         1.2 
         1.6 
         2.0 
      </constant>
<constant cols="1" digits="3" name="smallpw2" rows="6" units="ms">
         0.0 
         0.4 
         0.8 
         1.2 
         1.6 
         2.0 
      </constant>
<constant cols="1" digits="3" name="smallpw3" rows="6" units="ms">
         0.0 
         0.4 
         0.8 
         1.2 
         1.6 
         2.0 
      </constant>
<constant cols="1" digits="3" name="smallpwpw" rows="6" units="ms">
         0.0 
         0.4 
         0.8 
         1.2 
         1.6 
         2.0 
      </constant>
<constant cols="1" digits="0" name="waterinj_rpm" rows="8" units="RPM">
         1000.0 
         2000.0 
         2500.0 
         3000.0 
         3500.0 
         4000.0 
         5000.0 
         6000.0 
      </constant>
<constant cols="1" digits="0" name="waterinj_map" rows="4" units="kPa">
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="8" digits="0" name="waterinj_duty" rows="4" units="%">
         16.0 32.0 40.0 48.0 56.0 64.0 80.0 100.0 
         16.0 32.0 40.0 48.0 56.0 64.0 80.0 100.0 
         16.0 32.0 40.0 48.0 56.0 64.0 80.0 100.0 
         16.0 32.0 40.0 48.0 56.0 64.0 80.0 100.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_4_0" rows="8" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_4_1" rows="16" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_4" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
</page>
<page number="5" size="1024">
<constant cols="6" digits="1" name="spk_trima" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimb" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimc" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimd" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trime" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimf" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimg" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimh" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimi" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimj" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimk" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_triml" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimm" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimn" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimo" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="6" digits="1" name="spk_trimp" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="spk_trim_rpm" rows="6" units="rpm">
         500.0 
         1000.0 
         2000.0 
         4000.0 
         6000.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="spk_trim_load" rows="6" units="kPa">
         20.0 
         50.0 
         80.0 
         100.0 
         150.0 
         200.0 
      </constant>
<constant cols="1" digits="1" name="XAcc" rows="5" units="%">
         30.0 
         30.0 
         30.0 
         30.0 
         30.0 
      </constant>
<constant cols="1" digits="0" name="TauAcc" rows="5" units="ms">
         410.0 
         400.0 
         390.0 
         370.0 
         350.0 
      </constant>
<constant cols="1" digits="1" name="XDec" rows="5" units="%">
         20.0 
         20.0 
         20.0 
         20.0 
         20.0 
      </constant>
<constant cols="1" digits="0" name="TauDec" rows="5" units="ms">
         510.0 
         500.0 
         490.0 
         470.0 
         450.0 
      </constant>
<constant cols="1" digits="0" name="XTrpms" rows="5" units="rpm">
         600.0 
         1000.0 
         2000.0 
         3000.0 
         6000.0 
      </constant>
<constant cols="1" digits="0" name="XClt" rows="10" units="%">
         160.0 
         150.0 
         140.0 
         130.0 
         125.0 
         120.0 
         115.0 
         110.0 
         105.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="TauClt" rows="10" units="%">
         200.0 
         190.0 
         180.0 
         180.0 
         170.0 
         160.0 
         140.0 
         125.0 
         110.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="XClt_temps" rows="10" units="°F">
         -40.0 
         -20.0 
         0.0 
         20.0 
         40.0 
         60.0 
         80.0 
         120.0 
         140.0 
         160.0 
      </constant>
<constant cols="1" digits="1" name="TauClt_temps" rows="10" units="°F">
         -40.0 
         -20.0 
         0.0 
         20.0 
         40.0 
         60.0 
         80.0 
         120.0 
         140.0 
         160.0 
      </constant>
<constant cols="1" digits="2" name="launch_time" rows="10" units="s">
         0.0 
         0.556 
         1.111 
         1.667 
         2.222 
         2.778 
         3.333 
         3.889 
         4.444 
         5.0 
      </constant>
<constant cols="1" digits="1" name="launch_retard" rows="10" units="deg">
         10.0 
         7.2 
         4.7 
         3.3 
         1.9 
         0.6 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="8" digits="0" name="staged_percents" rows="8" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 5.0 5.0 10.0 20.0 30.0 
         0.0 0.0 0.0 5.0 10.0 20.0 30.0 40.0 
         0.0 0.0 0.0 10.0 20.0 30.0 40.0 50.0 
         0.0 0.0 10.0 20.0 30.0 40.0 50.0 60.0 
         0.0 0.0 10.0 30.0 50.0 70.0 90.0 100.0 
         0.0 0.0 10.0 30.0 60.0 80.0 100.0 100.0 
         0.0 0.0 10.0 30.0 60.0 80.0 100.0 100.0 
      </constant>
<constant cols="1" digits="0" name="staged_rpms" rows="8" units="rpm">
         500.0 
         1000.0 
         2000.0 
         3000.0 
         4000.0 
         5000.0 
         6000.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="staged_loads" rows="8" units="%">
         30.0 
         40.0 
         50.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="cranktaper_time" rows="6" units="s">
         0.0 
         2.0 
         4.0 
         6.0 
         8.0 
         12.0 
      </constant>
<constant cols="1" digits="0" name="cranktaper_timeevents" rows="6" units="events">
         0.0 
         20.0 
         40.0 
         60.0 
         80.0 
         120.0 
      </constant>
<constant cols="1" digits="0" name="cranktaper_pct" rows="6" units="%">
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_5_0" rows="68" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_5_1" rows="60" units="RAW">
         0.0 
         100.0 
         7.0 
         208.0 
         15.0 
         160.0 
         23.0 
         112.0 
         31.0 
         64.0 
         39.0 
         16.0 
         46.0 
         224.0 
         54.0 
         176.0 
         62.0 
         128.0 
         70.0 
         80.0 
         78.0 
         32.0 
         97.0 
         168.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         0.0 
         0.0 
         3.0 
         232.0 
         7.0 
         208.0 
         11.0 
         184.0 
         15.0 
         160.0 
         19.0 
         136.0 
         0.0 
         100.0 
         0.0 
         50.0 
         0.0 
         25.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_5" rows="6" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
</page>
<page number="6" size="1024">
<constant cols="16" digits="1" name="veTable1" rows="16" units="%">
         43.1 43.3 44.8 46.0 46.2 45.4 45.8 48.0 47.0 46.0 47.0 47.0 47.0 47.0 47.0 47.0 
         43.6 43.3 45.2 46.5 48.4 48.2 48.1 49.0 58.0 60.0 59.0 58.0 57.0 56.0 56.0 56.0 
         54.0 51.5 51.7 48.0 49.5 50.0 48.5 52.0 63.0 62.0 63.0 63.0 63.0 59.0 59.0 59.0 
         54.4 54.2 54.5 50.0 50.0 55.0 52.0 53.0 63.0 62.0 63.0 63.0 63.0 59.0 59.0 59.0 
         56.2 55.2 55.8 54.0 56.6 56.5 54.3 54.4 66.5 66.1 67.1 67.1 67.1 63.1 63.1 63.1 
         55.9 56.7 55.5 57.0 59.2 60.8 61.3 59.0 67.0 66.6 67.6 67.6 67.6 63.6 63.6 63.6 
         56.4 56.5 56.5 57.0 59.8 62.4 61.2 60.5 70.5 70.1 71.1 71.1 69.1 66.1 66.1 66.1 
         55.5 56.5 57.5 58.7 60.2 61.6 59.6 60.0 70.0 70.2 70.4 71.5 68.6 65.6 65.6 65.6 
         55.7 56.7 57.7 58.0 60.5 63.0 60.1 59.0 71.8 70.6 71.6 71.6 69.6 66.6 66.6 66.6 
         55.7 56.7 57.7 58.0 60.5 62.0 61.4 61.0 71.9 71.2 72.2 73.9 70.9 67.9 67.9 67.9 
         56.7 57.7 58.7 59.0 61.0 63.0 64.0 65.9 72.9 72.2 73.2 74.9 71.9 68.9 68.9 68.9 
         58.0 59.0 59.0 58.0 60.0 65.1 65.7 67.8 76.6 79.0 80.0 81.3 78.3 75.3 75.3 75.3 
         58.0 59.0 60.0 59.0 62.0 65.5 70.3 71.4 76.6 79.3 80.3 84.3 81.3 78.3 78.3 78.3 
         60.0 61.0 61.0 61.0 67.1 71.0 71.4 72.2 78.8 81.6 82.6 85.0 82.3 79.8 79.8 79.8 
         61.0 61.0 63.0 63.0 69.6 72.7 73.6 75.1 79.8 82.2 83.0 86.1 84.2 81.0 81.0 81.0 
         62.0 64.0 66.0 67.0 70.5 72.9 74.0 81.0 81.8 82.5 83.0 83.2 82.2 82.0 82.7 82.7 
      </constant>
<constant cols="16" digits="1" name="veTable2" rows="16" units="%">
         26.0 26.0 29.0 34.0 40.0 46.0 50.0 55.0 58.0 61.0 61.0 60.0 59.0 59.0 58.0 58.0 
         38.0 37.0 39.0 44.0 53.0 61.0 65.0 67.0 69.0 73.0 71.0 66.0 64.0 62.0 60.0 58.0 
         43.0 42.0 43.0 45.0 54.0 63.0 66.0 69.0 71.0 75.0 73.0 67.0 65.0 63.0 61.0 59.0 
         48.0 46.0 48.0 50.0 58.0 65.0 69.0 71.0 73.0 77.0 75.0 69.0 67.0 65.0 63.0 61.0 
         52.0 51.0 52.0 55.0 62.0 67.0 71.0 73.0 75.0 79.0 77.0 71.0 69.0 67.0 65.0 63.0 
         57.0 59.0 61.0 65.0 69.0 72.0 76.0 78.0 81.0 85.0 85.0 80.0 78.0 76.0 74.0 72.0 
         61.0 62.0 65.0 69.0 72.0 75.0 79.0 82.0 85.0 89.0 88.0 84.0 82.0 80.0 78.0 76.0 
         65.0 66.0 69.0 73.0 76.0 78.0 82.0 86.0 90.0 93.0 92.0 88.0 86.0 84.0 82.0 80.0 
         68.0 70.0 73.0 78.0 81.0 83.0 86.0 90.0 94.0 98.0 97.0 93.0 91.0 89.0 87.0 85.0 
         72.0 77.0 82.0 87.0 90.0 93.0 95.0 100.0 105.0 109.0 108.0 103.0 101.0 99.0 97.0 95.0 
         74.0 82.0 87.0 92.0 96.0 98.0 101.0 106.0 112.0 115.0 114.0 109.0 107.0 105.0 103.0 101.0 
         75.0 83.0 88.0 93.0 97.0 99.0 102.0 107.0 113.0 116.0 115.0 110.0 108.0 106.0 104.0 102.0 
         78.0 85.0 90.0 95.0 99.0 101.0 104.0 109.0 115.0 118.0 117.0 112.0 110.0 108.0 106.0 100.4 
         82.0 89.0 94.5 100.0 104.0 106.0 109.0 114.5 121.0 124.0 123.0 118.0 115.5 113.5 111.5 105.4 
         86.0 93.5 94.5 100.0 104.0 111.0 109.0 120.0 126.5 130.0 129.0 123.0 121.0 119.0 116.5 110.5 
         90.0 98.0 103.5 109.5 114.0 116.0 120.0 125.5 132.5 136.0 134.5 129.0 126.5 124.0 122.0 115.5 
      </constant>
</page>
<page number="7" size="1024">
<constant cols="16" digits="1" name="advanceTable1" rows="16" units="deg">
         24.0 19.0 19.0 28.0 36.0 36.4 36.8 37.2 37.7 38.1 38.5 38.9 39.3 39.6 39.8 40.0 
         24.0 19.0 19.0 28.8 36.0 36.3 36.6 36.9 37.2 37.5 37.7 38.0 38.3 38.5 38.6 38.8 
         24.0 23.0 24.0 30.8 36.0 36.2 36.4 36.7 36.9 37.2 37.4 37.6 37.8 38.0 38.1 38.2 
         25.0 26.0 27.0 32.0 36.0 36.2 36.3 36.5 36.7 36.8 37.0 37.2 37.3 37.5 37.5 37.6 
         26.0 26.0 28.0 34.5 36.0 36.1 36.2 36.3 36.4 36.5 36.6 36.7 36.8 36.9 36.9 37.0 
         25.1 25.3 27.2 33.5 34.8 35.1 35.3 35.4 35.5 35.6 35.7 35.7 35.8 35.9 35.9 36.0 
         24.2 24.5 26.5 32.6 33.7 34.1 34.4 34.5 34.5 34.6 34.7 34.8 34.8 34.9 34.9 35.0 
         23.3 23.8 25.7 31.6 32.5 33.1 33.5 33.5 33.6 33.7 33.7 33.8 33.8 33.9 33.9 34.0 
         22.5 23.1 24.9 30.6 31.4 32.0 32.5 32.6 32.7 32.7 32.8 32.8 32.9 32.9 32.9 32.9 
         21.6 22.4 24.1 29.6 30.2 31.0 31.6 31.7 31.7 31.8 31.8 31.8 31.9 31.9 31.9 31.9 
         21.8 22.9 24.6 29.7 29.9 31.0 31.8 32.8 33.8 34.8 35.9 35.9 35.9 35.9 35.9 35.9 
         20.0 21.2 23.0 27.0 27.9 29.1 30.0 31.0 32.0 33.0 34.0 34.0 34.0 34.0 34.0 34.0 
         16.0 18.0 21.0 24.0 25.6 27.4 29.0 30.0 31.0 32.0 33.0 33.0 33.0 33.0 33.0 33.0 
         14.5 15.0 16.8 19.5 21.2 21.7 22.1 23.6 25.0 26.5 27.9 28.4 28.8 29.1 29.3 29.5 
         5.0 7.5 8.5 10.0 11.4 11.7 11.9 13.3 14.6 15.9 17.2 17.5 17.7 18.0 18.1 18.3 
         5.0 5.0 6.5 7.0 7.5 7.7 7.8 9.0 10.1 11.3 12.4 12.6 12.7 12.9 12.9 13.0 
      </constant>
<constant cols="16" digits="1" name="advanceTable2" rows="16" units="deg">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
</page>
<page number="8" size="1024">
<constant cols="16" digits="1" name="veTable3" rows="16" units="%">
         26.0 26.0 29.0 34.0 40.0 46.0 50.0 55.0 58.0 61.0 61.0 60.0 59.0 59.0 58.0 58.0 
         38.0 37.0 39.0 44.0 53.0 61.0 65.0 67.0 69.0 73.0 71.0 66.0 64.0 62.0 60.0 58.0 
         43.0 42.0 43.0 45.0 54.0 63.0 66.0 69.0 71.0 75.0 73.0 67.0 65.0 63.0 61.0 59.0 
         48.0 46.0 48.0 50.0 58.0 65.0 69.0 71.0 73.0 77.0 75.0 69.0 67.0 65.0 63.0 61.0 
         52.0 51.0 52.0 55.0 62.0 67.0 71.0 73.0 75.0 79.0 77.0 71.0 69.0 67.0 65.0 63.0 
         57.0 59.0 61.0 65.0 69.0 72.0 76.0 78.0 81.0 85.0 85.0 80.0 78.0 76.0 74.0 72.0 
         61.0 62.0 65.0 69.0 72.0 75.0 79.0 82.0 85.0 89.0 88.0 84.0 82.0 80.0 78.0 76.0 
         65.0 66.0 69.0 73.0 76.0 78.0 82.0 86.0 90.0 93.0 92.0 88.0 86.0 84.0 82.0 80.0 
         68.0 70.0 73.0 78.0 81.0 83.0 86.0 90.0 94.0 98.0 97.0 93.0 91.0 89.0 87.0 85.0 
         72.0 77.0 82.0 87.0 90.0 93.0 95.0 100.0 105.0 109.0 108.0 103.0 101.0 99.0 97.0 95.0 
         74.0 82.0 87.0 92.0 96.0 98.0 101.0 106.0 112.0 115.0 114.0 109.0 107.0 105.0 103.0 101.0 
         75.0 83.0 88.0 93.0 97.0 99.0 102.0 107.0 113.0 116.0 115.0 110.0 108.0 106.0 104.0 102.0 
         78.0 85.0 90.0 95.0 99.0 101.0 104.0 109.0 115.0 118.0 117.0 112.0 110.0 108.0 106.0 100.4 
         82.0 89.0 94.5 100.0 104.0 106.0 109.0 114.5 121.0 124.0 123.0 118.0 115.5 113.5 111.5 105.4 
         86.0 93.5 94.5 100.0 104.0 111.0 109.0 120.0 126.5 130.0 129.0 123.0 121.0 119.0 116.5 110.5 
         90.0 98.0 103.5 109.5 114.0 116.0 120.0 125.5 132.5 136.0 134.5 129.0 126.5 124.0 122.0 115.5 
      </constant>
<constant cols="16" digits="1" name="advanceTable3" rows="16" units="deg">
         20.0 20.0 31.0 33.5 35.0 36.0 37.0 38.0 38.0 38.0 38.0 38.0 38.0 38.0 38.0 38.0 
         19.0 20.0 30.0 33.0 35.0 34.0 37.0 38.0 38.0 38.0 38.0 38.0 38.0 38.0 38.0 38.0 
         18.5 20.0 29.5 32.5 34.0 34.0 36.0 37.0 37.0 37.0 37.0 37.0 37.0 37.0 37.0 37.0 
         18.0 20.0 29.0 32.0 33.0 34.0 35.0 36.0 36.0 36.0 36.0 36.0 36.0 36.0 36.0 36.0 
         17.0 20.0 28.0 30.0 31.0 32.0 33.0 34.0 34.0 34.0 34.0 34.0 34.0 34.0 34.0 34.0 
         16.0 18.5 27.0 28.0 29.0 30.0 31.0 32.0 32.0 32.0 32.0 32.0 32.0 32.0 32.0 32.0 
         15.0 18.0 25.0 26.0 27.0 28.0 29.0 30.0 30.0 30.0 30.0 30.0 30.0 30.0 30.0 30.0 
         14.0 17.0 23.0 24.0 25.0 26.0 27.0 28.0 28.0 28.0 28.0 28.0 28.0 28.0 28.0 28.0 
         13.5 16.5 21.3 22.7 23.7 24.7 25.7 26.7 26.8 26.9 27.0 27.1 27.2 27.3 27.3 27.4 
         13.0 15.9 19.6 21.5 22.5 23.5 24.5 25.5 25.5 26.0 26.0 26.2 26.4 26.6 26.7 26.8 
         12.0 14.8 16.2 18.6 19.6 20.6 21.6 22.7 23.2 23.6 24.0 24.5 24.9 25.2 25.4 25.6 
         11.0 13.4 15.6 19.3 20.3 21.3 22.3 23.4 23.6 23.8 24.0 24.3 24.5 24.6 24.7 24.8 
         10.0 12.0 15.0 20.0 21.0 22.0 23.0 24.0 24.0 24.0 24.0 24.0 24.0 24.0 24.0 24.0 
         8.5 10.0 10.8 13.5 14.3 15.0 15.8 16.5 16.5 16.5 16.5 16.5 16.5 16.5 16.5 16.5 
         5.0 5.0 6.5 7.0 7.5 8.0 8.5 9.0 9.0 9.0 9.0 9.0 9.0 9.0 9.0 9.0 
         5.0 5.0 6.5 7.0 7.5 8.0 8.5 9.0 9.0 9.0 9.0 9.0 9.0 9.0 9.0 9.0 
      </constant>
</page>
<page number="9" size="1024">
<constant cols="1" digits="0" name="frpm_table1" rows="16" units="RPM">
         700.0 
         900.0 
         1200.0 
         1400.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
         6500.0 
         7000.0 
         7200.0 
         7500.0 
      </constant>
<constant cols="1" digits="0" name="frpm_table2" rows="16" units="RPM">
         500.0 
         800.0 
         1100.0 
         1400.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
         6500.0 
         7000.0 
         7200.0 
         7500.0 
      </constant>
<constant cols="1" digits="0" name="frpm_table3" rows="16" units="RPM">
         500.0 
         800.0 
         1100.0 
         1400.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
         6500.0 
         7000.0 
         7200.0 
         7500.0 
      </constant>
<constant cols="1" digits="1" name="fmap_table1" rows="16" units="kPa">
         25.0 
         30.0 
         35.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         85.0 
         90.0 
         95.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="fmap_table2" rows="16" units="%">
         30.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         90.0 
         95.0 
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="1" digits="1" name="fmap_table3" rows="16" units="kPa">
         30.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         90.0 
         95.0 
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="1" digits="0" name="srpm_table1" rows="16" units="RPM">
         700.0 
         950.0 
         1200.0 
         1500.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
         6500.0 
         7000.0 
         7200.0 
         7500.0 
      </constant>
<constant cols="1" digits="0" name="srpm_table2" rows="16" units="RPM">
         700.0 
         900.0 
         1200.0 
         1500.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
         6500.0 
         7000.0 
         7200.0 
         7500.0 
      </constant>
<constant cols="1" digits="0" name="srpm_table3" rows="16" units="RPM">
         700.0 
         900.0 
         1200.0 
         1500.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
         6500.0 
         7000.0 
         7200.0 
         7500.0 
      </constant>
<constant cols="1" digits="1" name="smap_table1" rows="16" units="kPa">
         30.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         90.0 
         95.0 
         100.0 
         150.0 
         200.0 
         250.0 
      </constant>
<constant cols="1" digits="1" name="smap_table2" rows="16" units="%">
         30.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         90.0 
         95.0 
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="1" digits="1" name="smap_table3" rows="16" units="kPa">
         30.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         90.0 
         95.0 
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="1" digits="0" name="EAEAWCRPMbins2" rows="12" units="rpm">
         800.0 
         1000.0 
         1500.0 
         2000.0 
         2500.0 
         3000.0 
         3500.0 
         4000.0 
         4500.0 
         5000.0 
         5500.0 
         6000.0 
      </constant>
<constant cols="1" digits="0" name="EAESOCRPMbins2" rows="12" units="rpm">
         800.0 
         1000.0 
         1500.0 
         2000.0 
         2500.0 
         3000.0 
         3500.0 
         4000.0 
         4500.0 
         5000.0 
         5500.0 
         6000.0 
      </constant>
<constant cols="1" digits="1" name="EAEAWCKPAbins2" rows="12" units="kPa">
         30.0 
         35.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="EAESOCKPAbins2" rows="12" units="kPa">
         30.0 
         35.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="EAEBAWC2" rows="12" units="%">
         22.0 
         28.0 
         30.0 
         32.0 
         38.0 
         40.0 
         42.0 
         48.0 
         50.0 
         52.0 
         58.0 
         60.0 
      </constant>
<constant cols="1" digits="1" name="EAEBSOC2" rows="12" units="%">
         2.2 
         2.8 
         3.0 
         3.2 
         3.8 
         4.0 
         4.2 
         4.8 
         5.0 
         5.2 
         5.8 
         6.0 
      </constant>
<constant cols="1" digits="0" name="EAEAWN2" rows="12" units="%">
         100.0 
         95.0 
         90.0 
         85.0 
         80.0 
         75.0 
         70.0 
         65.0 
         60.0 
         55.0 
         50.0 
         45.0 
      </constant>
<constant cols="1" digits="0" name="EAESON2" rows="12" units="%">
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         85.0 
         90.0 
         95.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="EAEAWW2" rows="12" units="%">
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="EAESOW2" rows="12" units="%">
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="EAEAWWCLTbins2" rows="12" units="deg">
         0.0 
         20.0 
         40.0 
         60.0 
         80.0 
         100.0 
         120.0 
         130.0 
         140.0 
         160.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="1" name="EAESOWCLTbins2" rows="12" units="deg">
         0.0 
         20.0 
         40.0 
         60.0 
         80.0 
         100.0 
         120.0 
         130.0 
         140.0 
         160.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="1" name="ITB_load_loadvals" rows="12" units="%">
         90.0 
         84.6 
         79.1 
         73.7 
         68.2 
         62.8 
         57.3 
         51.8 
         46.3 
         40.8 
         35.4 
         30.0 
      </constant>
<constant cols="1" digits="1" name="ITB_load_switchpoints" rows="12" units="%">
         5.0 
         7.7 
         10.4 
         13.1 
         15.8 
         18.5 
         21.2 
         23.9 
         26.6 
         29.3 
         32.0 
         34.7 
      </constant>
<constant cols="1" digits="0" name="ITB_load_rpms" rows="12" units="rpm">
         800.0 
         1454.0 
         2109.0 
         2763.0 
         3418.0 
         4072.0 
         4727.0 
         5381.0 
         6036.0 
         6690.0 
         7345.0 
         8000.0 
      </constant>
<constant cols="4" digits="1" name="idleve_table1" rows="4" units="%">
         49.8 49.8 41.5 41.8 
         55.1 55.0 55.6 56.0 
         55.4 55.5 55.7 56.3 
         55.7 55.8 55.9 56.3 
      </constant>
<constant cols="4" digits="1" name="idleve_table2" rows="4" units="%">
         30.0 32.0 34.0 36.0 
         32.0 34.0 36.0 38.0 
         34.0 36.0 38.0 40.0 
         36.0 38.0 40.0 42.0 
      </constant>
<constant cols="1" digits="1" name="idleve_loads1" rows="4" units="%">
         30.0 
         35.0 
         40.0 
         45.0 
      </constant>
<constant cols="1" digits="1" name="idleve_loads2" rows="4" units="%">
         30.0 
         35.0 
         40.0 
         45.0 
      </constant>
<constant cols="1" digits="0" name="idleve_rpms1" rows="4" units="rpm">
         800.0 
         900.0 
         1000.0 
         1100.0 
      </constant>
<constant cols="1" digits="0" name="idleve_rpms2" rows="4" units="rpm">
         800.0 
         900.0 
         1000.0 
         1100.0 
      </constant>
<constant cols="1" digits="1" name="tc_perfect_vss" rows="10" units="MPH">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="tc_perfect_time" rows="10" units="s">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="tc_react_x" rows="4" units="slip% x 0.01s">
         25.0 
         50.0 
         75.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="tc_retard" rows="4" units="deg">
         3.0 
         6.0 
         12.0 
         20.0 
      </constant>
<constant cols="1" digits="0" name="tc_spkcut" rows="4" units="cut%">
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="tc_addfuel" rows="4" units="add%">
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="tc_nitrous" rows="4" units="cut%">
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="tc_boost" rows="4" units="cut%">
         25.0 
         50.0 
         75.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="knock_rpms" rows="10" units="rpm">
         500.0 
         1000.0 
         1500.0 
         2000.0 
         2500.0 
         3000.0 
         4000.0 
         5000.0 
         6000.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="knock_thresholds" rows="10" units="%">
         50.0 
         50.0 
         50.0 
         50.0 
         50.0 
         50.0 
         50.0 
         50.0 
         50.0 
         50.0 
      </constant>
<constant cols="1" digits="1" name="knock_starts" rows="10" units="deg">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="knock_durations" rows="10" units="deg">
         20.0 
         20.0 
         20.0 
         20.0 
         20.0 
         20.0 
         20.0 
         20.0 
         20.0 
         20.0 
      </constant>
<constant cols="1" digits="0" name="pwmidle_cl_initialvalue_rpms" rows="5" units="rpm">
         800.0 
         1000.0 
         1200.0 
         1400.0 
         1600.0 
      </constant>
<constant cols="1" digits="0" name="pwmidle_cl_initialvalue_matorclt" rows="5" units="°F">
         20.0 
         50.0 
         80.0 
         110.0 
         140.0 
      </constant>
<constant cols="5" digits="1" name="pwmidle_cl_initialvalues_duties" rows="5" units="%">
         0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="5" digits="0" name="pwmidle_cl_initialvalues_steps" rows="5" units="steps">
         0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="1" name="knock_clts" rows="4" units="°F">
         40.0 
         80.0 
         120.0 
         160.0 
      </constant>
<constant cols="1" digits="1" name="knock_upscale" rows="4" units="%">
         250.0 
         200.0 
         150.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="tc_perfect_rpm" rows="10" units="rpm">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="tc_boost_duty_delta" rows="4" units="+/-duty">
         -5.0 
         -10.0 
         -15.0 
         -20.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_9_0" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_9" rows="18" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
</page>
<page number="10" size="1024">
<constant cols="1" digits="0" name="pwm_rpms_a" rows="6" units="rpm">
         0.0 
         400.0 
         1200.0 
         1700.0 
         5000.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="pwm_loadvals_a" rows="6" units="%">
         9.0 
         11.0 
         12.5 
         14.0 
         17.0 
         19.0 
      </constant>
<constant cols="1" digits="1" name="pwm_xaxis_a" rows="12">
         0.0 
         40.0 
         120.0 
         170.0 
         500.0 
         700.0 
         9.0 
         11.0 
         12.5 
         14.0 
         17.0 
         19.0 
      </constant>
<constant cols="1" digits="0" name="pwm_rpms_b" rows="6" units="rpm">
         5000.0 
         10000.0 
         20000.0 
         32767.0 
         32767.0 
         32767.0 
      </constant>
<constant cols="1" digits="1" name="pwm_loadvals_b" rows="6" units="%">
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="pwm_xaxis_b" rows="12">
         500.0 
         1000.0 
         2000.0 
         3276.7 
         3276.7 
         3276.7 
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="pwm_rpms_c" rows="6" units="rpm">
         5000.0 
         10000.0 
         20000.0 
         32767.0 
         32767.0 
         32767.0 
      </constant>
<constant cols="1" digits="1" name="pwm_loadvals_c" rows="6" units="%">
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="pwm_xaxis_c" rows="12">
         500.0 
         1000.0 
         2000.0 
         3276.7 
         3276.7 
         3276.7 
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="pwm_rpms_d" rows="6" units="rpm">
         5000.0 
         10000.0 
         20000.0 
         32767.0 
         32767.0 
         32767.0 
      </constant>
<constant cols="1" digits="1" name="pwm_loadvals_d" rows="6" units="%">
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="pwm_xaxis_d" rows="12">
         500.0 
         1000.0 
         2000.0 
         3276.7 
         3276.7 
         3276.7 
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="pwm_rpms_e" rows="6" units="rpm">
         5000.0 
         10000.0 
         20000.0 
         32767.0 
         32767.0 
         32767.0 
      </constant>
<constant cols="1" digits="1" name="pwm_loadvals_e" rows="6" units="%">
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="pwm_xaxis_e" rows="12">
         500.0 
         1000.0 
         2000.0 
         3276.7 
         3276.7 
         3276.7 
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="pwm_rpms_f" rows="6" units="rpm">
         5000.0 
         10000.0 
         20000.0 
         32767.0 
         32767.0 
         32767.0 
      </constant>
<constant cols="1" digits="1" name="pwm_loadvals_f" rows="6" units="%">
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="pwm_xaxis_f" rows="12">
         500.0 
         1000.0 
         2000.0 
         3276.7 
         3276.7 
         3276.7 
         20.0 
         40.0 
         60.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="6" digits="0" name="pwm_duties_a" rows="6" units="%">
         100.0 75.0 50.0 50.0 50.0 50.0 
         100.0 50.0 50.0 56.0 56.0 56.0 
         100.0 50.0 50.0 55.0 55.0 59.0 
         100.0 54.0 54.0 65.0 71.0 75.0 
         100.0 70.0 70.0 75.0 86.0 90.0 
         100.0 90.0 90.0 90.0 90.0 90.0 
      </constant>
<constant cols="1" digits="0" name="pwm_yaxis_a" rows="12" units="%">
         100.0 
         75.0 
         50.0 
         50.0 
         50.0 
         50.0 
         100.0 
         50.0 
         50.0 
         56.0 
         56.0 
         56.0 
      </constant>
<constant cols="6" digits="0" name="pwm_duties_b" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="pwm_yaxis_b" rows="12" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="6" digits="0" name="pwm_duties_c" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="pwm_yaxis_c" rows="12" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="6" digits="0" name="pwm_duties_d" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="pwm_yaxis_d" rows="12" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="6" digits="0" name="pwm_duties_e" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="pwm_yaxis_e" rows="12" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="6" digits="0" name="pwm_duties_f" rows="6" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="pwm_yaxis_f" rows="12" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="primePWTable2" rows="10" units="ms">
         6.0 
         5.6 
         5.2 
         4.8 
         4.4 
         4.0 
         3.6 
         3.2 
         2.6 
         2.0 
      </constant>
<constant cols="1" digits="0" name="crankPctTable2" rows="10" units="%">
         326.0 
         301.0 
         276.0 
         251.0 
         226.0 
         201.0 
         176.0 
         151.0 
         126.0 
         101.0 
      </constant>
<constant cols="1" digits="0" name="asePctTable2" rows="10" units="%">
         45.0 
         43.0 
         41.0 
         39.0 
         37.0 
         35.0 
         33.0 
         31.0 
         28.0 
         25.0 
      </constant>
<constant cols="1" digits="0" name="aseCntTable2" rows="10" units="cycles">
         350.0 
         330.0 
         310.0 
         290.0 
         270.0 
         250.0 
         230.0 
         210.0 
         180.0 
         150.0 
      </constant>
<constant cols="1" digits="0" name="wueBins2" rows="10" units="%">
         180.0 
         180.0 
         160.0 
         150.0 
         135.0 
         125.0 
         113.0 
         108.0 
         102.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="temp_table_p21" rows="10" units="°F">
         10.0 
         30.0 
         50.0 
         70.0 
         90.0 
         110.0 
         130.0 
         150.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="0" name="frpm_table4" rows="16" units="RPM">
         500.0 
         800.0 
         1100.0 
         1400.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
         6500.0 
         7000.0 
         7200.0 
         7500.0 
      </constant>
<constant cols="1" digits="1" name="fmap_table4" rows="16" units="%">
         30.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         90.0 
         95.0 
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="1" digits="0" name="srpm_table4" rows="16" units="RPM">
         700.0 
         900.0 
         1200.0 
         1500.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
         6500.0 
         7000.0 
         7200.0 
         7500.0 
      </constant>
<constant cols="1" digits="1" name="smap_table4" rows="16" units="%">
         30.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         90.0 
         95.0 
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="1" digits="1" name="dualfuel_temp" rows="10" units="°F">
         10.0 
         30.0 
         50.0 
         70.0 
         90.0 
         110.0 
         130.0 
         150.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="1" name="dualfuel_temp_adj" rows="10" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="dualfuel_press" rows="10" units="kPa">
         220.0 
         240.0 
         260.0 
         280.0 
         300.0 
         320.0 
         340.0 
         360.0 
         380.0 
         400.0 
      </constant>
<constant cols="1" digits="1" name="dualfuel_press_adj" rows="10" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="12" digits="1" name="inj_timing_sec" rows="12" units="deg">
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
         360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 360.0 
      </constant>
<constant cols="1" digits="1" name="inj_timing_sec_load" rows="12" units="%">
         20.0 
         25.0 
         30.0 
         40.0 
         45.0 
         50.0 
         60.0 
         70.0 
         75.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="inj_timing_sec_rpm" rows="12" units="rpm">
         300.0 
         1000.0 
         1500.0 
         2000.0 
         2500.0 
         3000.0 
         3500.0 
         4000.0 
         5000.0 
         6000.0 
         6500.0 
         7000.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_10" rows="10" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
</page>
<page number="11" size="1024">
<constant cols="16" digits="1" name="veTable4" rows="16" units="%">
         26.0 26.0 29.0 34.0 40.0 46.0 50.0 55.0 58.0 61.0 61.0 60.0 59.0 59.0 58.0 58.0 
         38.0 37.0 39.0 44.0 53.0 61.0 65.0 67.0 69.0 73.0 71.0 66.0 64.0 62.0 60.0 58.0 
         43.0 42.0 43.0 45.0 54.0 63.0 66.0 69.0 71.0 75.0 73.0 67.0 65.0 63.0 61.0 59.0 
         48.0 46.0 48.0 50.0 58.0 65.0 69.0 71.0 73.0 77.0 75.0 69.0 67.0 65.0 63.0 61.0 
         52.0 51.0 52.0 55.0 62.0 67.0 71.0 73.0 75.0 79.0 77.0 71.0 69.0 67.0 65.0 63.0 
         57.0 59.0 61.0 65.0 69.0 72.0 76.0 78.0 81.0 85.0 85.0 80.0 78.0 76.0 74.0 72.0 
         61.0 62.0 65.0 69.0 72.0 75.0 79.0 82.0 85.0 89.0 88.0 84.0 82.0 80.0 78.0 76.0 
         65.0 66.0 69.0 73.0 76.0 78.0 82.0 86.0 90.0 93.0 92.0 88.0 86.0 84.0 82.0 80.0 
         68.0 70.0 73.0 78.0 81.0 83.0 86.0 90.0 94.0 98.0 97.0 93.0 91.0 89.0 87.0 85.0 
         72.0 77.0 82.0 87.0 90.0 93.0 95.0 100.0 105.0 109.0 108.0 103.0 101.0 99.0 97.0 95.0 
         74.0 82.0 87.0 92.0 96.0 98.0 101.0 106.0 112.0 115.0 114.0 109.0 107.0 105.0 103.0 101.0 
         75.0 83.0 88.0 93.0 97.0 99.0 102.0 107.0 113.0 116.0 115.0 110.0 108.0 106.0 104.0 102.0 
         78.0 85.0 90.0 95.0 99.0 101.0 104.0 109.0 115.0 118.0 117.0 112.0 110.0 108.0 106.0 100.4 
         82.0 89.0 94.5 100.0 104.0 106.0 109.0 114.5 121.0 124.0 123.0 118.0 115.5 113.5 111.5 105.4 
         86.0 93.5 94.5 100.0 104.0 111.0 109.0 120.0 126.5 130.0 129.0 123.0 121.0 119.0 116.5 110.5 
         90.0 98.0 103.5 109.5 114.0 116.0 120.0 125.5 132.5 136.0 134.5 129.0 126.5 124.0 122.0 115.5 
      </constant>
<constant cols="16" digits="1" name="advanceTable4" rows="16" units="deg">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
</page>
<page number="12" size="1024">
<constant cols="1" digits="0" name="psEnabled" rows="51">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         1.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="51" digits="0" name="psCondition" rows="2">
         62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 60.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 60.0 60.0 60.0 
         62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 60.0 60.0 60.0 
      </constant>
<constant cols="1" digits="0" name="psConnector" rows="51">
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         38.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
      </constant>
<constant cols="1" digits="0" name="psInitValue" rows="51">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         1.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="psPortValue" rows="51">
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="51" digits="0" name="psOutSize" rows="2">
         130.0 2.0 2.0 130.0 2.0 2.0 2.0 130.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 0.0 0.0 0.0 
         130.0 0.0 0.0 130.0 0.0 0.0 130.0 130.0 130.0 0.0 130.0 0.0 130.0 2.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="51" digits="0" name="psOutOffset" rows="2">
         6.0 6.0 6.0 6.0 6.0 6.0 22.0 6.0 22.0 6.0 26.0 6.0 22.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 6.0 0.0 6.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="51" digits="0" name="psThreshold" rows="2">
         0.0 0.0 0.0 0.0 0.0 0.0 1950.0 0.0 195.0 0.0 143.0 0.0 1500.0 100.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 800.0 0.0 70.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="51" digits="0" name="psHysteresis" rows="2">
         0.0 0.0 0.0 0.0 0.0 0.0 50.0 0.0 10.0 0.0 0.0 0.0 10.0 1.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 400.0 0.0 20.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant name="vvt_softout1">"Stepper Out 1"</constant>
<constant name="vvt_softout2">"Stepper Out 1"</constant>
<constant name="vvt_softout3">"Stepper Out 1"</constant>
<constant name="vvt_softout4">"Stepper Out 1"</constant>
</page>
<page number="13" size="1024">
<constant cols="12" digits="3" name="narrowband_tgts" rows="12" units="V">
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
         0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 0.49776 
      </constant>
<constant cols="1" digits="0" name="narrowband_tgts_rpms" rows="12" units="rpm">
         800.0 
         1400.0 
         2000.0 
         2600.0 
         3200.0 
         3800.0 
         4400.0 
         5000.0 
         5600.0 
         6200.0 
         6800.0 
         7500.0 
      </constant>
<constant cols="1" digits="1" name="narrowband_tgts_loads" rows="12" units="%">
         20.0 
         27.2 
         34.6 
         41.9 
         49.1 
         56.3 
         63.5 
         70.7 
         78.0 
         85.2 
         92.4 
         100.0 
      </constant>
<constant name="als_opt_fc">"Off"</constant>
<constant name="als_opt_sc">"Off"</constant>
<constant name="als_opt_idle">"Off"</constant>
<constant name="als_opt_fuel">"Off"</constant>
<constant name="als_opt_pwmout">"Off"</constant>
<constant name="als_opt_ri">"Off"</constant>
<constant digits="1" name="als_maxtime" units="s">4.0</constant>
<constant digits="1" name="als_maxtps" units="%">30.0</constant>
<constant digits="1" name="als_iac_duty" units="%">58.8</constant>
<constant digits="0" name="als_iac_steps" units="steps">150.0</constant>
<constant name="als_in_pin">"Off"</constant>
<constant name="als_out_pin">"Off"</constant>
<constant digits="0" name="als_pwm_duty" units="%">75.0</constant>
<constant digits="1" name="als_pausetime" units="s">10.0</constant>
<constant digits="1" name="vvt_slew" units="deg">1.0</constant>
<constant digits="1" name="als_minclt" units="°F">122.0</constant>
<constant digits="1" name="als_maxclt" units="°F">230.0</constant>
<constant cols="1" digits="0" name="als_rpms" rows="6" units="rpm">
         1300.0 
         1600.0 
         1900.0 
         2200.0 
         2500.0 
         2800.0 
      </constant>
<constant cols="1" digits="0" name="als_tpss" rows="6" units="%">
         0.0 
         4.0 
         8.0 
         12.0 
         16.0 
         20.0 
      </constant>
<constant cols="6" digits="1" name="als_timing" rows="6" units="degrees">
         -30.0 -28.0 -26.0 -24.0 -22.0 -20.0 
         -30.0 -28.0 -26.0 -24.0 -22.0 -20.0 
         -30.0 -28.0 -26.0 -24.0 -22.0 -20.0 
         -30.0 -28.0 -26.0 -24.0 -22.0 -20.0 
         -30.0 -28.0 -26.0 -24.0 -22.0 -20.0 
         -30.0 -28.0 -26.0 -24.0 -22.0 -20.0 
      </constant>
<constant cols="6" digits="1" name="als_addfuel" rows="6" units="%">
         25.0 25.0 25.0 25.0 25.0 25.0 
         25.0 25.0 25.0 25.0 25.0 25.0 
         25.0 25.0 25.0 25.0 25.0 25.0 
         25.0 25.0 25.0 25.0 25.0 25.0 
         25.0 25.0 25.0 25.0 25.0 25.0 
         25.0 25.0 25.0 25.0 25.0 25.0 
      </constant>
<constant cols="6" digits="0" name="als_fuelcut" rows="6" units="%">
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
      </constant>
<constant cols="6" digits="0" name="als_sparkcut" rows="6" units="%">
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
         80.0 80.0 80.0 80.0 80.0 80.0 
      </constant>
<constant digits="0" name="als_minrpm" units="rpm">500.0</constant>
<constant digits="0" name="als_maxrpm" units="rpm">3000.0</constant>
<constant digits="1" name="als_maxmat" units="°F">170.0</constant>
<constant digits="1" name="vvt_onoff_ang" units="degrees">0.0</constant>
<constant name="vvt_opt1_on">"1"</constant>
<constant name="vvt_opt1_filter">"Off"</constant>
<constant name="vvt_opt1_int">"Synced to cam"</constant>
<constant name="vvt_opt1_tst">"Off"</constant>
<constant name="vvt_opt1_dir_exhaust">"Advance"</constant>
<constant digits="1" name="vvt_hold_duty" units="%">37.632</constant>
<constant name="vvt_out1">"High Current Out 1"</constant>
<constant name="vvt_out2">"Off"</constant>
<constant name="vvt_out3">"Off"</constant>
<constant name="vvt_out4">"Off"</constant>
<constant name="vvt_out1_dir">"Advance"</constant>
<constant name="vvt_out2_dir">"Advance"</constant>
<constant name="vvt_out3_dir">"Advance"</constant>
<constant name="vvt_out4_dir">"Advance"</constant>
<constant digits="0" name="vvt_ctl_ms" units="ms">40.0</constant>
<constant digits="0" name="vvt_ctl_Kp" units="%">50.0</constant>
<constant digits="0" name="vvt_ctl_Ki" units="%">10.0</constant>
<constant digits="0" name="vvt_ctl_Kd" units="%">25.0</constant>
<constant digits="1" name="vvt_test_duty" units="%">87.808</constant>
<constant digits="1" name="vvt_min_ang1" units="abs.deg.">275.0</constant>
<constant digits="1" name="vvt_min_ang2" units="abs.deg.">0.0</constant>
<constant digits="1" name="vvt_min_ang3" units="abs.deg.">0.0</constant>
<constant digits="1" name="vvt_min_ang4" units="abs.deg.">0.0</constant>
<constant digits="1" name="vvt_max_ang1" units="abs.deg.">318.0</constant>
<constant digits="1" name="vvt_max_ang2" units="abs.deg.">0.0</constant>
<constant digits="1" name="vvt_max_ang3" units="abs.deg.">0.0</constant>
<constant digits="1" name="vvt_max_ang4" units="abs.deg.">0.0</constant>
<constant name="vvt_opt2_pid">"PID"</constant>
<constant name="vvt_opt2_pid2">"Variable"</constant>
<constant name="vvt_opt2_use_hold_intake">"Off"</constant>
<constant name="vvt_opt2_use_hold_exhaust">"On"</constant>
<constant name="vvt_opt2_cam2pol">"Falling Edge"</constant>
<constant name="vvt_opt2_cam3pol">"Falling Edge"</constant>
<constant name="vvt_opt2_cam4pol">"Falling Edge"</constant>
<constant name="vvt_opt2_cam1pol">"Falling Edge"</constant>
<constant name="vvt_opt3_cam2">"Digital Frequency In 1"</constant>
<constant name="vvt_opt3_cam3">"Digital Frequency In 1"</constant>
<constant name="vvt_opt3_cam4">"Digital Frequency In 1"</constant>
<constant name="vvt_opt3_cam1">"Main cam"</constant>
<constant cols="1" digits="1" name="vvt_timing_load" rows="8" units="%">
         20.0 
         40.0 
         50.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="vvt_timing_rpm" rows="8" units="rpm">
         1000.0 
         1800.0 
         2000.0 
         3000.0 
         4000.0 
         5000.0 
         6000.0 
         7000.0 
      </constant>
<constant cols="8" digits="1" name="vvt_timing1" rows="8" units="deg">
         3.0 3.0 8.0 11.0 13.0 10.0 8.0 5.0 
         3.0 3.0 10.0 13.2 15.0 11.0 11.5 7.5 
         6.5 6.0 15.0 17.7 17.5 13.0 13.3 8.8 
         8.4 8.0 20.0 17.7 20.0 15.0 15.0 10.0 
         10.3 10.0 20.0 20.0 20.0 16.0 15.0 10.0 
         12.2 12.0 20.0 20.0 20.0 17.0 15.0 10.0 
         14.1 14.0 22.0 22.0 22.0 19.0 15.0 10.0 
         16.0 16.0 22.0 22.0 22.0 19.0 15.0 10.0 
      </constant>
<constant cols="8" digits="1" name="vvt_timing2" rows="8" units="deg">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant digits="0" name="vvt_tth1">1.0</constant>
<constant digits="0" name="vvt_tth2">1.0</constant>
<constant digits="0" name="vvt_tth3">1.0</constant>
<constant digits="0" name="vvt_tth4">1.0</constant>
<constant digits="1" name="vvt_coldpos1" units="degrees">0.0</constant>
<constant digits="1" name="vvt_coldpos2" units="degrees">0.0</constant>
<constant name="tclu_opt_vss">"Off"</constant>
<constant name="tclu_opt_gear">"Off"</constant>
<constant name="tclu_brakepin">"Off"</constant>
<constant name="tclu_enablepin">"Off"</constant>
<constant name="tclu_outpin">"Off"</constant>
<constant digits="0" name="tclu_gearmin">4.0</constant>
<constant digits="1" name="tclu_delay" units="s">4.0</constant>
<constant digits="0" name="tclu_vssmin" units="MPH">30.19815</constant>
<constant digits="1" name="tclu_tpsmin" units="%">5.0</constant>
<constant digits="1" name="tclu_tpsmax" units="%">80.0</constant>
<constant digits="1" name="tclu_mapmin" units="%">30.0</constant>
<constant digits="1" name="tclu_mapmax" units="%">90.0</constant>
<constant name="vvt_opt4_decode">"Standard"</constant>
<constant name="vvt_opt5_add1">"Cam 1"</constant>
<constant name="vvt_opt5_add2">"Actual"</constant>
<constant name="vvt_opt5_err">"Yes"</constant>
<constant name="vvt_opt5_vvt1">"Intake"</constant>
<constant name="vvt_opt5_vvt2">"Intake"</constant>
<constant name="vvt_opt5_vvt3">"Intake"</constant>
<constant name="vvt_opt5_vvt4">"Intake"</constant>
<constant digits="1" name="vvt_hold_duty_exh" units="%">19.6</constant>
<constant digits="0" name="vvt_ctl_Kp_exh" units="%">50.0</constant>
<constant digits="0" name="vvt_ctl_Ki_exh" units="%">50.0</constant>
<constant digits="0" name="vvt_ctl_Kd_exh" units="%">50.0</constant>
<constant digits="0" name="vvt_cam1tth1">0.0</constant>
<constant digits="0" name="vvt_cam1tth2">0.0</constant>
<constant digits="0" name="vvt_cam2tth1">0.0</constant>
<constant digits="0" name="vvt_cam2tth2">0.0</constant>
<constant digits="0" name="vvt_cam3tth1">0.0</constant>
<constant digits="0" name="vvt_cam3tth2">0.0</constant>
<constant digits="0" name="vvt_cam4tth1">0.0</constant>
<constant digits="0" name="vvt_cam4tth2">0.0</constant>
<constant name="vvt_opt6_freq">"383Hz"</constant>
<constant name="vvt_opt7_yaxis">"Fuelload"</constant>
<constant cols="6" digits="0" name="als_rifuelcut" rows="6" units="%">
         60.0 50.0 40.0 20.0 0.0 0.0 
         30.0 40.0 30.0 10.0 0.0 0.0 
         20.0 30.0 20.0 10.0 0.0 0.0 
         10.0 20.0 10.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="als_rirpms" rows="6" units="rpm">
         800.0 
         1000.0 
         1200.0 
         1400.0 
         1600.0 
         1800.0 
      </constant>
<constant cols="1" digits="0" name="als_ritpss" rows="6" units="%">
         0.0 
         2.0 
         4.0 
         6.0 
         8.0 
         10.0 
      </constant>
<constant name="als_pwm_opt_freq">"13Hz"</constant>
<constant name="als_pwm_opt2">"Stepper Out 1"</constant>
<constant digits="1" name="vvt_minclt" units="°F">-40.0</constant>
<constant digits="1" name="vvt_minduty1" units="%">19.992</constant>
<constant digits="1" name="vvt_maxduty1" units="%">99.96</constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_13_0" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
</page>
<page number="14" size="1024">
<constant cols="1" digits="3" name="mafv" rows="64" units="V">
         0.0 
         0.08 
         0.16 
         0.23 
         0.31 
         0.39 
         0.47 
         0.55 
         0.63 
         0.7 
         0.78 
         0.86 
         0.94 
         1.02 
         1.09 
         1.17 
         1.25 
         1.33 
         1.41 
         1.49 
         1.56 
         1.64 
         1.72 
         1.8 
         1.88 
         1.96 
         2.03 
         2.11 
         2.19 
         2.27 
         2.35 
         2.42 
         2.5 
         2.58 
         2.66 
         2.74 
         2.82 
         2.89 
         2.97 
         3.05 
         3.13 
         3.21 
         3.28 
         3.36 
         3.44 
         3.52 
         3.6 
         3.68 
         3.75 
         3.83 
         3.91 
         3.99 
         4.07 
         4.14 
         4.22 
         4.3 
         4.38 
         4.46 
         4.54 
         4.61 
         4.69 
         4.77 
         4.85 
         4.93 
      </constant>
<constant cols="1" digits="0" name="maff" rows="64" units="Hz">
         37.5 
         136.9 
         236.3 
         323.275 
         422.675 
         522.075 
         621.475 
         720.875 
         820.275 
         907.25 
         1006.65 
         1106.05 
         1205.45 
         1304.85 
         1391.825 
         1491.225 
         1590.625 
         1690.025 
         1789.425 
         1888.825 
         1975.8 
         2075.2 
         2174.6 
         2274.0 
         2373.4 
         2472.8 
         2559.775 
         2659.175 
         2758.575 
         2857.975 
         2957.375 
         3044.35 
         3143.75 
         3243.15 
         3342.55 
         3441.95 
         3541.35 
         3628.325 
         3727.725 
         3827.125 
         3926.525 
         4025.925 
         4112.9 
         4212.3 
         4311.7 
         4411.1 
         4510.5 
         4609.9 
         4696.875 
         4796.275 
         4895.675 
         4995.075 
         5094.475 
         5181.45 
         5280.85 
         5380.25 
         5479.65 
         5579.05 
         5678.45 
         5765.425 
         5864.825 
         5964.225 
         6063.625 
         6163.025 
      </constant>
<constant cols="1" digits="2" name="mafflow" rows="64" units="g/sec">
         0.0 
         0.5 
         1.0 
         1.51 
         2.02 
         2.54 
         3.07 
         3.61 
         4.17 
         4.77 
         5.49 
         6.32 
         7.21 
         8.13 
         9.09 
         10.08 
         11.02 
         11.93 
         12.92 
         14.26 
         16.16 
         18.65 
         21.01 
         22.76 
         24.22 
         26.02 
         28.16 
         30.51 
         33.1 
         35.92 
         38.95 
         42.33 
         46.3 
         50.49 
         54.27 
         58.05 
         62.15 
         66.49 
         70.99 
         75.65 
         80.55 
         85.74 
         91.19 
         96.87 
         102.71 
         108.69 
         114.79 
         121.01 
         127.37 
         133.87 
         140.53 
         147.39 
         154.51 
         161.95 
         169.78 
         177.9 
         186.12 
         194.2 
         202.14 
         210.56 
         220.17 
         231.68 
         245.56 
         261.22 
      </constant>
<constant cols="6" digits="1" name="alphaMAPtable" rows="6" units="kPa">
         100.0 40.0 35.0 30.0 25.0 20.0 
         100.0 60.0 40.0 30.0 25.0 25.0 
         100.0 100.0 80.0 60.0 50.0 40.0 
         100.0 100.0 100.0 90.0 75.0 60.0 
         100.0 100.0 100.0 100.0 100.0 80.0 
         100.0 100.0 100.0 100.0 100.0 100.0 
      </constant>
<constant cols="1" digits="1" name="amap_tps" rows="6" units="%">
         0.0 
         20.0 
         40.0 
         60.0 
         80.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="amap_rpm" rows="6" units="RPM">
         0.0 
         1000.0 
         2000.0 
         3000.0 
         4000.0 
         6000.0 
      </constant>
<constant cols="1" digits="1" name="tpswot_tps" rows="6" units="%">
         10.0 
         20.0 
         40.0 
         60.0 
         80.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="tpswot_rpm" rows="6" units="RPM">
         0.0 
         1000.0 
         2000.0 
         3000.0 
         4000.0 
         6000.0 
      </constant>
<constant cols="1" digits="1" name="matCorrTemps" rows="6" units="°F">
         40.0 
         60.0 
         100.0 
         130.0 
         160.0 
         180.0 
      </constant>
<constant cols="1" digits="1" name="matCorrDelta" rows="6" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="8" digits="0" name="boost_ctl_cl_pwm_targs1" rows="8" units="%">
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
      </constant>
<constant cols="8" digits="0" name="boost_ctl_cl_pwm_targs2" rows="8" units="%">
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
      </constant>
<constant cols="1" digits="0" name="boost_ctl_cl_pwm_rpms1" rows="8" units="rpm">
         1500.0 
         2500.0 
         3500.0 
         4500.0 
         5000.0 
         5500.0 
         6000.0 
         6500.0 
      </constant>
<constant cols="1" digits="0" name="boost_ctl_cl_pwm_rpms2" rows="8" units="rpm">
         1500.0 
         2500.0 
         3500.0 
         4500.0 
         5000.0 
         5500.0 
         6000.0 
         6500.0 
      </constant>
<constant cols="1" digits="0" name="boost_ctl_cl_pwm_targboosts1" rows="8" units="kPa">
         100.0 
         110.0 
         130.0 
         140.0 
         150.0 
         160.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="0" name="boost_ctl_cl_pwm_targboosts2" rows="8" units="kPa">
         100.0 
         110.0 
         130.0 
         140.0 
         150.0 
         160.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="0" name="blendx1" rows="9" units="X">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendx2" rows="9" units="X">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendx3" rows="9" units="X">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendx4" rows="9" units="X">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendx5" rows="9" units="X">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendx6" rows="9" units="X">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendx7" rows="9" units="X">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="blendx8" rows="9" units="Flex%">
         10.0 
         19.4 
         28.8 
         38.2 
         47.5 
         56.9 
         66.3 
         75.7 
         85.0 
      </constant>
<constant cols="1" digits="0" name="blendy1" rows="9" units="VE2">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendy2" rows="9" units="Spk2">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendy3" rows="9" units="VE3/4">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendy4" rows="9" units="Spk3/4">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendy5" rows="9" units="AFR2">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendy6" rows="9" units="Boost2">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendy7" rows="9" units="Crank%2">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="blendy8" rows="9" units="Blend%">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant cols="6" digits="1" name="fpd_duty" rows="6" units="%">
         25.088 25.088 25.088 25.088 25.088 25.088 
         25.088 25.088 25.088 25.088 25.088 25.088 
         25.088 25.088 25.088 35.28 39.2 39.2 
         31.36 39.2 50.96 58.8 58.8 78.4 
         39.2 58.8 66.64 99.96 99.96 99.96 
         50.176 78.4 78.4 99.96 99.96 99.96 
      </constant>
<constant cols="1" digits="1" name="fpd_load" rows="6" units="%">
         10.0 
         20.0 
         40.0 
         60.0 
         80.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="fpd_rpm" rows="6" units="RPM">
         0.0 
         1000.0 
         2000.0 
         3000.0 
         4000.0 
         6000.0 
      </constant>
<constant cols="1" digits="1" name="fp_temps" rows="10" units="°F">
         10.0 
         30.0 
         50.0 
         70.0 
         90.0 
         110.0 
         130.0 
         150.0 
         170.0 
         180.0 
      </constant>
<constant cols="1" digits="1" name="fp_temp_adj" rows="10" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="fp_presss" rows="10" units="kPa">
         220.0 
         240.0 
         260.0 
         280.0 
         300.0 
         320.0 
         340.0 
         360.0 
         380.0 
         400.0 
      </constant>
<constant cols="1" digits="1" name="fp_press_adj" rows="10" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="hpte_times" rows="6" units="s">
         0.0 
         7.0 
         10.0 
         15.0 
         20.0 
         25.0 
      </constant>
<constant cols="1" digits="1" name="hpte_afrs" rows="6" units="AFR">
         0.0 
         0.0 
         0.5 
         1.0 
         1.3 
         1.8 
      </constant>
<constant cols="1" digits="0" name="oil_rpm" rows="6" units="RPM">
         0.0 
         500.0 
         1000.0 
         2000.0 
         5000.0 
         8000.0 
      </constant>
<constant cols="1" digits="1" name="oil_press_min" rows="6">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="oil_press_max" rows="6">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="alt_dutyin" rows="7" units="%">
         0.0 
         16.0 
         33.0 
         50.0 
         66.0 
         83.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="alt_dutyout" rows="7" units="%">
         0.0 
         16.0 
         33.0 
         50.0 
         66.0 
         83.0 
         100.0 
      </constant>
<constant digits="0" name="UNALLOCATED_TOP_14" units="RAW">
         0.0 
      </constant>
</page>
<page number="15" size="1024">
<constant cols="1" digits="0" name="qfrtfielddata" rows="256">
         16384.0 
         16386.0 
         16390.0 
         16392.0 
         8203.0 
         16402.0 
         16406.0 
         16408.0 
         16424.0 
         16432.0 
         16450.0 
         8262.0 
         8270.0 
         8271.0 
         8272.0 
         8274.0 
         8275.0 
         8278.0 
         8279.0 
         8286.0 
         8444.0 
         8445.0 
         8446.0 
         8447.0 
         8448.0 
         8449.0 
         8450.0 
         8451.0 
         16684.0 
         16686.0 
         16688.0 
         16690.0 
         16692.0 
         16694.0 
         16696.0 
         16698.0 
         8522.0 
         8543.0 
         8639.0 
         8679.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="16" digits="1" name="ltt_table1" rows="16" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="ltt_rpms" rows="16" units="RPM">
         700.0 
         900.0 
         1200.0 
         1400.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
         6500.0 
         7000.0 
         7200.0 
         7500.0 
      </constant>
<constant cols="1" digits="1" name="ltt_loads" rows="16" units="%">
         25.0 
         30.0 
         35.0 
         40.0 
         45.0 
         50.0 
         55.0 
         60.0 
         65.0 
         70.0 
         75.0 
         80.0 
         85.0 
         90.0 
         95.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="portusage" rows="148">
         7.0 
         7.0 
         7.0 
         7.0 
         0.0 
         0.0 
         0.0 
         0.0 
         10.0 
         10.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         4.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         19.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         17.0 
         106.0 
         0.0 
         106.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         9.0 
         0.0 
         101.0 
         0.0 
         121.0 
         5.0 
         0.0 
         20.0 
         59.0 
         18.0 
         117.0 
         60.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         13.0 
         0.0 
         16.0 
         0.0 
         0.0 
         14.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         100.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         4.0 
         101.0 
         5.0 
         5.0 
      </constant>
<constant cols="1" digits="0" name="portusage_a" rows="8">
         7.0 
         7.0 
         7.0 
         7.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_b" rows="8">
         10.0 
         10.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_e" rows="8">
         0.0 
         0.0 
         0.0 
         0.0 
         4.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_h" rows="8">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         19.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_j" rows="8">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_k" rows="8">
         17.0 
         106.0 
         0.0 
         106.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_m" rows="8">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_p" rows="8">
         0.0 
         0.0 
         9.0 
         0.0 
         101.0 
         0.0 
         121.0 
         5.0 
      </constant>
<constant cols="1" digits="0" name="portusage_t" rows="8">
         0.0 
         20.0 
         59.0 
         18.0 
         117.0 
         60.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_ad0h" rows="8">
         0.0 
         0.0 
         0.0 
         13.0 
         0.0 
         16.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_ad0l" rows="8">
         14.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         100.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_canin" rows="8">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_canout" rows="16">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_canadc" rows="24">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_canpwm" rows="8">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_pwmscl" rows="4">
         4.0 
         101.0 
         5.0 
         5.0 
      </constant>
<constant cols="1" digits="0" name="portusage_loop" rows="8">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="portusage_s" rows="8">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_15" rows="28" units="RAW">
         16.0 
         96.0 
         142.0 
         82.0 
         97.0 
         181.0 
         53.0 
         156.0 
         136.0 
         114.0 
         41.0 
         138.0 
         74.0 
         197.0 
         41.0 
         243.0 
         160.0 
         236.0 
         192.0 
         26.0 
         85.0 
         147.0 
         212.0 
         62.0 
         3.0 
         205.0 
         60.0 
         42.0 
      </constant>
</page>
<page number="16" size="1024">
<constant cols="12" digits="1" name="ego_auth_table" rows="12" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         0.0 0.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         0.0 0.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         0.0 0.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         0.0 0.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         0.0 0.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         0.0 0.0 7.0 7.0 7.0 7.0 7.0 7.0 7.0 7.0 7.0 7.0 
         0.0 0.0 5.0 5.0 5.0 5.0 5.0 5.0 5.0 5.0 5.0 5.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="ego_auth_rpms" rows="12" units="RPM">
         500.0 
         800.0 
         1100.0 
         1400.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
      </constant>
<constant cols="1" digits="1" name="ego_auth_loads" rows="12" units="kPa">
         30.0 
         40.0 
         50.0 
         55.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant cols="1" digits="0" name="vsslaunch_vss" rows="10" units="MPH">
         0.0 
         1.78952 
         3.57904 
         5.36856 
         7.15808 
         8.9476 
         10.73712 
         12.52664 
         14.31616 
         16.10568 
      </constant>
<constant cols="1" digits="0" name="vsslaunch_rpm" rows="10" units="RPM">
         7000.0 
         7000.0 
         7000.0 
         7000.0 
         7000.0 
         7000.0 
         7000.0 
         7000.0 
         7000.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="vsslaunch_retard" rows="10" units="deg">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="12" digits="0" name="ego_delay_table" rows="12" units="ms">
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
      </constant>
<constant cols="1" digits="0" name="ego_delay_rpms" rows="12" units="rpm">
         500.0 
         800.0 
         1100.0 
         1400.0 
         2000.0 
         2600.0 
         3100.0 
         3700.0 
         4300.0 
         4900.0 
         5400.0 
         6000.0 
      </constant>
<constant cols="1" digits="0" name="ego_delay_loads" rows="12" units="%">
         30.0 
         40.0 
         50.0 
         55.0 
         60.0 
         70.0 
         80.0 
         90.0 
         100.0 
         200.0 
         300.0 
         400.0 
      </constant>
<constant digits="0" name="ego_sensor_delay" units="ms">50.0</constant>
<constant name="generic_pid_flags_a_on">"Off"</constant>
<constant name="generic_pid_flags_a_type">"Type B"</constant>
<constant name="generic_pid_flags_a_direction">"Inverted (lower duty = higher PV)"</constant>
<constant name="generic_pid_flags_a_output_type">"PWM"</constant>
<constant name="generic_pid_flags_a_lookup_type">"Table"</constant>
<constant name="generic_pid_flags_b_on">"Off"</constant>
<constant name="generic_pid_flags_b_type">"Type B"</constant>
<constant name="generic_pid_flags_b_direction">"Normal (higher duty = higher PV)"</constant>
<constant name="generic_pid_flags_b_output_type">"PWM"</constant>
<constant name="generic_pid_flags_b_lookup_type">"Table"</constant>
<constant name="generic_pid_pwm_opts_freq_a">"250Hz"</constant>
<constant name="generic_pid_pwm_opts_load_a">"RPM"</constant>
<constant name="generic_pid_pwm_opts_freq_b">"11.1Hz"</constant>
<constant name="generic_pid_pwm_opts_load_b">"RPM"</constant>
<constant name="generic_pid_pwm_outs_a">"PWM Out 3"</constant>
<constant name="generic_pid_pwm_outs_b">"High Current Out 2"</constant>
<constant digits="0" name="generic_pid_load_offset_a">26.0</constant>
<constant digits="0" name="generic_pid_load_offset_b">24.0</constant>
<constant digits="0" name="generic_pid_load_size_a">2.0</constant>
<constant digits="0" name="generic_pid_load_size_b">2.0</constant>
<constant digits="0" name="generic_pid_PV_offset_a">26.0</constant>
<constant digits="0" name="generic_pid_PV_offset_b">106.0</constant>
<constant digits="0" name="generic_pid_PV_size_a">2.0</constant>
<constant digits="0" name="generic_pid_PV_size_b">2.0</constant>
<constant digits="1" name="generic_pid_upper_inputlim_a">19.0</constant>
<constant digits="1" name="generic_pid_upper_inputlim_b">100.0</constant>
<constant digits="1" name="generic_pid_lower_inputlim_a">7.0</constant>
<constant digits="1" name="generic_pid_lower_inputlim_b">0.0</constant>
<constant digits="1" name="generic_pid_output_upperlim_a" units="%">90.16</constant>
<constant digits="1" name="generic_pid_output_upperlim_b" units="%">98.784</constant>
<constant digits="1" name="generic_pid_output_lowerlim_a" units="%">5.096</constant>
<constant digits="1" name="generic_pid_output_lowerlim_b" units="%">1.176</constant>
<constant cols="1" digits="0" name="generic_pid_rpms_a" rows="8" units="rpm">
         0.0 
         285.0 
         742.0 
         1271.0 
         1628.0 
         3585.0 
         5000.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="generic_pid_loadvals_a" rows="8" units="%">
         9.0 
         11.0 
         11.0 
         12.0 
         13.0 
         14.0 
         15.0 
         17.0 
      </constant>
<constant cols="1" digits="0" name="generic_pid_rpms_b" rows="8" units="rpm">
         500.0 
         1000.0 
         1500.0 
         2000.0 
         3000.0 
         4000.0 
         5000.0 
         6000.0 
      </constant>
<constant cols="1" digits="1" name="generic_pid_loadvals_b" rows="8" units="%">
         0.0 
         20.0 
         30.0 
         40.0 
         50.0 
         60.0 
         80.0 
         100.0 
      </constant>
<constant cols="8" digits="1" name="generic_pid_targets_a" rows="8">
         100.0 82.2 64.3 50.0 50.0 50.0 50.0 50.0 
         100.0 64.4 50.0 50.9 55.1 56.0 56.0 56.0 
         100.0 64.4 50.0 50.9 55.1 56.0 56.0 56.0 
         100.0 64.4 50.0 50.8 54.6 55.3 55.3 58.0 
         100.0 65.6 51.7 52.6 57.4 59.5 60.3 64.3 
         100.0 67.9 55.0 56.4 63.6 68.4 71.0 75.0 
         100.0 71.5 60.0 62.1 72.8 81.3 86.0 90.0 
         100.0 92.9 90.0 90.0 90.0 90.0 90.0 90.0 
      </constant>
<constant cols="8" digits="1" name="generic_pid_targets_b" rows="8">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant digits="0" name="generic_pid_control_interval_a" units="ms">20.0</constant>
<constant digits="0" name="generic_pid_control_interval_b" units="ms">100.0</constant>
<constant digits="0" name="generic_pid_P_a" units="%">0.0</constant>
<constant digits="0" name="generic_pid_P_b" units="%">100.0</constant>
<constant digits="0" name="generic_pid_I_a" units="%">100.0</constant>
<constant digits="0" name="generic_pid_I_b" units="%">100.0</constant>
<constant digits="0" name="generic_pid_D_a" units="%">0.0</constant>
<constant digits="0" name="generic_pid_D_b" units="%">100.0</constant>
<constant cols="1" digits="0" name="tcslipx" rows="9" units="Knob%">
         0.0 
         12.5184 
         25.0368 
         37.5552 
         49.9758 
         62.0052 
         75.1104 
         88.02 
         100.0494 
      </constant>
<constant cols="1" digits="0" name="tcslipy" rows="9" units="Slip threshold %">
         0.0 
         12.0 
         25.0 
         38.0 
         50.0 
         62.0 
         75.0 
         88.0 
         100.0 
      </constant>
<constant digits="0" name="outmsg1_offset01">0.0</constant>
<constant digits="0" name="outmsg1_offset02">0.0</constant>
<constant digits="0" name="outmsg1_offset03">0.0</constant>
<constant digits="0" name="outmsg1_offset04">0.0</constant>
<constant digits="0" name="outmsg1_offset05">0.0</constant>
<constant digits="0" name="outmsg1_offset06">0.0</constant>
<constant digits="0" name="outmsg1_offset07">0.0</constant>
<constant digits="0" name="outmsg1_offset08">0.0</constant>
<constant digits="0" name="outmsg1_offset09">0.0</constant>
<constant digits="0" name="outmsg1_offset10">0.0</constant>
<constant digits="0" name="outmsg1_offset11">0.0</constant>
<constant digits="0" name="outmsg1_offset12">0.0</constant>
<constant digits="0" name="outmsg1_offset13">0.0</constant>
<constant digits="0" name="outmsg1_offset14">0.0</constant>
<constant digits="0" name="outmsg1_offset15">0.0</constant>
<constant digits="0" name="outmsg1_offset16">0.0</constant>
<constant digits="0" name="outmsg1_size01">0.0</constant>
<constant digits="0" name="outmsg1_size02">0.0</constant>
<constant digits="0" name="outmsg1_size03">0.0</constant>
<constant digits="0" name="outmsg1_size04">0.0</constant>
<constant digits="0" name="outmsg1_size05">0.0</constant>
<constant digits="0" name="outmsg1_size06">0.0</constant>
<constant digits="0" name="outmsg1_size07">0.0</constant>
<constant digits="0" name="outmsg1_size08">0.0</constant>
<constant digits="0" name="outmsg1_size09">0.0</constant>
<constant digits="0" name="outmsg1_size10">0.0</constant>
<constant digits="0" name="outmsg1_size11">0.0</constant>
<constant digits="0" name="outmsg1_size12">0.0</constant>
<constant digits="0" name="outmsg1_size13">0.0</constant>
<constant digits="0" name="outmsg1_size14">0.0</constant>
<constant digits="0" name="outmsg1_size15">0.0</constant>
<constant digits="0" name="outmsg1_size16">0.0</constant>
<constant digits="0" name="outmsg2_offset01">0.0</constant>
<constant digits="0" name="outmsg2_offset02">0.0</constant>
<constant digits="0" name="outmsg2_offset03">0.0</constant>
<constant digits="0" name="outmsg2_offset04">0.0</constant>
<constant digits="0" name="outmsg2_offset05">0.0</constant>
<constant digits="0" name="outmsg2_offset06">0.0</constant>
<constant digits="0" name="outmsg2_offset07">0.0</constant>
<constant digits="0" name="outmsg2_offset08">0.0</constant>
<constant digits="0" name="outmsg2_offset09">0.0</constant>
<constant digits="0" name="outmsg2_offset10">0.0</constant>
<constant digits="0" name="outmsg2_offset11">0.0</constant>
<constant digits="0" name="outmsg2_offset12">0.0</constant>
<constant digits="0" name="outmsg2_offset13">0.0</constant>
<constant digits="0" name="outmsg2_offset14">0.0</constant>
<constant digits="0" name="outmsg2_offset15">0.0</constant>
<constant digits="0" name="outmsg2_offset16">0.0</constant>
<constant digits="0" name="outmsg2_size01">0.0</constant>
<constant digits="0" name="outmsg2_size02">0.0</constant>
<constant digits="0" name="outmsg2_size03">0.0</constant>
<constant digits="0" name="outmsg2_size04">0.0</constant>
<constant digits="0" name="outmsg2_size05">0.0</constant>
<constant digits="0" name="outmsg2_size06">0.0</constant>
<constant digits="0" name="outmsg2_size07">0.0</constant>
<constant digits="0" name="outmsg2_size08">0.0</constant>
<constant digits="0" name="outmsg2_size09">0.0</constant>
<constant digits="0" name="outmsg2_size10">0.0</constant>
<constant digits="0" name="outmsg2_size11">0.0</constant>
<constant digits="0" name="outmsg2_size12">0.0</constant>
<constant digits="0" name="outmsg2_size13">0.0</constant>
<constant digits="0" name="outmsg2_size14">0.0</constant>
<constant digits="0" name="outmsg2_size15">0.0</constant>
<constant digits="0" name="outmsg2_size16">0.0</constant>
<constant digits="0" name="outmsg3_offset01">0.0</constant>
<constant digits="0" name="outmsg3_offset02">0.0</constant>
<constant digits="0" name="outmsg3_offset03">0.0</constant>
<constant digits="0" name="outmsg3_offset04">0.0</constant>
<constant digits="0" name="outmsg3_offset05">0.0</constant>
<constant digits="0" name="outmsg3_offset06">0.0</constant>
<constant digits="0" name="outmsg3_offset07">0.0</constant>
<constant digits="0" name="outmsg3_offset08">0.0</constant>
<constant digits="0" name="outmsg3_offset09">0.0</constant>
<constant digits="0" name="outmsg3_offset10">0.0</constant>
<constant digits="0" name="outmsg3_offset11">0.0</constant>
<constant digits="0" name="outmsg3_offset12">0.0</constant>
<constant digits="0" name="outmsg3_offset13">0.0</constant>
<constant digits="0" name="outmsg3_offset14">0.0</constant>
<constant digits="0" name="outmsg3_offset15">0.0</constant>
<constant digits="0" name="outmsg3_offset16">0.0</constant>
<constant digits="0" name="outmsg3_size01">0.0</constant>
<constant digits="0" name="outmsg3_size02">0.0</constant>
<constant digits="0" name="outmsg3_size03">0.0</constant>
<constant digits="0" name="outmsg3_size04">0.0</constant>
<constant digits="0" name="outmsg3_size05">0.0</constant>
<constant digits="0" name="outmsg3_size06">0.0</constant>
<constant digits="0" name="outmsg3_size07">0.0</constant>
<constant digits="0" name="outmsg3_size08">0.0</constant>
<constant digits="0" name="outmsg3_size09">0.0</constant>
<constant digits="0" name="outmsg3_size10">0.0</constant>
<constant digits="0" name="outmsg3_size11">0.0</constant>
<constant digits="0" name="outmsg3_size12">0.0</constant>
<constant digits="0" name="outmsg3_size13">0.0</constant>
<constant digits="0" name="outmsg3_size14">0.0</constant>
<constant digits="0" name="outmsg3_size15">0.0</constant>
<constant digits="0" name="outmsg3_size16">0.0</constant>
<constant digits="0" name="outmsg4_offset01">0.0</constant>
<constant digits="0" name="outmsg4_offset02">0.0</constant>
<constant digits="0" name="outmsg4_offset03">0.0</constant>
<constant digits="0" name="outmsg4_offset04">0.0</constant>
<constant digits="0" name="outmsg4_offset05">0.0</constant>
<constant digits="0" name="outmsg4_offset06">0.0</constant>
<constant digits="0" name="outmsg4_offset07">0.0</constant>
<constant digits="0" name="outmsg4_offset08">0.0</constant>
<constant digits="0" name="outmsg4_offset09">0.0</constant>
<constant digits="0" name="outmsg4_offset10">0.0</constant>
<constant digits="0" name="outmsg4_offset11">0.0</constant>
<constant digits="0" name="outmsg4_offset12">0.0</constant>
<constant digits="0" name="outmsg4_offset13">0.0</constant>
<constant digits="0" name="outmsg4_offset14">0.0</constant>
<constant digits="0" name="outmsg4_offset15">0.0</constant>
<constant digits="0" name="outmsg4_offset16">0.0</constant>
<constant digits="0" name="outmsg4_size01">0.0</constant>
<constant digits="0" name="outmsg4_size02">0.0</constant>
<constant digits="0" name="outmsg4_size03">0.0</constant>
<constant digits="0" name="outmsg4_size04">0.0</constant>
<constant digits="0" name="outmsg4_size05">0.0</constant>
<constant digits="0" name="outmsg4_size06">0.0</constant>
<constant digits="0" name="outmsg4_size07">0.0</constant>
<constant digits="0" name="outmsg4_size08">0.0</constant>
<constant digits="0" name="outmsg4_size09">0.0</constant>
<constant digits="0" name="outmsg4_size10">0.0</constant>
<constant digits="0" name="outmsg4_size11">0.0</constant>
<constant digits="0" name="outmsg4_size12">0.0</constant>
<constant digits="0" name="outmsg4_size13">0.0</constant>
<constant digits="0" name="outmsg4_size14">0.0</constant>
<constant digits="0" name="outmsg4_size15">0.0</constant>
<constant digits="0" name="outmsg4_size16">0.0</constant>
<constant digits="0" name="UNALLOCATED_SPACE_16_0" units="RAW">
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_16_1" units="RAW">
         0.0 
      </constant>
</page>
<page number="17" size="1024">
<constant name="etc_opt_on">"Off"</constant>
<constant name="etc_opt_follow">"Off"</constant>
<constant digits="0" name="etc_canbase">256.0</constant>
<constant digits="0" name="etc_app_min">0.0</constant>
<constant digits="0" name="etc_app_max">1023.0</constant>
<constant digits="0" name="etc_tp_min">0.0</constant>
<constant digits="0" name="etc_tp_max">1023.0</constant>
<constant digits="0" name="etc_tp_act_min">0.0</constant>
<constant digits="0" name="etc_tp_act_max">1023.0</constant>
<constant digits="2" name="etc_testpos" units="%">0.0</constant>
<constant cols="1" digits="2" name="etc_pedal_pos" rows="10" units="%">
         0.0 
         5.0 
         10.0 
         20.0 
         30.0 
         40.0 
         50.0 
         70.0 
         90.0 
         100.0 
      </constant>
<constant cols="1" digits="0" name="etc_rpms" rows="10">
         0.0 
         500.0 
         1000.0 
         2000.0 
         3000.0 
         4000.0 
         5000.0 
         6000.0 
         7000.0 
         8000.0 
      </constant>
<constant cols="10" digits="2" name="etc_targ_pos" rows="10" units="%">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         2.5 5.0 5.0 5.0 5.0 5.0 5.0 5.0 5.0 5.0 
         5.0 7.5 10.0 10.0 10.0 10.0 10.0 10.0 10.0 10.0 
         10.0 15.0 20.0 20.0 20.0 20.0 20.0 20.0 20.0 20.0 
         15.0 22.5 30.0 30.0 30.0 30.0 30.0 30.0 30.0 30.0 
         20.0 30.0 40.0 40.0 40.0 40.0 40.0 40.0 40.0 40.0 
         25.0 37.5 50.0 50.0 50.0 50.0 50.0 50.0 50.0 50.0 
         35.0 52.5 70.0 70.0 70.0 70.0 70.0 70.0 70.0 70.0 
         45.0 67.5 90.0 90.0 90.0 90.0 90.0 90.0 90.0 90.0 
         50.0 75.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
      </constant>
<constant digits="2" name="etc_idlescale" units="%">5.0</constant>
<constant cols="8" digits="1" name="dwell_table_values" rows="8" units="%">
         2.5 2.5 2.5 2.5 2.5 2.5 2.5 2.5 
         2.5 2.5 2.5 2.5 2.5 2.5 2.5 2.5 
         2.5 2.5 2.5 2.5 2.5 2.5 2.5 2.5 
         2.5 2.5 2.5 2.5 2.5 2.5 2.5 2.5 
         2.5 2.5 2.5 2.5 2.5 2.5 2.5 2.5 
         2.5 2.5 2.5 2.5 2.5 2.5 2.5 2.5 
         2.5 2.5 2.5 2.5 2.5 2.5 2.5 2.5 
         2.5 2.5 2.5 2.5 2.5 2.5 2.5 2.5 
      </constant>
<constant cols="1" digits="0" name="dwell_table_rpms" rows="8" units="RPM">
         500.0 
         1000.0 
         1500.0 
         2000.0 
         3000.0 
         4000.0 
         6000.0 
         8000.0 
      </constant>
<constant cols="1" digits="1" name="dwell_table_loads" rows="8" units="kPa">
         20.0 
         40.0 
         60.0 
         80.0 
         100.0 
         150.0 
         200.0 
         255.0 
      </constant>
<constant name="can_rcv_var1">"Off"</constant>
<constant name="can_rcv_var2">"Off"</constant>
<constant name="can_rcv_var3">"Off"</constant>
<constant name="can_rcv_var4">"Off"</constant>
<constant name="can_rcv_var5">"Off"</constant>
<constant name="can_rcv_var6">"Off"</constant>
<constant name="can_rcv_var7">"Off"</constant>
<constant name="can_rcv_var8">"Off"</constant>
<constant name="can_rcv_var9">"Off"</constant>
<constant name="can_rcv_var10">"Off"</constant>
<constant name="can_rcv_var11">"Off"</constant>
<constant name="can_rcv_var12">"Off"</constant>
<constant name="can_rcv_var13">"Off"</constant>
<constant name="can_rcv_var14">"Off"</constant>
<constant name="can_rcv_var15">"Off"</constant>
<constant name="can_rcv_var16">"Off"</constant>
<constant digits="0" name="can_rcv_off1">0.0</constant>
<constant digits="0" name="can_rcv_off2">0.0</constant>
<constant digits="0" name="can_rcv_off3">0.0</constant>
<constant digits="0" name="can_rcv_off4">0.0</constant>
<constant digits="0" name="can_rcv_off5">0.0</constant>
<constant digits="0" name="can_rcv_off6">0.0</constant>
<constant digits="0" name="can_rcv_off7">0.0</constant>
<constant digits="0" name="can_rcv_off8">0.0</constant>
<constant digits="0" name="can_rcv_off9">0.0</constant>
<constant digits="0" name="can_rcv_off10">0.0</constant>
<constant digits="0" name="can_rcv_off11">0.0</constant>
<constant digits="0" name="can_rcv_off12">0.0</constant>
<constant digits="0" name="can_rcv_off13">0.0</constant>
<constant digits="0" name="can_rcv_off14">0.0</constant>
<constant digits="0" name="can_rcv_off15">0.0</constant>
<constant digits="0" name="can_rcv_off16">0.0</constant>
<constant name="can_rcv_size1">"1U"</constant>
<constant name="can_rcv_size2">"1U"</constant>
<constant name="can_rcv_size3">"1U"</constant>
<constant name="can_rcv_size4">"1U"</constant>
<constant name="can_rcv_size5">"1U"</constant>
<constant name="can_rcv_size6">"1U"</constant>
<constant name="can_rcv_size7">"1U"</constant>
<constant name="can_rcv_size8">"1U"</constant>
<constant name="can_rcv_size9">"1U"</constant>
<constant name="can_rcv_size10">"1U"</constant>
<constant name="can_rcv_size11">"1U"</constant>
<constant name="can_rcv_size12">"1U"</constant>
<constant name="can_rcv_size13">"1U"</constant>
<constant name="can_rcv_size14">"1U"</constant>
<constant name="can_rcv_size15">"1U"</constant>
<constant name="can_rcv_size16">"1U"</constant>
<constant name="can_rcv_size_ext1">"Std"</constant>
<constant name="can_rcv_size_ext2">"Std"</constant>
<constant name="can_rcv_size_ext3">"Std"</constant>
<constant name="can_rcv_size_ext4">"Std"</constant>
<constant name="can_rcv_size_ext5">"Std"</constant>
<constant name="can_rcv_size_ext6">"Std"</constant>
<constant name="can_rcv_size_ext7">"Std"</constant>
<constant name="can_rcv_size_ext8">"Std"</constant>
<constant name="can_rcv_size_ext9">"Std"</constant>
<constant name="can_rcv_size_ext10">"Std"</constant>
<constant name="can_rcv_size_ext11">"Std"</constant>
<constant name="can_rcv_size_ext12">"Std"</constant>
<constant name="can_rcv_size_ext13">"Std"</constant>
<constant name="can_rcv_size_ext14">"Std"</constant>
<constant name="can_rcv_size_ext15">"Std"</constant>
<constant name="can_rcv_size_ext16">"Std"</constant>
<constant digits="0" name="can_rcv_mult1">1.0</constant>
<constant digits="0" name="can_rcv_mult2">1.0</constant>
<constant digits="0" name="can_rcv_mult3">1.0</constant>
<constant digits="0" name="can_rcv_mult4">1.0</constant>
<constant digits="0" name="can_rcv_mult5">1.0</constant>
<constant digits="0" name="can_rcv_mult6">1.0</constant>
<constant digits="0" name="can_rcv_mult7">1.0</constant>
<constant digits="0" name="can_rcv_mult8">1.0</constant>
<constant digits="0" name="can_rcv_mult9">1.0</constant>
<constant digits="0" name="can_rcv_mult10">1.0</constant>
<constant digits="0" name="can_rcv_mult11">1.0</constant>
<constant digits="0" name="can_rcv_mult12">1.0</constant>
<constant digits="0" name="can_rcv_mult13">1.0</constant>
<constant digits="0" name="can_rcv_mult14">1.0</constant>
<constant digits="0" name="can_rcv_mult15">1.0</constant>
<constant digits="0" name="can_rcv_mult16">1.0</constant>
<constant digits="0" name="can_rcv_div1">1.0</constant>
<constant digits="0" name="can_rcv_div2">1.0</constant>
<constant digits="0" name="can_rcv_div3">1.0</constant>
<constant digits="0" name="can_rcv_div4">1.0</constant>
<constant digits="0" name="can_rcv_div5">1.0</constant>
<constant digits="0" name="can_rcv_div6">1.0</constant>
<constant digits="0" name="can_rcv_div7">1.0</constant>
<constant digits="0" name="can_rcv_div8">1.0</constant>
<constant digits="0" name="can_rcv_div9">1.0</constant>
<constant digits="0" name="can_rcv_div10">1.0</constant>
<constant digits="0" name="can_rcv_div11">1.0</constant>
<constant digits="0" name="can_rcv_div12">1.0</constant>
<constant digits="0" name="can_rcv_div13">1.0</constant>
<constant digits="0" name="can_rcv_div14">1.0</constant>
<constant digits="0" name="can_rcv_div15">1.0</constant>
<constant digits="0" name="can_rcv_div16">1.0</constant>
<constant digits="0" name="can_rcv_add1">0.0</constant>
<constant digits="0" name="can_rcv_add2">0.0</constant>
<constant digits="0" name="can_rcv_add3">0.0</constant>
<constant digits="0" name="can_rcv_add4">0.0</constant>
<constant digits="0" name="can_rcv_add5">0.0</constant>
<constant digits="0" name="can_rcv_add6">0.0</constant>
<constant digits="0" name="can_rcv_add7">0.0</constant>
<constant digits="0" name="can_rcv_add8">0.0</constant>
<constant digits="0" name="can_rcv_add9">0.0</constant>
<constant digits="0" name="can_rcv_add10">0.0</constant>
<constant digits="0" name="can_rcv_add11">0.0</constant>
<constant digits="0" name="can_rcv_add12">0.0</constant>
<constant digits="0" name="can_rcv_add13">0.0</constant>
<constant digits="0" name="can_rcv_add14">0.0</constant>
<constant digits="0" name="can_rcv_add15">0.0</constant>
<constant digits="0" name="can_rcv_add16">0.0</constant>
<constant digits="0" name="can_bcast_user_id">1234.0</constant>
<constant digits="0" name="can_bcast_user_d0">0.0</constant>
<constant digits="0" name="can_bcast_user_d1">0.0</constant>
<constant digits="0" name="can_bcast_user_d2">0.0</constant>
<constant digits="0" name="can_bcast_user_d3">0.0</constant>
<constant digits="0" name="can_bcast_user_d4">0.0</constant>
<constant digits="0" name="can_bcast_user_d5">0.0</constant>
<constant digits="0" name="can_bcast_user_d6">0.0</constant>
<constant digits="0" name="can_bcast_user_d7">0.0</constant>
<constant name="iobox_opta1">"Off"</constant>
<constant name="iobox_opta1adv">"Automatic"</constant>
<constant name="iobox_opta1canin">"CANIN1"</constant>
<constant name="iobox_opta1canout">"CANOUT1"</constant>
<constant name="iobox_opta1canadc">"CANADC1"</constant>
<constant name="iobox_opta2">"Off"</constant>
<constant name="iobox_opta2adv">"Automatic"</constant>
<constant name="iobox_opta2canin">"CANIN4"</constant>
<constant name="iobox_opta2canout">"CANOUT9"</constant>
<constant name="iobox_opta2canadc">"CANADC9"</constant>
<constant name="iobox_opta3">"Off"</constant>
<constant name="iobox_opta3adv">"Automatic"</constant>
<constant name="iobox_opta3canin">"CANIN7"</constant>
<constant name="iobox_opta3canout">"Off"</constant>
<constant name="iobox_opta3canadc">"CANADC17"</constant>
<constant name="iobox_opta4">"Off"</constant>
<constant name="iobox_opta4adv">"Automatic"</constant>
<constant name="iobox_opta4canin">"CANIN7"</constant>
<constant name="iobox_opta4canout">"Off"</constant>
<constant name="iobox_opta4canadc">"CANADC17"</constant>
<constant name="iobox_optb1tachrate">"50Hz"</constant>
<constant name="iobox_optb1inrate">"20Hz"</constant>
<constant name="iobox_optb1outrate">"20Hz"</constant>
<constant name="iobox_optb1vss">"Speed in 1,2"</constant>
<constant name="iobox_optb2tachrate">"50Hz"</constant>
<constant name="iobox_optb2inrate">"20Hz"</constant>
<constant name="iobox_optb2outrate">"20Hz"</constant>
<constant name="iobox_optb2vss">"Off"</constant>
<constant name="iobox_optb3tachrate">"50Hz"</constant>
<constant name="iobox_optb3inrate">"20Hz"</constant>
<constant name="iobox_optb3outrate">"20Hz"</constant>
<constant name="iobox_optb3vss">"Off"</constant>
<constant name="iobox_optb4tachrate">"50Hz"</constant>
<constant name="iobox_optb4inrate">"20Hz"</constant>
<constant name="iobox_optb4outrate">"20Hz"</constant>
<constant name="iobox_optb4vss">"Off"</constant>
<constant digits="0" name="iobox_id1">512.0</constant>
<constant digits="0" name="iobox_id2">544.0</constant>
<constant digits="0" name="iobox_id3">576.0</constant>
<constant digits="0" name="iobox_id4">608.0</constant>
<constant name="pitlim_opt_on">"Off"</constant>
<constant name="pitlim_opt_mode">"Fixed"</constant>
<constant name="pitlim_opt_retard">"Off"</constant>
<constant name="pitlim_opt_spkcut">"Off"</constant>
<constant name="pitlim_opt_fuelcut">"Off"</constant>
<constant name="pitlim_opt_fuelprog">"Off"</constant>
<constant name="pitlim_opt_vssrpm">"VSS"</constant>
<constant name="pitlim_enin">"Off"</constant>
<constant digits="0" name="pitlim_speed" units="MPH">10.06605</constant>
<constant digits="1" name="pitlim_retardmax" units="deg">30.0</constant>
<constant digits="0" name="pitlim_sensitivity">10.0</constant>
<constant digits="1" name="pitlim_speed_range" units="MPH">11.1845</constant>
<constant digits="0" name="pitlim_rpm_range" units="RPM">200.0</constant>
<constant cols="1" digits="0" name="taeBins" rows="4" units="%">
         20.0 
         20.0 
         20.0 
         19.0 
      </constant>
<constant cols="1" digits="0" name="maeBins" rows="4" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="taeRates" rows="4" units="%/s">
         24.0 
         297.6 
         576.0 
         864.0 
      </constant>
<constant cols="1" digits="0" name="maeRates" rows="4" units="kPa/s">
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="taeBins2" rows="4" units="%">
         6.0 
         15.0 
         30.0 
         40.0 
      </constant>
<constant cols="1" digits="0" name="maeBins2" rows="4" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="taeRates2" rows="4" units="%/s">
         210.0 
         400.0 
         800.0 
         1000.0 
      </constant>
<constant cols="1" digits="0" name="maeRates2" rows="4" units="kPa/s">
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="accel_mapdots" rows="8" units="kpa/sec">
         -500.0 
         -200.0 
         -100.0 
         -50.0 
         50.0 
         200.0 
         500.0 
         1000.0 
      </constant>
<constant cols="1" digits="1" name="accel_tpsdots" rows="8" units="%/sec">
         -500.0 
         -200.0 
         6.1 
         67.1 
         195.1 
         408.5 
         579.3 
         780.5 
      </constant>
<constant cols="1" digits="1" name="accel_mapdot_amts" rows="8" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         1.0 
         10.0 
         100.0 
         120.0 
      </constant>
<constant cols="1" digits="1" name="accel_tpsdot_amts" rows="8" units="%">
         0.0 
         0.0 
         0.0 
         65.0 
         75.0 
         77.0 
         78.0 
         79.0 
      </constant>
<constant cols="1" digits="0" name="accel_mapdots2" rows="8" units="kpa/sec">
         -500.0 
         -200.0 
         -100.0 
         -50.0 
         50.0 
         200.0 
         500.0 
         1000.0 
      </constant>
<constant cols="1" digits="1" name="accel_tpsdots2" rows="8" units="%/sec">
         -500.0 
         -200.0 
         -100.0 
         -50.0 
         50.0 
         200.0 
         500.0 
         1000.0 
      </constant>
<constant cols="1" digits="1" name="accel_mapdot_amts2" rows="8" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         1.0 
         10.0 
         100.0 
         120.0 
      </constant>
<constant cols="1" digits="1" name="accel_tpsdot_amts2" rows="8" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         1.0 
         10.0 
         100.0 
         120.0 
      </constant>
<constant digits="0" name="dashbcast_id1">1512.0</constant>
<constant name="dashbcast_opta1">"Off"</constant>
<constant name="dashbcast_opta1adv">"Automatic"</constant>
<constant name="dashbcast_opta4outrate">"50Hz"</constant>
<constant name="canrx1_opt_accel">"Off"</constant>
<constant digits="0" name="canrx1_rt_gps_base">769.0</constant>
<constant digits="0" name="canrx1_rt_accel_base">768.0</constant>
<constant digits="0" name="can_rcv_id1">0.0</constant>
<constant digits="0" name="can_rcv_id2">0.0</constant>
<constant digits="0" name="can_rcv_id3">0.0</constant>
<constant digits="0" name="can_rcv_id4">0.0</constant>
<constant digits="0" name="can_rcv_id5">0.0</constant>
<constant digits="0" name="can_rcv_id6">0.0</constant>
<constant digits="0" name="can_rcv_id7">0.0</constant>
<constant digits="0" name="can_rcv_id8">0.0</constant>
<constant digits="0" name="can_rcv_id9">0.0</constant>
<constant digits="0" name="can_rcv_id10">0.0</constant>
<constant digits="0" name="can_rcv_id11">0.0</constant>
<constant digits="0" name="can_rcv_id12">0.0</constant>
<constant digits="0" name="can_rcv_id13">0.0</constant>
<constant digits="0" name="can_rcv_id14">0.0</constant>
<constant digits="0" name="can_rcv_id15">0.0</constant>
<constant digits="0" name="can_rcv_id16">0.0</constant>
<constant digits="0" name="UNALLOCATED_SPACE_17_0" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_17_1" rows="2" units="RAW">
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_SPACE_17_2" rows="32" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_17" rows="204" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
</page>
<page number="18" size="1024">
<constant cols="8" digits="0" name="boost_dome_targets1" rows="8" units="kPa">
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
      </constant>
<constant cols="8" digits="0" name="boost_dome_targets2" rows="8" units="kPa">
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
         100.0 100.0 100.0 100.0 100.0 100.0 100.0 100.0 
      </constant>
<constant cols="1" digits="0" name="boost_dome_target_rpms1" rows="8" units="RPM">
         1500.0 
         2180.0 
         2860.0 
         3540.0 
         4220.0 
         4900.0 
         5580.0 
         6260.0 
      </constant>
<constant cols="1" digits="0" name="boost_dome_target_rpms2" rows="8" units="RPM">
         1500.0 
         2180.0 
         2860.0 
         3540.0 
         4220.0 
         4900.0 
         5580.0 
         6260.0 
      </constant>
<constant cols="1" digits="0" name="boost_dome_target_kpas1" rows="8" units="kPa">
         100.0 
         140.0 
         180.0 
         220.0 
         260.0 
         300.0 
         340.0 
         380.0 
      </constant>
<constant cols="1" digits="0" name="boost_dome_target_kpas2" rows="8" units="kPa">
         100.0 
         140.0 
         180.0 
         220.0 
         260.0 
         300.0 
         340.0 
         380.0 
      </constant>
<constant digits="1" name="boost_dome_Kp1" units="%">100.0</constant>
<constant digits="1" name="boost_dome_Kp2" units="%">100.0</constant>
<constant digits="1" name="boost_dome_Ki1" units="%">100.0</constant>
<constant digits="1" name="boost_dome_Ki2" units="%">100.0</constant>
<constant digits="1" name="boost_dome_Kd1" units="%">100.0</constant>
<constant digits="1" name="boost_dome_Kd2" units="%">100.0</constant>
<constant name="boost_dome_outputs_fill1">"Stepper Out 1"</constant>
<constant name="boost_dome_outputs_fill2">"Stepper Out 1"</constant>
<constant name="boost_dome_settings1_emptydome_offboost">"Do not empty"</constant>
<constant name="boost_dome_settings1_advanced">"Basic mode"</constant>
<constant name="boost_dome_settings1_mode">"Simple"</constant>
<constant digits="0" name="boost_dome_empty_out_mins1" units="%">0.0</constant>
<constant digits="0" name="boost_dome_empty_out_mins2" units="%">0.0</constant>
<constant digits="0" name="boost_dome_empty_out_maxs1" units="%">100.0</constant>
<constant digits="0" name="boost_dome_empty_out_maxs2" units="%">100.0</constant>
<constant digits="1" name="boost_dome_hyst1" units="kPa">10.0</constant>
<constant digits="1" name="boost_dome_hyst2" units="kPa">10.0</constant>
<constant digits="1" name="boost_dome_testtarg" units="kPa">130.0</constant>
<constant cols="1" digits="2" name="n2o1_time" rows="10" units="s">
         0.0 
         0.556 
         1.111 
         1.667 
         2.222 
         2.778 
         3.333 
         3.889 
         4.444 
         5.0 
      </constant>
<constant cols="1" digits="0" name="n2o1_rpm" rows="10" units="RPM">
         3000.0 
         3278.0 
         3556.0 
         3833.0 
         4111.0 
         4389.0 
         4667.0 
         4944.0 
         5222.0 
         5500.0 
      </constant>
<constant cols="1" digits="1" name="n2o1_vss" rows="10" units="MPH">
         0.0 
         22.369 
         44.738 
         67.107 
         89.476 
         111.845 
         134.214 
         156.583 
         178.952 
         201.321 
      </constant>
<constant cols="1" digits="1" name="n2o1_duty" rows="10" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="3" name="n2o1_pw" rows="10" units="ms">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="n2o1_retard" rows="10" units="deg">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="2" name="n2o2_time" rows="10" units="s">
         5.0 
         5.556 
         6.111 
         6.667 
         7.222 
         7.778 
         8.333 
         8.889 
         9.444 
         10.0 
      </constant>
<constant cols="1" digits="0" name="n2o2_rpm" rows="10" units="RPM">
         3000.0 
         3278.0 
         3556.0 
         3833.0 
         4111.0 
         4389.0 
         4667.0 
         4944.0 
         5222.0 
         5500.0 
      </constant>
<constant cols="1" digits="1" name="n2o2_vss" rows="10" units="MPH">
         0.0 
         22.369 
         44.738 
         67.107 
         89.476 
         111.845 
         134.214 
         156.583 
         178.952 
         201.321 
      </constant>
<constant cols="1" digits="1" name="n2o2_duty" rows="10" units="%">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="3" name="n2o2_pw" rows="10" units="ms">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="n2o2_retard" rows="10" units="deg">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="1" name="alternator_pvolts" rows="6" units="V">
         12.0 
         12.8 
         13.6 
         14.4 
         15.2 
         16.0 
      </constant>
<constant cols="1" digits="1" name="alternator_periodv" rows="6" units="ms">
         0.512 
         3.456 
         6.4 
         9.344 
         12.288 
         15.104 
      </constant>
<constant cols="1" digits="1" name="alternator_temp" rows="6" units="°F">
         -40.0 
         -12.0 
         16.0 
         44.0 
         72.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="alternator_targvolts" rows="6" units="V">
         14.8 
         14.6 
         14.4 
         14.2 
         14.0 
         13.8 
      </constant>
<constant cols="1" digits="1" name="alternator_dvolts" rows="6" units="V">
         11.0 
         11.8 
         12.0 
         13.8 
         14.8 
         15.7 
      </constant>
<constant cols="1" digits="1" name="alternator_dutyv" rows="6">
         10.0 
         26.0 
         45.0 
         47.0 
         44.0 
         47.0 
      </constant>
<constant digits="0" name="boost_dome_sensitivities1">200.0</constant>
<constant digits="0" name="boost_dome_sensitivities2">200.0</constant>
<constant digits="0" name="boost_dome_fill_out_mins1" units="%">0.0</constant>
<constant digits="0" name="boost_dome_fill_out_mins2" units="%">0.0</constant>
<constant digits="0" name="boost_dome_fill_out_maxs1" units="%">100.0</constant>
<constant digits="0" name="boost_dome_fill_out_maxs2" units="%">100.0</constant>
<constant digits="1" name="boost_ctl_dome_min" units="kPa">100.0</constant>
<constant digits="1" name="boost_ctl_dome_max" units="kPa">400.0</constant>
<constant name="boost_dome_inputs1">"Sensor 1"</constant>
<constant name="boost_dome_inputs2">"Sensor 1"</constant>
<constant name="boost_dome_outputs_empty1">"Stepper Out 2"</constant>
<constant name="boost_dome_outputs_empty2">"Stepper Out 2"</constant>
<constant cols="1" digits="0" name="vvt_onoff_rpms" rows="8" units="rpm">
         2400.0 
         3000.0 
         3600.0 
         4200.0 
         4800.0 
         5500.0 
         6260.0 
         7000.0 
      </constant>
<constant cols="1" digits="1" name="vvt_onoff_loads" rows="8" units="%">
         40.0 
         48.0 
         56.0 
         63.1 
         69.4 
         76.5 
         83.8 
         90.0 
      </constant>
<constant name="boost_dome_testopt">"Off"</constant>
<constant cols="1" digits="1" name="n2o1_fuelpct" rows="10" units="%">
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
      </constant>
<constant cols="1" digits="1" name="n2o2_fuelpct" rows="10" units="%">
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
         100.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_18_0" units="RAW">
         0.0 
      </constant>
<constant digits="0" name="UNALLOCATED_SPACE_18_1" units="RAW">
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_18" rows="332" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
</page>
<page number="19" size="1024">
<constant cols="1" digits="0" name="psEnabled_2" rows="24">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="24" digits="0" name="psCondition_2" rows="2">
         62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 
         62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 62.0 
      </constant>
<constant cols="1" digits="0" name="psConnector_2" rows="24">
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
         32.0 
      </constant>
<constant cols="1" digits="0" name="psInitValue_2" rows="24">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="psPortValue_2" rows="24">
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
         1.0 
      </constant>
<constant cols="24" digits="0" name="psOutSize_2" rows="2">
         130.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 2.0 
         130.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="24" digits="0" name="psOutOffset_2" rows="2">
         6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 6.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="24" digits="0" name="psThreshold_2" rows="2">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="24" digits="0" name="psHysteresis_2" rows="2">
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
         0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 0.0 
      </constant>
<constant cols="1" digits="0" name="logFieldOffset" rows="100">
         0.0 
         2.0 
         6.0 
         8.0 
         16.0 
         18.0 
         20.0 
         22.0 
         24.0 
         26.0 
         38.0 
         40.0 
         48.0 
         50.0 
         54.0 
         58.0 
         94.0 
         252.0 
         352.0 
         364.0 
         372.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="logFieldLength" rows="100">
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         2.0 
         1.0 
         1.0 
         2.0 
         2.0 
         1.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
<constant cols="1" digits="0" name="UNALLOCATED_TOP_19" rows="244" units="RAW">
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
         0.0 
      </constant>
</page>
<settings Comment="These setting are only used if this msq is opened without a project.">
<setting name="FAHRENHEIT" value="FAHRENHEIT"/>
<setting name="PW_4X_OFF" value="PW_4X_OFF"/>
<setting name="CAN_COMMANDS" value="CAN_COMMANDS"/>
<setting name="PORT_STATUS_OFF" value="PORT_STATUS_OFF"/>
<setting name="OUTMSG_EDITING_OFF" value="OUTMSG_EDITING_OFF"/>
<setting name="INTERNAL_LOG_FIELDS_OFF" value="INTERNAL_LOG_FIELDS_OFF"/>
</settings>
<userComments Comment="These are user comments that can be related to a particular setting or dialog."/>
</msq>
