#Project Attributes.
#TunerStudio by EFI Analytics, Inc
#Last Saved on: Wed Apr 11 20:37:05 MDT 2018
#Wed Apr 11 20:37:05 MDT 2018
boostctlSettingsBoost\ Control\ Settings_width=372
egoControlEGO\ Control_width=372
Triggers.ActiveTriggers=
battcalibBattery\ Voltage\ Calibration_height=206
asePctAfterstart\ Enrichment\ Percentage_Y=143
asePctAfterstart\ Enrichment\ Percentage_X=376
idleControlIdle\ Control_Y=166
idleControlIdle\ Control_X=497
pwmidle_target_curve_Auto\ Scale\ X\ Axis\ Maximum=false
ignitionTbl1Ignition\ Table\ 1\ (Spark\ Advance)_width=538
egoControlEGO\ Control_height=540
revlimiterRev\ Limiter_width=372
veGenerator_txtPkTqMap=200
veGenerator_cBoost=Turbo w/Intercooler
dwellSettingsDwell\ Battery\ Adjustment_height=328
flexFuelSettingsFlex\ Fuel\ Settings_width=372
veTable3TblVE\ Table\ 3_height=438
crsettingsCranking\ settings_height=339
warmup_curveWarmup\ Enrichment\ Curve_Y=143
warmup_curveWarmup\ Enrichment\ Curve_X=376
outputtestOutput\ test\ mode_Y=0
outputtestOutput\ test\ mode_X=342
sensorCalSensor\ Calibration_Y=142
sensorCalSensor\ Calibration_X=629
tuneFileDir=C\:\\Users\\dfl\\Documents\\TunerStudioProjects\\MyCar
idle_voltage_comp_curveIdle\ Voltage\ Compensation_width=372
tachoTachometer\ output_height=271
RotaryTrailingSettingsRotary\ Settings_Y=249
RotaryTrailingSettingsRotary\ Settings_X=497
idleEnhanceIdle\ Enhancements_Y=121
idleEnhanceIdle\ Enhancements_X=487
seq_injectionSequential\ Injection_Y=62
seq_injectionSequential\ Injection_X=98
CommSettingDESKTOP-MDTRFETCommDriver.RS232\ Serial\ InterfaceBluetooth\ Port=false
noisefilteringNoise\ filtering_Y=101
refTable_000_chkCelsius=false
noisefilteringNoise\ filtering_X=497
NoiseFiltercurveNoise\ filter\ curve_height=277
limitsettingsLimit\ settings_height=250
N2OSystemNitrous\ System_Y=90
N2OSystemNitrous\ System_X=493
noisefilteringNoise\ filtering_height=537
pwmidle_target_curve_Set\ Y\ Axis\ Minimum=700.0
refTable_000_txtBiasResistor=50000.0
projectName=MyCar
selectedComDriver=Multi Interface MegaSquirt Driver
tableswTable\ Switching_height=469
secondaryLoadSecondary\ load\ parameters_height=450
crankingPWCranking\ Pulse\ %_Y=125
overrunOver-Run\ Fuel\ Cut_Y=181
crankingPWCranking\ Pulse\ %_X=376
veGenerator_txtDisplacementCid=110
overrunOver-Run\ Fuel\ Cut_X=497
rmt_port_editRemote\ On/Off\ Outputs_height=323
knockSettingsKnock\ Sensor\ Settings_width=372
veTable1TblVE\ Table\ 1_Y=217
ipwBinsPWM\ Idle\ Duty\ Cycle_width=613
veTable1TblVE\ Table\ 1_X=70
CommSettingMSCommDriver.RS232\ Serial\ InterfaceBluetooth\ Port=false
ignitionTbl3Spark\ Advance\ Table1_Y=129
ignitionTbl3Spark\ Advance\ Table1_X=647
refTable_000_txtResistor3=3715.0
idleAdvanceIdle\ Advance\ Settings_Y=206
refTable_000_txtResistor2=68273.0
veGenerator_txtPkTqRpm=6000
idleAdvanceIdle\ Advance\ Settings_X=497
refTable_000_txtResistor1=2022088.0
2DTable_ignitionTbl3_tableInitialDir=C\:\\Users\\dfl\\Documents\\TunerStudioProjects\\MyCar
veTable1TblFuel\ VE\ Table\ 1_Y=158
veTable1TblFuel\ VE\ Table\ 1_X=13
revlimiterRev\ Limiter_Y=193
CommSettingDESKTOP-MDTRFETCommDriver.Bluetooth\ DirectBluetooth\ Device=EFI Analytics 04 (00126FDFC9E3)
revlimiterRev\ Limiter_X=497
VeAnalyzeConsole.veTable1Tbl_verticalSplitPos=538
veTable3TblVE\ Table\ 3_width=694
veTable1Map3DVE\ Table\ 1_Y=97
NoiseFiltercurveNoise\ filter\ curve_width=372
veTable1Map3DVE\ Table\ 1_X=275
veTrim1TblFuel\ VE\ Trim\ Table\ 1_Y=150
veTrim1TblFuel\ VE\ Trim\ Table\ 1_X=336
commPort=COM5
injCharsInjector\ Characteristics_width=372
knockSettingsKnock\ Sensor\ Settings_Y=97
knockSettingsKnock\ Sensor\ Settings_X=497
veTrim1TblFuel\ VE\ Trim\ Table\ 1_height=438
veTable1TblVE\ Table\ 1_width=694
VeAnalyzePanel_veTable1Tbl_maxWeight=1.7976931348623157E308
pwmidle_PIDClosed\ Loop\ Idle\ PID\ Settings_height=574
accelsettingsAccel\ enrich\ settings_Y=254
accelsettingsAccel\ enrich\ settings_X=489
egoControlEGO\ Control_Y=91
egoControlEGO\ Control_X=698
CommSettingMSCommDriver.RS232\ Serial\ InterfaceCom\ Port=COM5
pwmidle_crank_dutyorsteps_dutycurveCoolant-based\ crank\ duty_Y=156
CommSettingDESKTOP-MDTRFETCommDriver.RS232\ Serial\ InterfaceBaud\ Rate=115200
pwmidle_crank_dutyorsteps_dutycurveCoolant-based\ crank\ duty_X=463
crankingPWCranking\ Pulsewidth%_Y=143
crankingPWCranking\ Pulsewidth%_X=376
refTable_001_txtTemp3=100.0
refTable_001_txtTemp2=30.0
WueAnalyzeConsole.wueAnalyzer_warmup_curve_horizontalSplitPos=144
refTable_001_txtTemp1=-40.0
VeAnalyzePanel_veTable1Tbl_weightThreshold=0.0
overrunOver\ Run\ Fuel\ Cut_height=363
tachoTachometer\ output_Y=235
tachoTachometer\ output_X=497
veTrim1TblVE\ Trim\ Table\ 1_Y=150
veTrim1TblVE\ Trim\ Table\ 1_X=336
outputtestOutput\ test\ mode_width=682
moreIgnitionOptionsMore\ Ignition\ Options_Y=97
moreIgnitionOptionsMore\ Ignition\ Options_X=497
baseEngine\ and\ Sequential\ Settings_width=713
baudRate=115200
veTable3Map3DVE\ Table\ 3_Y=107
veTable3Map3DVE\ Table\ 3_X=343
ipwsetPWM\ idle\ settings_width=372
overboostOverboost\ Protection_width=372
injseqInjector\ Sequence_Y=254
injseqInjector\ Sequence_X=497
VeAnalyzeConsole.veTable1Tbl_selectedDash=Histogram
pwmidle_PIDClosed\ Loop\ Idle\ PID\ Settings_width=372
ignitionTbl1Spark\ Advance\ Table1_Y=138
injCharsInjector\ Characteristics_Y=148
ignitionTbl1Spark\ Advance\ Table1_X=593
injCharsInjector\ Characteristics_X=497
revlimiterRev\ Limiter_height=351
pwmidle_crank_dutyorsteps_dutycurveCoolant-based\ crank\ duty_height=452
crsettingsCranking\ settings_Y=203
pwmidle_target_curveClosed\ loop\ idle\ target\ rpms_width=411
crsettingsCranking\ settings_X=497
ignitionMap13DSpark\ Advance\ Table1_height=543
ignitionMap33DSpark\ Advance\ Table1_Y=97
ignitionMap33DSpark\ Advance\ Table1_X=275
canparamsCAN\ Parameters_width=391
veTable1Map3DVE\ Table\ 1_height=543
crsettingsCranking\ /\ Startup\ Settings_Y=213
crsettingsCranking\ /\ Startup\ Settings_X=486
experimentalExperimental\ settings_height=187
warmup_curveWarmup\ Enrichment\ Curve_height=452
rmt_port_editRemote\ On/Off\ Outputs_width=515
aseTaperAfterstart\ Enrichment\ Taper_Y=143
aseTaperAfterstart\ Enrichment\ Taper_X=376
2DTable_veTable1Tbl_tableInitialDir=C\:\\Users\\dfl\\Documents\\TunerStudioProjects\\MyCar
overboostOverboost\ Protection_height=257
WueAnalyzeConsole.wueAnalyzer_warmup_curve_selectedDash=Standard
refTable_001_chkFahrenheit=false
veGenerator_txtIdleMap=20
ipwsetPWM\ idle\ settings_height=291
ignitionTbl1Spark\ Advance\ Table1_width=538
PersistedAccumulatedValue_(\ (\ tsFuelFlowGph\ *\ deltatime\ /\ 3600.0\ )\ )=-0.0
pwmidle_target_curve_Set\ X\ Axis\ Minimum=0.0
std_port_editOutput\ port\ Settings_height=345
limitsettingsLimit\ settings_width=372
veTable1TblFuel\ VE\ Table\ 1_height=438
VeAnalyzePanel_veTable1Tbl_targetLambdaChannelName=
projectDescription=
aseTaperAfterstart\ Enrichment\ Taper_height=452
limitsettingsLimit\ settings_Y=244
CommSettingCom\ Port=COM4
baseEngine\ and\ Sequential\ Settings_height=566
limitsettingsLimit\ settings_X=497
pwmidle_target_curveClosed\ loop\ idle\ target\ rpms_height=365
setbaudMegasquirt\ baud\ rate_Y=277
pwmidle_closedloopClosed\ Loop\ Idle\ Valve\ Settings_Y=141
setbaudMegasquirt\ baud\ rate_X=497
pwmidle_closedloopClosed\ Loop\ Idle\ Valve\ Settings_X=494
pwmidle_crank_dutyorsteps_dutycurveCoolant-based\ crank\ duty_width=622
refTable_000_chkFahrenheit=true
overrunOver\ Run\ Fuel\ Cut_width=372
CommSettingBaud\ Rate=115200
pwmidle_closedloopClosed\ Loop\ Idle\ Valve\ Settings_width=378
flexFuelSettingsFlex\ Fuel\ Settings_Y=191
flexFuelSettingsFlex\ Fuel\ Settings_X=497
veGenerator_txtPkHp=250
idleEnhanceIdle\ Enhancements_height=503
pwmidle_target_curveClosed\ loop\ idle\ target\ rpms_Y=159
pwmidle_target_curveClosed\ loop\ idle\ target\ rpms_X=552
injseqInjector\ Sequence_width=372
dwellSettingsDwell\ Battery\ Adjustment_width=372
idleControlIdle\ Control_height=407
flexFuelSettingsFlex\ Fuel\ Settings_height=355
logFileDir=C\:\\Users\\dfl\\Documents\\TunerStudioProjects\\MyCar\\DataLogs
veGenerator_txtDisplacementCc=1803
overrunOver-Run\ Fuel\ Cut_width=372
MATCorrvalMAT\ correction\ value_width=372
setbaudMegasquirt\ baud\ rate_width=372
crsettingsCranking\ /\ Startup\ Settings_height=311
RotaryTrailingSettingsRotary\ Settings_height=240
CommSettingDESKTOP-MDTRFETCommDriver.controllerInterfaceId=RS232 Serial Interface
manifoldTempCorrNon-Linear\ MAT\ Correction_Y=156
manifoldTempCorrNon-Linear\ MAT\ Correction_X=425
logTuningPanel_selectionTable2=RotarySplitTbl
logTuningPanel_selectionTable1=veTable1Tbl
overrunOver-Run\ Fuel\ Cut_height=375
refTable_001_chkCelsius=true
accelsettingsAccel\ enrich\ settings_width=387
N2OSystemNitrous\ System_width=379
WueAnalyzeConsole.wueAnalyzer_warmup_curve_verticalSplitPos=545
ignitionMap13DSpark\ Advance\ Table1_width=816
Accel\ Enrichment\ Wizard_width=630
crankingPWCranking\ Pulse\ %_width=613
veGenerator_txtIdleRpm=850
asePctAfterstart\ Enrichment\ Percentage_width=613
iactestIdle\ valve\ test_height=273
idleAdvanceIdle\ Advance\ Settings_height=327
Accel\ Enrichment\ Wizard_height=553
ipwsetPWM\ idle\ settings_Y=225
ipwsetPWM\ idle\ settings_X=497
launchLaunch\ Control_height=437
recordsPerSec=5
canparamsCAN\ Parameters_height=649
knockSettingsKnock\ Sensor\ Settings_height=545
crankingPWCranking\ Pulsewidth%_width=613
crankingPWCranking\ Pulsewidth%_height=452
primingPWPriming\ Pulsewidth_width=613
dwellSettingsDwell\ Battery\ Adjustment_Y=205
dwellSettingsDwell\ Battery\ Adjustment_X=497
ignitionTbl1Spark\ Advance\ Table1_height=374
launchLaunch\ Control_Y=150
pwmidle_target_curve_Set\ Y\ Axis\ Maximum=1800.0
launchLaunch\ Control_X=497
refTable_002_txtY2=19.5
refTable_002_txtY1=9.5
CommSettingMSCommDriver.controllerInterfaceId=RS232 Serial Interface
ipwBinsPWM\ Idle\ Duty\ Cycle_Y=143
ipwBinsPWM\ Idle\ Duty\ Cycle_X=376
battcalibBattery\ Voltage\ Calibration_Y=261
battcalibBattery\ Voltage\ Calibration_X=497
ignitionTbl3Spark\ Advance\ Table1_width=538
veTrim1TblFuel\ VE\ Trim\ Table\ 1_width=694
veTable3Map3DVE\ Table\ 3_width=816
std_port_editOutput\ port\ Settings_width=495
refTable_002_txtX2=4
refTable_002_txtX1=1
tsSupplementalFieldsVehicle\ Specifications_Y=162
tsSupplementalFieldsVehicle\ Specifications_X=358
secondaryLoadSecondary\ load\ parameters_Y=139
RotaryTrailingSettingsRotary\ Settings_width=372
secondaryLoadSecondary\ load\ parameters_X=497
boostctlSettingsBoost\ Control\ Settings_height=463
manifoldTempCorrNon-Linear\ MAT\ Correction_height=425
moreIgnitionOptionsMore\ Ignition\ Options_width=372
seq_injectionSequential\ Injection_width=389
PersistedAccumulatedValue_(\ (\ tsInputSpeedMPH\ *\ 1.60934\ )\ /\ 3600.0\ *\ deltatime\ )=97.37469984983937
VeAnalyzePanel_veTable1Tbl_targetLambdaTableName=afrTable1Tbl
matBasedRetardMAT-Based\ Timing\ Retard_Y=156
matBasedRetardMAT-Based\ Timing\ Retard_X=425
veTrim1TblVE\ Trim\ Table\ 1_width=694
injCharsInjector\ Characteristics_height=441
Accel\ Enrichment\ Wizard_Y=92
Accel\ Enrichment\ Wizard_X=368
canId=0
baseEngine\ and\ Sequential\ Settings_Y=86
baseEngine\ and\ Sequential\ Settings_X=326
tsSupplementalFieldsVehicle\ Specifications_width=650
secondaryLoadSecondary\ load\ parameters_width=372
refTable_000_txtTemp3=210.200
refTable_000_txtTemp2=69.800
experimentalExperimental\ settings_width=377
refTable_000_txtTemp1=-40.000
refTable_001_txtBiasResistor=2490.0
veTable1TblFuel\ VE\ Table\ 1_width=694
veGenerator_txtPkHpMap=200
ipwBinsPWM\ Idle\ Duty\ Cycle_height=452
setbaudMegasquirt\ baud\ rate_height=183
ecuSettings=CAN_COMMANDS_OFF|EGTFULL_OFF|EXPANDED_CLT_TEMP_OFF|FAHRENHEIT|USE_CRC_DATA_CHECK_OFF|
experimentalExperimental\ settings_Y=276
iactestIdle\ valve\ test_width=372
experimentalExperimental\ settings_X=494
veTable1Map3DVE\ Table\ 1_width=816
limitsettingsGauge\ and\ Settings\ Limits_height=343
pwmidle_target_curve_Auto\ Scale\ Y\ Axis\ Maximum=false
launchLaunch\ Control_width=372
VeAnalyzePanel_veTable1Tbl_baseWeight=0.5
veGenerator_txtMaxRpm=8000
WueAnalyzePanel_wueAnalyzer_warmup_curve_applyPeriod=Manually
primingPWPriming\ Pulsewidth_height=488
stagingStaged\ Injection_width=398
MyCar.veTable1Tbl_std_xAxisMax=8000.0
boostctlSettingsBoost\ Control\ Settings_Y=138
boostctlSettingsBoost\ Control\ Settings_X=497
barometerCorrNon-Linear\ Barometric\ Correction_height=425
pwmidle_closedloopClosed\ Loop\ Idle\ Valve\ Settings_height=457
injseqInjector\ Sequence_height=229
tachoTachometer\ output_width=372
idleEnhanceIdle\ Enhancements_width=392
afrTable1TblAFR\ Table\ 1_Y=96
tableswTable\ Switching_Y=135
afrTable1TblAFR\ Table\ 1_X=744
tableswTable\ Switching_X=497
accelsettingsAccel\ enrich\ settings_height=231
VeAnalyzeConsole.veTable3Tbl_selectedDash=Standard
idle_voltage_comp_curveIdle\ Voltage\ Compensation_Y=205
idle_voltage_comp_curveIdle\ Voltage\ Compensation_X=497
sensorCalSensor\ Calibration_height=332
afrTable1TblAFR\ Table\ 1_height=374
aseTaperAfterstart\ Enrichment\ Taper_width=613
ignitionTbl1Ignition\ Table\ 1\ (Spark\ Advance)_height=374
MyCar.veTable1Tbl_minRPMFilter=1500.0
iactestIdle\ valve\ test_Y=234
iactestIdle\ valve\ test_X=497
veTable3TblVE\ Table\ 3_Y=301
tableswTable\ Switching_width=372
veTable3TblVE\ Table\ 3_X=439
moreIgnitionOptionsMore\ Ignition\ Options_height=547
afrTable1TblAFR\ Table\ 1_width=538
CommSettingDESKTOP-MDTRFETCommDriver.RS232\ Serial\ InterfaceCom\ Port=COM5
canparamsCAN\ Parameters_Y=44
canparamsCAN\ Parameters_X=487
generalSettingsGeneral\ Settings_Y=76
generalSettingsGeneral\ Settings_X=497
veGenerator_txtPkHpRpm=7000
ignitionOptionsIgnition\ Options_width=392
overboostOverboost\ Protection_Y=240
stagingStaged\ Injection_Y=131
stagingStaged\ Injection_X=484
overboostOverboost\ Protection_X=497
ignitionMap33DSpark\ Advance\ Table1_height=543
limitsettingsGauge\ and\ Settings\ Limits_Y=197
limitsettingsGauge\ and\ Settings\ Limits_X=490
noisefilteringNoise\ filtering_width=372
pwmidle_target_curve_Set\ X\ Axis\ Maximum=255.0
ignitionOptionsIgnition\ Options_height=485
crsettingsCranking\ settings_width=372
crankingPWCranking\ Pulse\ %_height=488
2DTable_veTable3Tbl_tableInitialDir=C\:\\Users\\dfl\\Documents\\TunerStudioProjects\\MyCar
protocolEnvelope=
NoiseFiltercurveNoise\ filter\ curve_Y=230
matBasedRetardMAT-Based\ Timing\ Retard_height=425
NoiseFiltercurveNoise\ filter\ curve_X=497
CommSettingMSCommDriver.Bluetooth\ DirectBluetooth\ Device=EFI Analytics 04 (00126FDFC9E3)
barometerCorrNon-Linear\ Barometric\ Correction_Y=151
barometerCorrNon-Linear\ Barometric\ Correction_X=425
idle_voltage_comp_curveIdle\ Voltage\ Compensation_height=328
ignitionTbl3Spark\ Advance\ Table1_height=374
refTable_001_txtResistor3=186.6
refTable_001_txtResistor2=1707
outputtestOutput\ test\ mode_height=738
refTable_001_txtResistor1=45313
seq_injectionSequential\ Injection_height=664
idleAdvanceIdle\ Advance\ Settings_width=372
primingPWPriming\ Pulsewidth_Y=125
primingPWPriming\ Pulsewidth_X=376
CommSettingMSCommDriver.RS232\ Serial\ InterfaceBaud\ Rate=115200
crsettingsCranking\ /\ Startup\ Settings_width=393
std_port_editOutput\ port\ Settings_Y=196
warmup_curveWarmup\ Enrichment\ Curve_width=613
std_port_editOutput\ port\ Settings_X=435
limitsettingsGauge\ and\ Settings\ Limits_width=385
MATCorrvalMAT\ correction\ value_Y=235
N2OSystemNitrous\ System_height=558
MATCorrvalMAT\ correction\ value_X=497
battcalibBattery\ Voltage\ Calibration_width=372
asePctAfterstart\ Enrichment\ Percentage_height=452
matBasedRetardMAT-Based\ Timing\ Retard_width=516
veTable3Map3DVE\ Table\ 3_height=543
veTable1TblVE\ Table\ 1_height=438
PersistedAccumulatedValue_(\ tsInputSpeedMPH\ /\ 3600.0\ *\ deltatime\ )=61.00734258388392
ignitionMap33DSpark\ Advance\ Table1_width=816
sensorCalSensor\ Calibration_width=372
MATCorrvalMAT\ correction\ value_height=275
idleControlIdle\ Control_width=372
manifoldTempCorrNon-Linear\ MAT\ Correction_width=516
stagingStaged\ Injection_height=475
veTrim1TblVE\ Trim\ Table\ 1_height=438
barometerCorrNon-Linear\ Barometric\ Correction_width=516
ignitionMap13DSpark\ Advance\ Table1_Y=97
ignitionMap13DSpark\ Advance\ Table1_X=275
pwmidle_PIDClosed\ Loop\ Idle\ PID\ Settings_Y=99
pwmidle_PIDClosed\ Loop\ Idle\ PID\ Settings_X=160
veGenerator_txtPkTq=220
VeAnalyzePanel_veTable1Tbl_minChangeThreshold=0.0
ignitionOptionsIgnition\ Options_Y=127
dashBoardFile=\\dashboard\\\\dashboard.dash
ignitionOptionsIgnition\ Options_X=487
ecuConfigFile=mainController.ini
tsSupplementalFieldsVehicle\ Specifications_height=413
rmt_port_editRemote\ On/Off\ Outputs_Y=207
generalSettingsGeneral\ Settings_width=372
ignitionTbl1Ignition\ Table\ 1\ (Spark\ Advance)_Y=273
rmt_port_editRemote\ On/Off\ Outputs_X=425
ignitionTbl1Ignition\ Table\ 1\ (Spark\ Advance)_X=272
generalSettingsGeneral\ Settings_height=587
overrunOver\ Run\ Fuel\ Cut_Y=147
overrunOver\ Run\ Fuel\ Cut_X=651
